World GT-R Rules - Updated 08/01/2019
- Chassis – 200mm pan car chassis (WGT car)
-Minimum Ride Height – 5mm
-Minimum Weight – 1025 grams
-Maximum Track Width - 200mm
- Tire and Wheel Rules – Starting with the 2015-2016 season, Team CRC GTR rims will be the only rims allowed (Part #2310). The only front tires that will be allowed are Team CRC RT-1 (Part#2311), Team CRC Mounted RT-1 (Part#2314), and TCS fronts (Part#1031). The only rear tires that will be allowed are Team CRC RT-1 (Part#2312), Team CRC Mounted RT-1 (Part#2316), and TCS (Part#1032). Tires can be mounted “F1/Nascar” or “GT” style. If mounted “GT” style, the inner lip can be trimmed for clearance, however the molded letters (either CRC or TCS) must not be removed. The is no performance advantage to either mounting style, it is just for scale appearance. Stock inserts only. No Modifying inserts or “double stuffing” of inserts will be allowed.
-Battery – ROAR approved 1 cell (3.7v) hard case lipo. Voltage limit to be set by track (4.20-4.22)
-Motor – Any ROAR approved 17.5 turn brushless motor (Smaller tracks are encouraged to use 21.5)
-Rotor – ROAR approved tuning rotors are allowed
-Speed Control – Any ROAR approved spec class (blinky) speed control in “blinky” mode. NO RECEIVER PACKS. You may use a specific 1 cell speed control, or a two cell speed control with an external booster. Stock 2 or 4 cap banks that come with the ESC's only. There will be a limit of 10,000 micro farad on cap banks.
-Bodies – Bodies must be cut on the mold lines. No excessive cutting or lowering of the body is permitted. No lightening of the body is permitted. Wings and spoilers that are included with the body kits are ok if cut on one of the mold lines (if multiple mold lines are present). Wings are not mandatory. No additional aerodynamic aids are allowed. Backs of the bodies (including rear bumpers) are to be left in. No bodies that were designed for pan cars, no GTP, Daytona Prototype, IMSA, or bodies that look like 1/12th or 1/8th on road bodies with an integrated rear wing. Tires cannot stick outside the body. If the body has bolt on pieces (for example the Ford GT B pillar side wings, or some of the HPI bodies have a bolt on rear bumper area), these must be used. This does not apply to the side dams that can be added to the rear wing. Bodies must weigh a minimum of 95 grams. Any weight added to the body to assist in the making of the 95 gram minimum weight must be added to what would be considered the roof of the vehicle in a non easily removed form (if you need to add weight, put some shoe goo in the roof). Any foam needed to take up space in between the body and front bumper must be added to the chassis, not the body. These rules are to encourage racers to actually put a paint job on the body and not just a spray bomb, as well as to keep some of the older heavier bodies competitive.
-Race Length- Have fun with this. If 5 minute qualifiers and 5 minute mains fit in your race program, do that. If you want to do 8 minute races, do that. If you want to do shorter qualifiers and longer mains, do that. We have run 15 minutes with ease. Work with your race director to fit into the program. Run time and traction are not an issue for longer races.
-Fun- 100% Mandatory!
Approved Body list:
- Any body currently on the USVTA approved body list 
- Protoform 1543-00 Cadillac ATS-V.R
- Protoform 1544-30 Chevy Camaro Z28
- Protoform 1548-30 Cadillac ATS-V.R (200mm version)
- Protoform 1532-30 Chevy Camaro ZL1
- Protoform 1542-30 PFM-10
- Protoform 1549-30 Ford GT
- Protoform 1557-30 Chevrolet Corvette C7R
- Protoform 1563-25 Chevrolet Corvette ZR1
- McAllister 307 MX Stang GT
- McAllister 233 Lexus IS
- McAllister 211 Jaguar XKR
- McAllister 282 Mercedes DTM
- McAllister 311 WGT-R LeMans C6
- McAllister 191 2004 Chevrolet Corvette
- McAllister 192 Mustang Cobra
- KYOFAB451 Kyosho Dodge Challenger SRT
- KYOFAB158 Toyota Supra
- HPI Racing 103886 Nissan 350z Hankook 
- HPI Racing 106108 2011 Ford Mustang
- HPI Racing 108064 Scion FR-S
- HPI Racing 108370 2012 Porsche 911 GT3
- HPI Racing 109930 1969 Ford Mustang
- HPI Racing 17502 De Tomaso Pantera
- HPI Racing 17503 Chevrolet Corvette C6
- HPI Racing 17504 Ford Mustang GT-R
- HPI Racing 17518 Nissan 350z Greddy
- HPI Racing 17526 1967 Chevrolet Corvette
- HPI Racing 17527 Porsche 911 Turbo
- HPI Racing 17530 Nissan Silvia
- HPI Racing 17538 Nissan GT-R (R35)
- HPI Racing 17539 Toyota Supra Aero
- HPI Racing 17541 Porsche 911 GT3 RS
- HPI Racing 17542 Lexus IS F
- HPI Racing 17543 2010 Chevy Camaro
- HPI Racing 17544 Alfa Romeo 8C
- HPI Racing 17548 BMW M3 GT2
- HPI Racing 30730 Lexus LS430
- HPI Racing 7038 Porsche 911 GT1
- HPI Racing 7418 Porsche 911 GT3
- HPI Racing 7424 Toyota Supra
- HPI Racing 7427 Nissan Skyline R34 GT-R
- HPI Racing 7435 Porsche 911 Turbo
- HPI Racing 7440 Toyota Celica
- HPI Racing 7452 BMW M3 GT
- HPI Racing 7485 Nissan 350z Nismo GT
- HPI Racing 7486 Toyota Supra GT
- HPI Racing 7495 Ford GT
- HPI Racing 7499 HPI Racing Impreza
- Tamiya 51450 Raybrig Honda HSV-010
- Tamiya 51200 Xanavi NISMO GT-R
- Tamiya 51195 Raybrig NSX 2004
- Tamiya 51544 LaFerrari
- Tamiya 51526 Ferrari 458
- Tamiya 51590 Mercedes AMG GT3
- Tamiya 51592 Ferrari F12 TDF
- Delta Plastik 0034 Subaru
- Delta Plastik 0037 Porsche 911
- Delta Plastik 0040 F50
- Delta Plastik 0049 Viper
- Delta Plastik 0050 Lotus Elise
- Delta Plastik 0052 CLK
- Delta Plastik 0055 Ferrari Enzo
- Delta Plastik 0056 Diablo
- Delta Plastik 0058 BMW M Coupe
- Delta Plastik 0402 Panoz Esp. GTR-1
- Delta Plastik 0405 Mustang
- Delta Plastik 0417 Ferrari F355 Challenge
- Pitlane Hobbies PLAMGT AM-GT
-Bitty Designs BDGT-190AGT Agata
-Zoo Racing ZR-0007-07 Zoodiac
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