Arduino

Reference Language | Libraries | Comparison | Changes

## goto

Transfers program flow to a labeled point in the program

#### Syntax

label:

goto label; // sends program flow to the label

#### Tip

The use of goto is discouraged in C programming, and some authors of C programming books claim that the goto statement is never necessary, but used judiciously, it can simplify certain programs. The reason that many programmers frown upon the use of goto is that with the unrestrained use of goto statements, it is easy to create a program with undefined program flow, which can never be debugged.

With that said, there are instances where a goto statement can come in handy, and simplify coding. One of these situations is to break out of deeply nested for loops, or if logic blocks, on a certain condition.

#### Example

    for(byte r = 0; r < 255; r++){
        for(byte g = 255; g > -1; g--){
            for(byte b = 0; b < 255; b++){
                if (analogRead(0) > 250){ goto bailout;}
                // more statements ...
            }
        }
    }
    bailout:

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes