Arduino

Reference Language | Libraries | Comparison | Changes

## setup()

The setup() function is called when a sketch starts. Use it to initialize variables, pin modes, start using libraries, etc. The setup function will only run once, after each powerup or reset of the Arduino board.

### Example

    int buttonPin = 3;

    void setup()
    {
      Serial.begin(9600);
      pinMode(buttonPin, INPUT);
    }

    void loop()
    {
      // ...
    }

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes