Next: Alignment Output, Previous: Dispatch Tables, Up: Assembler Format

#### 15.21.9 Assembler Commands for Exception Regions

This describes commands marking the start and the end of an exception region.

— Macro: EH_FRAME_SECTION_NAME

> If defined, a C string constant for the name of the section containing exception handling frame unwind information. If not defined, GCC will provide a default definition if the target supports named sections. crtstuff.c uses this macro to switch to the appropriate section.

> You should define this symbol if your target supports DWARF 2 frame unwind information and the default definition does not work.

— Macro: EH_FRAME_IN_DATA_SECTION

> If defined, DWARF 2 frame unwind information will be placed in the data section even though the target supports named sections. This might be necessary, for instance, if the system linker does garbage collection and sections cannot be marked as not to be collected.

> Do not define this macro unless `TARGET_ASM_NAMED_SECTION` is also defined.

— Macro: EH_TABLES_CAN_BE_READ_ONLY

> Define this macro to 1 if your target is such that no frame unwind information encoding used with non-PIC code will ever require a runtime relocation, but the linker may not support merging read-only and read-write sections into a single read-write section.

— Macro: MASK_RETURN_ADDR

> An rtx used to mask the return address found via `RETURN_ADDR_RTX`, so that it does not contain any extraneous set bits in it.

— Macro: DWARF2_UNWIND_INFO

> Define this macro to 0 if your target supports DWARF 2 frame unwind information, but it does not yet work with exception handling. Otherwise, if your target supports this information (if it defines INCOMING_RETURN_ADDR_RTX and either UNALIGNED_INT_ASM_OP or OBJECT_FORMAT_ELF), GCC will provide a default definition of 1.

> If `TARGET_UNWIND_INFO` is defined, the target specific unwinder will be used in all cases. Defining this macro will enable the generation of DWARF 2 frame debugging information.

> If `TARGET_UNWIND_INFO` is not defined, and this macro is defined to 1, the DWARF 2 unwinder will be the default exception handling mechanism; otherwise, the `setjmp`/`longjmp`-based scheme will be used by default.

— Macro: TARGET_UNWIND_INFO

> Define this macro if your target has ABI specified unwind tables. Usually these will be output by `TARGET_UNWIND_EMIT`.

— Variable: Target Hook bool TARGET_UNWIND_TABLES_DEFAULT

> This variable should be set to `true` if the target ABI requires unwinding tables even when exceptions are not used.

— Macro: MUST_USE_SJLJ_EXCEPTIONS

> This macro need only be defined if `DWARF2_UNWIND_INFO` is runtime-variable. In that case, except.h cannot correctly determine the corresponding definition of `MUST_USE_SJLJ_EXCEPTIONS`, so the target must provide it directly.

— Macro: DONT_USE_BUILTIN_SETJMP

> Define this macro to 1 if the `setjmp`/`longjmp`-based scheme should use the `setjmp`/`longjmp` functions from the C library instead of the `__builtin_setjmp`/`__builtin_longjmp` machinery.

— Macro: DWARF_CIE_DATA_ALIGNMENT

> This macro need only be defined if the target might save registers in the function prologue at an offset to the stack pointer that is not aligned to `UNITS_PER_WORD`. The definition should be the negative minimum alignment if `STACK_GROWS_DOWNWARD` is defined, and the positive minimum alignment otherwise. See SDB and DWARF. Only applicable if the target supports DWARF 2 frame unwind information.

— Variable: Target Hook bool TARGET_TERMINATE_DW2_EH_FRAME_INFO

> Contains the value true if the target should add a zero word onto the end of a Dwarf-2 frame info section when used for exception handling. Default value is false if `EH_FRAME_SECTION_NAME` is defined, and true otherwise.

— Target Hook: rtx TARGET_DWARF_REGISTER_SPAN (rtx reg)

> Given a register, this hook should return a parallel of registers to represent where to find the register pieces. Define this hook if the register and its mode are represented in Dwarf in non-contiguous locations, or if the register should be represented in more than one register in Dwarf. Otherwise, this hook should return `NULL_RTX`. If not defined, the default is to return `NULL_RTX`.

— Target Hook: void TARGET_INIT_DWARF_REG_SIZES_EXTRA (tree address)

> If some registers are represented in Dwarf-2 unwind information in multiple pieces, define this hook to fill in information about the sizes of those pieces in the table used by the unwinder at runtime. It will be called by `expand_builtin_init_dwarf_reg_sizes` after filling in a single size corresponding to each hard register; address is the address of the table.

— Target Hook: bool TARGET_ASM_TTYPE (rtx sym)

> This hook is used to output a reference from a frame unwinding table to the type_info object identified by sym. It should return `true` if the reference was output. Returning `false` will cause the reference to be output using the normal Dwarf2 routines.

— Target Hook: bool TARGET_ARM_EABI_UNWINDER

> This hook should be set to `true` on targets that use an ARM EABI based unwinding library, and `false` on other targets. This effects the format of unwinding tables, and how the unwinder in entered after running a cleanup. The default is `false`.