Arduino

Reference Language | Libraries | Comparison | Changes

## do - while

The do loop works in the same manner as the while loop, with the exception that the condition is tested at the end of the loop, so the do loop will always run at least once.

    do
    {
        // statement block
    } while (test condition);

#### Example

    do
    {
      delay(50);          // wait for sensors to stabilize
      x = readSensors();  // check the sensors

    } while (x < 100);

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes