Next: Aggregate Return, Previous: Register Arguments, Up: Stack and Calling

#### 15.10.8 How Scalar Function Values Are Returned

This section discusses the macros that control returning scalars as values—values that can fit in registers.

— Target Hook: rtx TARGET_FUNCTION_VALUE (tree ret_type, tree fn_decl_or_type, bool outgoing)

> Define this to return an RTX representing the place where a function returns or receives a value of data type ret_type, a tree node node representing a data type. fn_decl_or_type is a tree node representing `FUNCTION_DECL` or `FUNCTION_TYPE` of a function being called. If outgoing is false, the hook should compute the register in which the caller will see the return value. Otherwise, the hook should return an RTX representing the place where a function returns a value.

> On many machines, only `TYPE_MODE (`ret_type`)` is relevant. (Actually, on most machines, scalar values are returned in the same place regardless of mode.) The value of the expression is usually a `reg` RTX for the hard register where the return value is stored. The value can also be a `parallel` RTX, if the return value is in multiple places. See `FUNCTION_ARG` for an explanation of the `parallel` form. Note that the callee will populate every location specified in the `parallel`, but if the first element of the `parallel` contains the whole return value, callers will use that element as the canonical location and ignore the others. The m68k port uses this type of `parallel` to return pointers in both %a0 (the canonical location) and %d0.

> If `TARGET_PROMOTE_FUNCTION_RETURN` returns true, you must apply the same promotion rules specified in `PROMOTE_MODE` if valtype is a scalar type.

> If the precise function being called is known, func is a tree node (`FUNCTION_DECL`) for it; otherwise, func is a null pointer. This makes it possible to use a different value-returning convention for specific functions when all their calls are known.

> Some target machines have “register windows” so that the register in which a function returns its value is not the same as the one in which the caller sees the value. For such machines, you should return different RTX depending on outgoing.

> `TARGET_FUNCTION_VALUE` is not used for return values with aggregate data types, because these are returned in another way. See `TARGET_STRUCT_VALUE_RTX` and related macros, below.

— Macro: FUNCTION_VALUE (valtype, func)

> This macro has been deprecated. Use `TARGET_FUNCTION_VALUE` for a new target instead.

— Macro: FUNCTION_OUTGOING_VALUE (valtype, func)

> This macro has been deprecated. Use `TARGET_FUNCTION_VALUE` for a new target instead.

— Macro: LIBCALL_VALUE (mode)

> A C expression to create an RTX representing the place where a library function returns a value of mode mode. If the precise function being called is known, func is a tree node (`FUNCTION_DECL`) for it; otherwise, func is a null pointer. This makes it possible to use a different value-returning convention for specific functions when all their calls are known.

> Note that “library function” in this context means a compiler support routine, used to perform arithmetic, whose name is known specially by the compiler and was not mentioned in the C code being compiled.

> The definition of `LIBRARY_VALUE` need not be concerned aggregate data types, because none of the library functions returns such types.

— Macro: FUNCTION_VALUE_REGNO_P (regno)

> A C expression that is nonzero if regno is the number of a hard register in which the values of called function may come back.

> A register whose use for returning values is limited to serving as the second of a pair (for a value of type `double`, say) need not be recognized by this macro. So for most machines, this definition suffices:

>               #define FUNCTION_VALUE_REGNO_P(N) ((N) == 0)

> If the machine has register windows, so that the caller and the called function use different registers for the return value, this macro should recognize only the caller's register numbers.

— Macro: APPLY_RESULT_SIZE

> Define this macro if untyped_call and untyped_return need more space than is implied by `FUNCTION_VALUE_REGNO_P` for saving and restoring an arbitrary return value.

— Target Hook: bool TARGET_RETURN_IN_MSB (tree type)

> This hook should return true if values of type type are returned at the most significant end of a register (in other words, if they are padded at the least significant end). You can assume that type is returned in a register; the caller is required to check this.

> Note that the register provided by `TARGET_FUNCTION_VALUE` must be able to hold the complete return value. For example, if a 1-, 2- or 3-byte structure is returned at the most significant end of a 4-byte register, `TARGET_FUNCTION_VALUE` should provide an `SImode` rtx.