Next: PCH Target, Previous: Target Attributes, Up: Target Macros

### 15.26 Defining coprocessor specifics for MIPS targets.

The MIPS specification allows MIPS implementations to have as many as 4 coprocessors, each with as many as 32 private registers. GCC supports accessing these registers and transferring values between the registers and memory using asm-ized variables. For example:

           register unsigned int cp0count asm ("c0r1");
           unsigned int d;

           d = cp0count + 3;

(“c0r1” is the default name of register 1 in coprocessor 0; alternate names may be added as described below, or the default names may be overridden entirely in `SUBTARGET_CONDITIONAL_REGISTER_USAGE`.)

Coprocessor registers are assumed to be epilogue-used; sets to them will be preserved even if it does not appear that the register is used again later in the function.

Another note: according to the MIPS spec, coprocessor 1 (if present) is the FPU. One accesses COP1 registers through standard mips floating-point support; they are not included in this mechanism.

There is one macro used in defining the MIPS coprocessor interface which you may want to override in subtargets; it is described below.

— Macro: ALL_COP_ADDITIONAL_REGISTER_NAMES

> A comma-separated list (with leading comma) of pairs describing the alternate names of coprocessor registers. The format of each entry should be

>               { alternatename, register_number}

> Default: empty.