Scarlet Build 3 v3.2.16 Firmware        June 14, 2012

Note: Download the latest versions of REDCINE-X and RED Rocket installer/drivers from www.red.com/support. 

IMPORTANT: 
* You will not be able to roll back to earlier firmware revisions than v2.0.2 after installing v3.2.16
* REDMote firmware v3.1.x is required to be functional and can be downloaded from www.red.com/support.
* Refer to the Ops Guide for REDmote upgrade instructions.
* Preset files are not compatible with previous versions

Installation Instructions for Build 3 v3.2.16 camera firmware: 
1. Uncompress the v3.2.16 firmware zip file. 

NOTE: RED Watchdog (MAC Only) mounts the MAG read-only by default. Change preference to mount Read-Write before attempting to copy firmware to the MAG.

2. Using RED STATION REDMAG 1.8", copy the "force_upgrade" folder and its contents to the top level of the REDMAGĻ 1.8" SSD directory. 3. Eject or unmount the SSD, then remove the SSD from RED STATION.  
4. Ensure camera is powered down and REDmote undocked.  
5. Insert the SSD into your Epic-X and power up. Force upgrade will automatically run only at power up and will not display anything on the external monitors.

NOTE: During upgrade, fans will run at high speed and the PWR and REC LEDs will blink Green. After approximately 45 seconds, the LEDs will stop blinking and the camera will power down. 

6. After camera power down, remove the SSD and wait 10 seconds.
7. Power up the camera.
8. Go to the SETTINGS/MAINTENANCE/SYSTEM INFO menu and verify that the camera monitor output(s) report back - Version 3.2.16 and PIN (value specific to camera)
9. Installation is now complete. 

NOTE: After the firmware upgrade, it is mandatory that you re-format the REDMAG SSDs before use.

Significant changes since previous build v3.0.7:
* Added 5K HD, 3K HD, 2K HD, 1K HD formats
* Added 1K WS format (Epic 400fps, Scarlet 120fps)
* Added Target REDCode feature
* Added Post Record Fan Delay (max 1 minute)
* Added 1-camera to multiple REDMote support
* Added Slate Information Dialog
* Added User RGB curves capability
* Added RMD file import/save/apply
* Added Gyro support
* Added Side Handle Key Lock Feature
* Added Audio Gain/Limiter Controls
* Added Phantom Power Support(Hardware Rev Dependent)
* Added External record mode
* Added Force Restore Feature using Power Button
* Added HD-SDI Format controls
* Added 9" LCD Touchscreen support
* Added Dual Battery Module support
* Added Rear SSD Module support
* Added OLED EVF Brightness support
* Added Playback Frame, Title and Action Guide status
* Added PL Lens short circuit detection
* Added HDMI 1080p/720p refresh rates of 24,25,30,50,60
* Enhanced Keys assignment dialog
* Enhanced Preset dialog
* Enhanced Playback load notifications and error handling
* Enhanced UI usability
* Enhanced AF capability
* Camera Name defaults to camera type (i.e., SCARLET/EPIC)
* Fix for Playback using EVF
* Fix for Playback support of 5K and 5K ANA
* Fix for Zoom Rocker +/- Mapping
* Fix for HD-SDI output scaling
* Fix for LCD image 'stutter' when panning
* Fix for camera freeze when changing AF/MF with Focus dialog open
* Fix for Zebras disappearing after disconnect/reconnect of RED monitor
* Fix for scaling of 5K clips during Playback
* Fix for HD-SDI test pattern output levels
* Fix for record error 0x00001E seen on some cameras 
* Fix for multi-clip load issue in Playback
* Fix for audio in HDRx mode
* Fix for frame drift with Sensor Sync = Genlock on some cameras
* Fix for camera not completing clip recording to end of media
* Fix for camera hang mapping actions to rocker switch
* Fix for LCD w/half white screen on start-up
* Fix for RED EVF connection problems 

Operational notes specific to Build v3.2.16:
* Sensor Flip disabled
* Detaching monitor during playback will require reboot on monitor re-attach
* Camera powered by RED BRICK may display voltage instead of battery capacity on some cameras.
* EVF black level raised in some cases
* ISO setting limited to min of 250 
* Image Magnify is available during preview, but not during recording.
* HD-SDI is True Progressive and does not support 1080i or 1080 PsF signal formats. 
Copyright (c) 2012 RED Digital Cinema, All Rights Reserved.