****************************************************************************
 HDVR integration Interface for C•CURE 9000 Version 1.93 November 2010
 Copyright © 2010 Tyco International Ltd. and its Respective Companies.
****************************************************************************

This readme file provides important information about the HDVR Integration Interface for C•CURE 9000 Version 1.93. Please read this file before installing the product.

Contents
-----------------------------
1. Feature
2. Requirements
3. Contents of the DVD
4. Installation
5. Problems Fixed in this Release
6. Limitations
-----------------------------

1. Feature
-----------------------------
The HDVR integration is a C•CURE 9000 application that can be used to
configure HDVR video servers and video cameras. Users can show video views,
video tours, do PTZ controls and trigger alarm events or camera actions when
a camera is in an alarm state.


----------------------------

2. Requirements
----------------------------
The C•CURE 9000 HDVR integration for version 1.93 requires the following software versions.

 •  Exacq API version 1.9.0.22273
 •  HDVR Software version 1.2.4.22317
 •  Exacq Software version  4.1.5.21712
 •  C•CURE 9000 Security and Event Management System version 1.93.

The integration supports deployment on the following 32-bit operating systems.
An additional requirement for the final three is noted in the Limitations section.

 •  Windows XP Professional
 •  Windows 2003
 •  Windows Vista (Client only)
 •  Windows 7
 •  Windows 2008
 
----------------------------

3. Contents of the DVD
----------------------------
This DVD contains the following files:
    
 •  CCURE_9000_Hybrid_DVR_Integration - HDVR Integration software (C•CURE 9000 HDVR Integration software)
 •  HDVR Integration User Guide.pdf
 •  CCURE9000_HDVR_Integration_readme.txt - Readme file

----------------------------

4. Installation
----------------------------
Perform the following steps to install the C•CURE 9000 HDVR Integration Interface:

Notes: You must install the HDVR Integration Interface in the same folder as 
       C•CURE 9000 v1.93. Also, you must have administrator privileges to do the 
       install. Otherwise the system displays the error message: "The system 
       administrator has set policies to prevent this installation."

       Before starting the installation process, stop the Crossfire Services.
 
 1. Insert the DVD into a DVD drive on your C•CURE 9000 system. The Connected Program Driver DVD
    Welcome screen should display automatically.
 2. The installation program determines if the correct version of C•CURE 9000 is installed on your system
    and if it is not, a message is displayed stating that V1.93 and later of 9000 is needed.
 3. Click the HDVR Integration button from the displayed list. The
    InstallShield Wizard begins installing the software, and after the initial 
    C•CURE 9000 splash screen displays, the HDVR Integration Interface 
    Welcome screen appears.
 4. Click Next and follow the Installshield Wizard prompts. (Software House 
    recommends that you accept all defaults during the installation process.)  
 5. Click Finish to complete the Installation and restart the computer.
 6. Restart the Crossfire Services
 7. Start ConnectedPro.HardwareInterface.HDVR.HardwareInterface
 8. Open the HDVR Integration User Guide.pdf and read the guide 
    for information about using the C•CURE 9000 HDVR Integration product. 
    


Hardware and Video Driver Manual Start

 •  After you have installed the C•CURE 9000 HDVR Integration Interface 
    Version 1.93, you must start the HDVR Integration Driver manually.
    
    To access: Click Start menu->Run command "Services.msc"->Start the service 
               "SoftwareHouse CrossFire HDVR Video Driver Service"

    (By default, the Server Components (Drivers) are not all started automatically 
    because enabling drivers for devices that are not used by the server can affect 
    system performance.)
----------------------------

5. Problems Fixed in this Release
----------------------------
This is the initial release of the HDVR Integration Interface product.
----------------------------

6. Limitations
----------------------------
 •  The HDVR Integration works on the following 32-bit operating systems only if 
    DEP is turned off by using the command "bcdedit /set nx alwaysoff":
	Windows Server 2008
	Windows 7
	Vista (Client only)
 •  If the video size is more than 20G, it is recommended to retrieve video clips 
    by splitting the video. 
 •  No support for exporting video files over 2G.


---------------------------- 

End of Readme File
