***********************************************************************************
C•CURE 9000 VideoEdge 4.0 Integration with C•CURE 9000 March 2011
Copyright © 2011 Tyco International Ltd. and its Respective Companies.
***********************************************************************************

This ReadMe file provides important information about the VideoEdge 4.0 Integration 
for C•CURE 9000 Version 1.93. Please read this file before installing the product.

************************************************************
*  Product: C•CURE 9000 VideoEdge 4.0 Integration Software
*  Release: Initial Release
*  Version: 1.93 Build 3362
*  VideoEdge 4.0 Integration version: 1.0.57.0
*  videoEdge 4.0 Software AD SDK Version: 4.1.112.15
*  Company: Software House (Tyco International)
*  Date: March, 2011

************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1. Overview
2. Features
3. Hardware Requirements
4. Software Requirements
5. Qualified Operating Systems
6. Qualified Hardware/Software
7. Contents of the Installation Kit
8. Pre-installation
9. Installation
10. Post-installation
11. Issues and Limitations

************************************************************
* 1. OVERVIEW
************************************************************

The C•CURE 9000 VideoEdge 4.0 Integration product provides advanced, seamless 
integration with videoEdge 4.0 interface. You can monitor and control your 
surveillance cameras, show video view, video tour, do PTZ controls, replay and 
export videos, also receive status and events from the C•CURE 9000 Monitoring Station.

************************************************************
* 2. FEATURES
************************************************************

The C•CURE 9000 VideoEdge 4.0 Integration software offers the following features:

 • Live video
 • Simultaneous live and recorded video views from up to 16 video cameras
 • Audio support
 • Import of camera information
 • VideoEdge 4.0 Camera status information
 • VideoEdge 4.0 video server status information
 • Monitor Video Server and Camera Events
 • Export of video to MP4 format
 • Playback of pre-recorded video
 • Video control such as PTZ (domes only)
 • Playback of pre-recorded video
 • Video Tours
 • PTZ presets based on event, alarm input or video tour
 • PTZ patterns based on event, alarm input or video tour
 • Display up to 4 live video layouts (4*4 view) at the same time based on an event with up to 64 cameras accross all layouts

************************************************************
* 3. HARDWARE REQUIREMENTS 
************************************************************

The minimum hardware requirements are as follows:

 • Intel Xeon CPU W3530 2.8GHZ
 • 4.00GB RAM
 • 250 GB SATA Hard Drive 7200 r.p.m.
 • 1000 Mbps Gigabit-Ethernet
 • Graphics card: NVIDIA Quadro FX 580 [2] (512 MB)
 • Intel X58 Chipset

************************************************************
* 4. SOFTWARE REQUIREMENTS 
************************************************************

The C•CURE 9000 VideoEdge 4.0 Integration requires the following software versions 
of C•CURE 9000 and VideoEdge 4.0:

 • C•CURE 9000 Security and Event Management System version 1.93 Build 3362

 • VideoEdge 4.0 version 4.00.828.00

    Close any running applications to avoid installation problems.

************************************************************
* 5. QUALIFIED OPERATING SYSTEMS
************************************************************

32-bit operating systems:

 • Windows XP Service Pack 3
 • Windows Vista Business
 • Windows 2003 Service Pack 2
 • Windows 7 Professional
 • Windows 2008 (see Issues and Limitations section)

64-bit operating systems:

 • Windows 7 Professional
 • Windows 2008 (see Issues and Limitations section)

************************************************************
* 6. QUALIFIED HARDWARE/SOFTWARE
************************************************************

 • VideoEdge 4.0 Dome cameras - Axis 214, IP Dome ADVEIPSD35P
 • VideoEdge 4.0 Fixed camera - ApproH ADCIPH2709BTP, Arecont AV1300 M-A, etc.
 • VideoEdge 4.0 software version 4.00.828.00

************************************************************
* 7. CONTENTS OF THE INSTALLATION KIT
************************************************************

The C•CURE 9000 VideoEdge 4.0 Integration software package contains the following items:

 • CCURE_9000_VideoEdge4.0_Integration_User_Guide.pdf - C•CURE 9000 (version 1.93) VideoEdge 4.0 Integration Software User Guide
 • CCURE_9000_videoEdge4.0_Integration_readme.txt - C•CURE 9000 VideoEdge 4.0 Integration Software ReadMe file
 • CCURE_9000_VideoEdge4.0_Integration.exe - VideoEdge 4.0 Integration software setup file
 • IsSetupPrequisites - Directory containing files needed for setup program
 • DirectX9c - Folder that contains several files for Directx9c

************************************************************
* 8. PRE-INSTALLATION
************************************************************

To perform the installation, you must have appropriate Windows permissions. You must 
have membership in the local Administrators group, or equivalent privileges. See the 
Microsoft Operating System document or your system administrator for more information.

************************************************************
* 9. INSTALLATION
************************************************************
Perform the following steps to install the C•CURE 9000 VideoEdge4.0 Integration:

Note: You must install the VideoEdge 4.0 Integration in the same folder as 
      C•CURE 9000 v1.93. Also, you must have administrator privileges to do the 
      install. Otherwise the system displays the error message: "The system 
      administrator has set policies to prevent this installation."

 1. Double-click the CCURE_9000_VideoEdge4.0_Integration.exe file.
 2. The installation program determines if the correct version of C•CURE 9000 
    is installed on your system, and if it is not, a message is displayed 
    stating that a supported version of C•CURE 9000 is needed.
 3. Click Next and follow the Install Wizard prompts. Software House recommends
    that you take the default selections (for example, a Server installation 
    should include both Client and Server options) during the installation process.
 4. Click Finish to complete the Installation, and use the Server Management 
    Application to start the Crossfire Service.
 5. Start ConnectedPro.HardwareInterface.VideoEdge4.HardwareInterface
 6. Open the VideoEdge 4.0 Integration User Guide.pdf and read the guide 
    for information about using the C•CURE 9000 VideoEdge 4.0 Integration product. 

************************************************************
* 10. POST-INSTALLATION
************************************************************

 1. From the Start Menu, select Start>All Programs>Software House>Server Configuration to open the C•CURE 9000 Server Management Application.
 2. Restart the CrossFire services and the Server Component Framework services.
 3. Verify the license for the VideoEdge 4.0 Integration by running C•CURE 9000 Licensing utility on the C•CURE 9000 server.
 4. Under Server Components tab, right-click ConnectedPro.HardwareInterface.VideoEdge4.HardwareInterface under Video and select Enable Server Component from
    the context menu, then select Start Server Component.
 5. When the server component icon for VideoEdge 4.0 Integration changes from Disabled (Red) to Enabled (Green), you can use the VideoEdge 4.0 Integration
    software.

You can also install C•CURE 9000 VideoEdge 4.0 Integration software on a local computer 
from a shared folder over a network.

************************************************************
* 11. ISSUES AND LIMITATIONS
************************************************************

 • Integration client features have not been fully qualified on Windows 2008.
 • View requests require a lot of resources (memory and display card), so you cannot open too many views at the same time (including views in tours). It is recommended to open fewer than 7 views at the same time. Otherwise, a D3D error may be encountered.
 • It will take a few seconds to open a view for the first time, but it will be faster next time.
 • In a live view with audio enabled, clicking the "Reconnect" button will deactivate the audio. Click the "Audio" button again to stream audio.
 • The "Reconnect" button doesn't work on 2x2, 3x3, and 4x4 views.
 • In maps, the VideoEdge 4.0 Server icon will only change to reflect the online, offline, and unknown states.
 • If you enable audio on playback mode and then switch back to live stream mode, the audio is still on.
 • The 1x5 and 2x8 views may open slowly, and a layout change will be evident.
 • The preset and pattern configured on tour cannot be triggered on the first time when open tour view, but can be triggered when sequenced the view at the second time.
 • When You add a VideoEdge 4.0 Camera into the view,only displays VideoEdge 4.0 server name and VideoEdge4.0 camera name, no video, in the camera preview window.
 • Video clips are exported in Native format .ISO, which includes MP4 files. You can open MP4 files to play recorded videos.
 • In 2x2 views, if you select one camera and then click the record button, all four cameras will record.
 • In 2x8 views, if you select one camera (other than the first one) and click the record button, the first camera will always record.
 • In Monitoring Station, if you click the record begin message to pop up a view to display recorded video for a PTZ camera, the View, PTZ, Preset, and Pattern buttons should be disabled but are not.


************************************************************

Copyright and Trademarks
C•CURE® and Software House are registered trademarks of Tyco International Ltd. 
and its respective Companies.

The trademarks, logos, and service marks displayed on this document are registered 
in the United States [or other countries]. Any misuse of the trademarks is strictly 
prohibited and Tyco International Ltd. will aggressively enforce its intellectual 
property rights to the fullest extent of the law, including pursuit of criminal 
prosecution wherever necessary. All trademarks not owned by Tyco International Ltd. 
are the property of their respective owners, and are used with permission or allowed 
under applicable laws.

Product offerings and specifications are subject to change without notice. Actual 
products may vary from photos. Not all products include all features. Availability 
varies by region; contact your regional sales manager.

Software version: C•CURE 9000 version 1.93.
Print Date: March, 2011

This manual is proprietary information of Software House. Unauthorized reproduction 
of any portion of this manual is prohibited. The material in this manual is for 
information purposes only. It is subject to change without notice. Software House 
assumes no responsibility for incorrect information this manual may contain.

All rights reserved.
Copyright © 2011 Tyco International Ltd. and its Respective Companies.

***********************************************************************************

End of ReadMe File


