Resolved CPR’s
CAMWorks 2012 – SP 3.2
CPR Number	Help Desk ID	Area	Description	
CW-35946	10-7181	System	When user installs CAMWorks 2013 SP 3.1 on a system with SolidWorks 2012, a Self-Registration error message is displayed but installation is successful and CAMWorks functions properly. Not observed on systems with SolidWorks 2013. 	
CW-35995	10-7210	Translation	Help of the Italian version of CAMWorks is not available. Instead the help files of French language are seen.	

CAMWorks 2012 – SP 3.1
CPR Number	Help Desk ID	Area	Description	
CW-35440	10-6928	System	When a SolidWorks part or assembly file is opened in SolidWorks 2013 by using the shortcut on RMB menu in windows explorer, then the CAMWorks data does not get restored. This works fine with SolidWorks 2012. 	

CAMWorks 2012 – SP 3.0
CPR Number	Help Desk ID	Area	Description	
CW-32281	10-5690	Toolpath	For the specific part, when Area Clearance operation is generated, the system goes into loop. This happens with the combination of CAMWorks 2012 with SolidWorks 2011.	
CW-32424	10-5753	Translation	In Japanese language version, the turn holder orientation ‘Down left’ is missing for turn operations.	
CW-32602	10-5852	Features	For the specific part, the part perimeter feature generated using Automatic feature recognition is incorrect when generated in SolidWorks 2012 SP 4.0 environment with CAMWorks 2012/2013.  The same was found to be correctly generated in SolidWorks 2012 SP 2.0 environment. 	
CW-33128	10-4585	Toolpath	For the specific part, SolidWorks crashes when the user selects the Area Clearance operation in the CAMWorks operation tree while the toolpath is being generated.	
CW-33797	----	System	For turn features, if the same tool is being used across different configurations, then the settings for hand condition of the holder is not retained after the file is saved and reopened.	
CW-33805	----	Toolpath	When extends are given for OD features, then variable allowance is not considered while tool paths are generated. 	
CW-34201	10-6336	Toolpath	CAMWorks toolpath does not update correctly for hole features between SolidWorks configurations.	
CW-34218	----	Configuration	While switching between configurations, the location of the toolpath changes for wrap features. Toolpath is corrected only on executing Generate Toolpath command. 	
CW-34223	10-6409	API	API ‘CreateMillFeature’ does not work properly for engrave features.	
CW-35057	10-6731	System	Turn and Mill turn files saved in CAMWorks 2012 SP3 version cannot be opened with CAMWorks2012 SP2 version. An error message is displayed.	

CAMWorks 2012 – SP 2.2
CPR Number	Help Desk ID	Area	Description	
CW-32845	----	Toolpath	When arc fit is enabled, the toolpath for the given open profile feature defined using a sketch changes and cuts in a different area.	
CW-32963	----	Features Rebuild	Rebuild of CAMWorks data in the assemblies saved in 2009 version results in features changing their setups.	
CW-33037	----	Post	For the specific part, in the case of bore rough operations, when the Program point is set to ‘tool nose tip’ in the Posting tab of Operation Parameters dialog, the NC codes are generated with respect to ‘tool nose center’ instead of ‘tool nose tip’.  	

CAMWorks 2012 – SP 2.1
CPR Number	Help Desk ID	Area	Description	
CW-32505	----	API	Face feature is not getting created through API. 	

CAMWorks 2012 – SP 2.0
CPR Number	Help Desk ID	Area	Description	
CW-23675	2-2926	Toolpath	Fixed OD Milling in a contour mill turn operation does not do a Rapid down to the start of the cut. It does a feed move instead, which is incorrect.	
CW-25918	10-1223	Simulation	For the specific part, SolidWorks and CAMWorks crashes when user tries to machine simulate this file after defining the stock with specific STL file and offset any axis by some value on 64-bit machine.	
CW-26862	10-1953	Simulation	For this specific part, when arc leadin is given for contour mill operation, the simulation shows an error and does not continue.	
CW-28877	10-3273	Post	In setup tab of machine definition, when origin offset is ‘non-rotated’, then the posted output is different than when ‘rotated’ is selected. Ideally, there should be no difference in post. 	
CW-28948	10-3355	Feature	For the specific part, SolidWorks crashes when Feature Recognition using MfgView is executed.	
CW-29474	10-3646	Toolpath	In this part when from WIP option is set to previous left over for rough mill then, the generated rough mill toolpath is not satisfactory. The previous operation defined is a face mill operation.	
CW-29113	10-3401	Feature	Feature segments are not getting highlighted by specific color when selected to define the variable allowance. This behavior was not observed in CW2011. 	
CW-29181	10-3444	Configuration	In EDM, when user adds two configurations and select a different make and model for both the configurations, then the machines are not saved for the configuration which is activated. 	
CW-29236	10-3479	Operation	In CAMWorks operations, if the checkbox of ‘Lock spindle speed’ is checked, then XY feedrate is not updated when spindle speed is changed. 	
CW-30004	10-3971	License	CAMWORKS FlexLM License Manager given in CW2012 DVD does not work with Windows Server operating machines. Teksoft.exe error message is displayed.	
CW-30107	10-4389	Translation	In the Polish language version of CAMWorks, when user does RMB on the setup in the CAMWorks Feature Tree and selects, ‘Insert Multi surface Feature’, the dialog that pops up doesn’t have any alignment and resultant dialog controls are not clear. This issue is not observed for any other language version.	
CW-30222	10-4104	Toolpath	For the specific part, rough mill toolpath generated for irregular pocket feature is incorrect. 	
CW-30277	10-4135	VoluMill	For the specific part, the Max cut amount value entered by the user for the VoluMill toolpath changes every time the focus shifts to a different tab in the Operation Parameters dialog. 	
CW-30280
CW-30438	10-4152,
10-4272	Features	For the specific part, when Feature extraction method is set to ‘Revolved Section’ and ‘Extract Machinable Features’ command is executed, then CAMWorks crashes out after some time. 	
CW-30335	10-4185	Operation	Camworks crashes when the specific part is opened with CAMWorks Add-in set to ‘Active’ in SolidWorks.	
CW-30344	10-4199	Toolpath	In Turn Finish operation, if the first entity of the feature is a fillet  and leadin is applied, then the toolpath does not cut the complete fillet and leaves some material. The leadin is applied at the wrong position on the feature.	
CW-30423	10-4264	Toolpath	For the specific part, in bore rough operation, if start length is defined under Feature Option tab of the Operation Parameters dialog, then the bore rough toolpath is not generated.	
CW-30424	10-4263	Toolpath	If a turn feature starts with a radius, then the step out amount or lead out is not applied to the last cut properly. It seems to be applied parallel to the cut move irrespective of the step out or lead out angle.	
CW-30479	10-4308	Toolpath	For the specific part, in, if the rest machining method is set to ‘Previous tool’ in the Rest tab for Constant Stepover operation and an avoid area is selected, then the toolpath is not generated. The error message is displayed for a very short time. 	
CW-30492		Toolpath	For the specific assembly, the toolpath generated for a 3 axis operation doesn’t lie within the defined contain area.	
CW-30493		Toolpath	If copying an operation with a contain area, while toolpath is generating, the contain area of the copied operation is rotated.	
CW-30495	10-3771	Operation	While inserting features in assembly mode, clicking on the new feature to generate operations will cause CAMWorks to crash.	
CW-30554	10-4360	Post	NC code for turn and bore finish toolpaths of parts saved in CW 2011 changes in CW2012 after executing ‘Generate Toolpath’ command. 	
CW-30665	10-4438	Post	Add post variable called "OPR_HAND_OF_TOOL" to store the "Hand" selection in the Turn tool holder tab.	
CW-30673
CW-31511	10-4429
10-4972
10-5097	Toolpath	For Part-perimeter features, the arcs in the feature get converted into splines and this results in toolpath having too many points. This behavior was not observed in CW 2011.	
CW-30672	10-4435	Operation	For the specific part’s pencil mill operation, if pencil mill pattern is selected as ‘Mixed’, then the option- ‘Enable Holder avoidance’ and ‘Calculate min tool protrusion’ do not work. 	
CW-30683	10-4437	Operation	This issue observed in 64-bit operating systems for centre drill operations. Under the Optimize tab of the Operation parameter dialog, when Corner option is selected and corner is set to ‘Bottom left’ and the same operation is edited after applying the changes, then SolidWorks crashes. No log files of the crash are created. 	
CW-30717	10-4475	Features Rebuild	For the specific part, grouped features are not getting rebuilt on executing full rebuild after changes are made in SolidWorks Pattern.	
CW-30743		Features Rebuild	For some parts, the OD feature created on Rebuild is incorrect and resultant toolpath gouges the part. This behavior was not observed in CW 2011.	
CW-30745	10-4496,
10-4512	Toolpath	For the specific part, when user regenerates the contour mill operation of Wrap engrave feature, CAMWorks crashes. 	
CW-30791	10-4535	Features	For the specific mill turn part file, turn features are not getting recognized at all.	
CW-30859	10-4581	Operation	CAMWorks loses gouge checking options in multiaxis mill operation.	
CW-30915	10-4585	Operation	For the specific part, while calculating multiple 3 axis operations, if we select 3 operations in the Operations tree (when other operations are being generated) and do a RMB, then CAMWorks crashes. 	
CW-31027	10-4714	Post	Create new Query System command for getting estimated machine time from Statistics tab of an operation. 	
CW-31055	10-4757	Post	Turn canned tapping cycle is not being output to posted code correctly. This behavior was not observed in CW 2011.	
CW-31260	10-4894	Operation	For the specific part CAMWorks crashes when parameters are changed in the 3 axis operation. 	
CW-31338	10-4951	Simulation	During simulation, the X direction of mill setup triad for the Mill-Turn machine is not seen at all during simulation. 	
CW-31380	10-4989	Features	For the specific part, when the Turn machine is selected and the sketch for the Base Revolve feature is edited, then CAMWorks crashes. This crash is observed only when the machine selected is a Turn machine and not for mill machines.	
CW-31420	10-5006	Features	For the specific part, CAMWorks crashes any of the turn features are edited.	
CW-31421	10-5007	Toolpath	For this specific turn part, when extends of the Turn ID feature are changed from Along Z to Along X, and roughing operation is regenerated, then the toolpath gets reversed. This behavior was not observed in CW2011. 	
CW-31441	10-5025	Operation	In Rough Turning operation, if canned cycle is selected on the Sub spindle, then the boundary goes in the wrong direction and the arcs are reversed.	
CW-31626	10-5162	Features	The filleted faces of tapered and filleted faces get highlighted when ‘Highlight Unrecognized Faces’ is selected from NC manager. Ideally they should not get highlighted as they are part of the feature recognized by CAMWorks.	
CW-31633	10-5148	TechDB	When TechDB of CAMWorks 2011 is imported in CAMWorks 2012 in SQL mode, the data does not get imported properly. The user gets blank fields.	
CW-31728	10-5214	Post	When posting a multiaxis operation in part mode and using an FCS, if not selecting the FCS in the setup the posted numbers are changing.	
CW-31762	10-5268	Toolpath	In multiaxis milling operation, while using Table/Table “0” configuration in the KIN file, the tool length comp is being added on to the toolpath.  	
CW-31872	10-5346	Rebuild	For the specific assembly, when user does a Full rebuild, all the operations get deleted. This behavior is not observed for Light Rebuild. 	
CW-31928	10-5394	Operation	4 and 5 axis preposition indexing for milling is not correct if the feature is a pattern. 	
CW-31933	10-5398	Operation	In assembly mode, when we split set up, output angles for tilt axis are not getting copied.	
CW-32424	10-5753	Translation	In Japanese language version of CAMWorks 2012, the holder orientation ‘Down Left’ is missing for Turn operations. 	

CAMWorks 2012 – SP 1.4
CPR Number	Help Desk ID	Area	Description	
CW-31028	10-4610	Simulation	If a Machine Simulation license is available, it cannot be selected from the NC Manager in Part mode as well as the Machine node in Assembly mode.	
CW-31223	-----	Post	In posting, add a query to retrieve the minimum tool protrusion length for 3 axis operations.	
CW-31811	10-5288	Post	In Posting, add new post variable for Corner Round and Countersink tool for effective diameter and end diameter	

CAMWorks 2012 – SP 1.3
CPR Number	Help Desk ID	Area	Description	
CW-31050, CW-31101	10-4812, 10-4737	System	In 4 axis and 5 axis machining, the option fixture co-ordinate system under Axis tab of part set up parameters dialog is not working.	

CAMWorks 2012 – SP 1.2
CPR Number	Help Desk ID	Area	Description	
CW-30857	-----	Post	In the APT CL output, the definition of the Bore, Ream and Tap tools is not correct. 	
CW-30563	-----	Post	Add ‘Dwell’ to posting tab for CAMWorks Drill, Bore and Ream cycles when APT CL post is selected. The types are: 
1.	Spot Drilling of centre drill operation, 
2.	Bore with Dwell of boring operation
3.	Ream with Dwell of ream operation	

CAMWorks 2012 – SP 1.1
CPR Number	Help Desk ID	Area	Description	
CW-30614	10-4387 	UI	“Fixture coordinate system" option is missing from mill part setup's axis tab	
CW-30495	10-3771	Features	When inserting features in assembly mode, right-clicking on the new feature to generate operations may cause CAMWorks to hang or to crash.	

CAMWorks 2012 – SP 1.0
CPR Number	Help Desk ID	Area	Description	
CW-24491	10-0289	System	While checking for the online service update, CAMWorks doesn’t display an error message if internet connection not there on the system.	
CW-25214	10-0713	EDM	In EDM tab of an EDM operation, the glue stop distance does not change  to new values when ‘Use same length’ parameter is unchecked in Glue Stops tab.	
CW-25651	10-1005	Toolpath	For the specific part’s contour mill operation, the depth processing settings when set to ‘depth by region’ incorrectly generates toolpaths for the ‘by level’ settings. Observed when side parameter values are given for multiple passes along with final cut amount pass.	
CW-25718	10-0750	UI	The machining depth or feature depth values for the operations on the multi surface features are erroneously displayed in setup sheets. 	
CW-25030	10-0548	Toolpath	Posted output of a lathe canned threading cycle has the wrong Z direction values	
CW-25541	10-0878	Toolpath	For the specific part, the rough mill toolpath generated for the open pocket feature with islands contains an unnecessary circular move which is gouges the part.	
CW-25677	10-1026	EDM	In EDM, for spline-based features, the lead-in and lead-outs are applied on the wrong side of the feature. 	
CW-25918	10-1223	System	CAMWorks crashes after updating axis offset values while machine simulating this part on Win 64 bit machine when define the stock with the attached STL file	
CW-26086	10-1382	Operation	In TechDB, when RPM in operations exceeds the max RPM defined in machine definition, then for the assembly, the feed rates do not get adjusted as per the RPM defined in machine definition. Observed in assembly mode and not in part mode.	
CW-26229	10-1458	TechDB	In TechDB, if thread mill operation is added to Multi Stepped hole and operations table, then in operation parameters, allowance, cut amt, final cut amt does not take decimal numbers.	
CW-26582	10-1738	Features	For the specific assembly, the display of the open profile feature defined using a sketch is transformed from its original location. The display is reset if user does Edit Definition on the feature.	
CW-26640	10-0320	Turn	After fix of CW-25110, the Axial (Z) clearance value doesn't affect the retract move of toolpath but if Radial (X) clearance value is changed, then it affects both the approach and retract move.	
CW-26642	10-0320	Toolpath	For the specific part, the defined Lead In/out for the finish Groove toolpath is not being applied to the toolpath. The toolpath enters into the part with a very small feed move which is impossible to control. 	
CW-26747	10-1776	Toolpath	For the specific assembly’s contour mill operation, the CNC comp changes direction when a negative allowance is set. 	
CW-26770
CW-28041	10-1896
10-2704	Turn	During toolpath simulation, the display of a user defined turn insert is a mirror display of how it is oriented in the operation. 	
CW-26927
CW-26955
CW-27300	10-1981
10-1991
10-2233	Features	For the specific part, rough mill operation created from Irregular Slot feature found from Mfgview gouges the part.	
CW-27073	10-2075	Turn	If the Window selection option in the ‘Insert Turn Feature’ dialog box is enabled and the segments are selected in the Graphics area, then the user cannot insert the feature by using the OK button at the top right corner of the display area.	
CW-27155	10-2154	Toolpath	For the specific part file, the roughing operation of Irregular Slot1 feature is incorrect. It does not completely machine the feature.	
CW-27167	10-2154	Toolpath	For the specific part, the contour mill operation generated for Irregular Slot feature is incorrect. It does not machine the feature completely.	
CW-27269	10-2209	Toolpath	Rough mill toolpath gouges islands of open pocket feature when optimization is selected in Optimize tab of the Operation parameters. Observed for parts created in CAMWorks 2009 version.	
CW-27277	10-2212	Features	For the specific part, the toolpath generated for the irregular slot recognized by MfgView gouges the part.	
CW-27333	10-2268	Features	For the specific part, the display of a pocket feature recognized by Interactive Feature Recognition is reversed. Due to this reversal, toolpath is not generated. However, when the user edits the pocket feature and closes it by clicking Finish the display gets corrected. 	
CW-27518	10-2382	TechDB	When TechDB is linked to SQL server, the user cannot update the Stock Material or Tool Material data in Feed/Speed section of the TechDB. An error message is displayed when the user clicks on the ‘Update Stock Material Data’ or ‘Update Tool Material Data’ buttons.	
CW-27556	10-2382	TechDB	If TechDB is linked to SQL database, then user cannot create or copy a new machine in Mill. User is able to create/copy in Turn and Mill-Turn.	
CW-27579	10-2398	Toolpath	For the specific part, If the sketch selected for the curve feature operation has an entity of size less than 0.012in, then a curve project operation is not generated for this curve feature.	
CW-27590	10-2396	EDM	In EDM 2axis profile the tab cut is cutting in the wrong direction.	
CW-27711	10-2483	Setup Sheet	If entry drill is defined for contour mill operation of all the features, then CAMWorks crashes while creating setup sheet in XML. It also does not generate the Setup Sheet in Access.	
CW-27853	10-2580	Simulation	In Assembly mode, while simulating the tool path, the X and Y axis display does not matches with the Mill part set up co-ordinate system. Rather it matches with Solid works co-ordinate system.	
CW-27964	10-2612	Post	In Assembly mode the posted code shows I, J and K vectors that are wrong which creates problems when posting.	
CW-27975	10-2653	Toolpath	For the specific part, when the user changes dimensions of the part within SolidWorks and does a full update, then the Flat area operation does not get generated. The user has to manually do the regeneration.	
CW-27978	10-2658	UI	In Turn and Mill/Turn, the stock manager doesn't differentiate between two sketches if the names of both sketches have some common alphabets at the beginning.	
CW-27994	10-2665	System	CAMWorks crashes on Edit Definition of stock manager after user renames the sketch which has been used to define the stock.	
CW-28091	10-2750	EDM	For the specific part, when the user selects ‘core less’ from the Glue stop dropdown list in the EDM tab of the Operation parameters dialog for an EDM contour operation.	
CW-28096	10-2735	Operation	When generating XML setup sheet for drill operation, the user gets a XY Feedrate value while actually there is no XY feedrate for drilling operations.	
CW-28212	10-2843	System	In Assembly, the Feed and Speed is not updated when user changes the machine unless user does Edit Definition of all the operations. This issue was fixed in Part mode.	
CW-28293	10-2893	Features	For the specific part, when the user right-clicks on the circular pocket present in the recycle bin, then CW crashes.	
CW-28579	10-3087	Features Rebuild	Multiaxis mill operation loses the curve definition for pattern on rebuild called after change in SolidWorks feature if the curve is selected by selecting the part edge.	
CW-28663	10-3133	Simulation	In CAMWorks 2011 & 2012, when the user generates XML setup sheet, the images displayed do not show origin. The origin was displayed in CAMWorks 2010.	
CW-28796	10-3308	Toolpath	For the specific part when Z allowance is changed to a different value from the X allowance for the Bore Rough operation, then the toolpath generated does not make required moves to rough out the feature.	
CW-28802	10-3221	Toolpath	For contour mill operations, when compensation is ‘on’ and leadin is selected as arc with leadin angle of 270 degrees, then additional toolpath is added in ‘leadin’. This is observed only in the display and the posted toolpath is a correct one.	
CW-29137	10-3421	VoluMill	Volumill tool path leaves material at the corners for Area Clearance Operations.	
CW-29143	10-3427	TechDB	Any post processor assigned to a mill machine using the TechDB form is not reloaded when TechDB is reopened. It is also not getting assigned to specific machine when the user selects the machine in CAMWorks.	
CW-29151	10-3435	Post	The APT output generated with Mill.aptctl doesn't generate input value for first peck and sub peck. It outputs 1000 times of the defined values.	
CW-29250	10-3461	System	CAMWorks selects out of limit angle pairs though valid indexing pairs for mill part setups are available as per the defined rotary/tilt limit. The valid pair gets selected if the ‘Edit Definition’ is done on machine node but it goes back to an invalid pair on sorting operations.	
CW-29265	10-3502	Features	In turn, mill turn and Wire EDM module, user cannot move features at the top position in the feature tree, Rather it moves to bottom of the tree.	
CW-29267	10-3503	Toolpath	For specific part file, flat area operation does not machine the entire flat surface. Leaves some bunch of toolpath in some areas.	
CW-29311	10-3506	System	When trying to choose another machine or update the current machine in a Machine Simulator the system will crash for this specific  assembly	
CW-29312	10-3531	Post	To handle patterns in drilling and milling within the posting output, two new variables need to be put into the posting system which will increment at every different feature and operation respectively, thus enabling easier handling of patterns.	
CW-29331	10-3553	Simulation	CAMWorks exception report is observed when user enters a Z offset in Machine Simulation and presses update button	
CW-29400
CW-30005	10-3602
10-3975	Features	In SolidWorks 2012, irrespective of CAMWorks version, when we insert a Mill part setup then it takes long time to show the mill part setup box. This issue is not observed when working in SolidWorks 2011.	
CW-29432	10-3615	Operation	CAMWorks exception report is observed when a start hint point is changed Pencil mill operation.	
CW-29444	10-3564	Post	For the specific part, the starting angle posted in the NC code is incorrect for a wrapped mill contour toolpath. 	
CW-29540	10-3681	VoluMill	For the attached part’s rough mill operation, when the user changes the pattern to ‘Volumill’, then the first cut amount is not updated and the down step taken in toolpath is wrong. The user has to turn off the percentage button and then turn it on again to correct the first cut and down step values.	
CW-29552	10-3665	Post	For the specific part, the operation posted using the Mill.apt post is incorrect for non-360 degree arcs. 	
CW-29594	10-3724	EDM	For the specific part, the 4 axis EDM toolpath generated is incorrect and causes the stock to be cut incorrectly.	
CW-29734	10-3809	VoluMill	For the VoluMill area clearance toolpaths, the contain area and avoid area do not observe the tool conditions option applied (on center/ upto / past). The only condition observed is ‘Upto’. 	
CW-29737	10-3808	VoluMill	In assembly mode, 3axis VoluMill toolpath doesn't consider the user defined ‘Set Z limit’ if the mill part setup is inserted by selecting face or plane which is below the selected user defined point. This issue is observed only in assembly mode and not in part mode.	
CW-29770	--	Translation	In the German translation version, for the Insert Pattern dialog, the right side of the controls is not visible.	
CW-29772	--	UI	For all Insert operation dialogs, the operation type dropdown list and toolpath image should be of the same width as all other controls in the dialog to ensure uniformity. 
This uniformity needs to be enforced the Insert Mill, Insert EDM and Insert Turn operation dialogs.	
CW-29773	--	System	In the CAMWorks Options/General tab, the controls for Configurations "Use CAMWorks configurations" and "Save with Document" are not stored as system defaults. Users who do not want to use these configurations need to disable this option for each new part which is time –consuming.	
CW-29796	--	Operation	In CAMWorks 2012, editing operations on a specific assembly file erroneously reports that the tool has changed though no changes were done.	
CW-29799	--	VoluMill	In this particular assembly, the VoluMill toolpath doesn’t observe the minimum Z depth defined and goes below the defined value. 	
CW-29812	10-3863	Operation	User defined turn insert doesn't orient itself correctly if front turret is selected. Due to this, display of insert with holder is not proper in case if left up, left down and other orientation. This affects the toolpath generation.	
CW-29814	10-3865	Features Rebuild	In assembly mode, features are not getting rebuilt properly. When a feature is changed in SolidWorks, then a new feature is created. Old features are not updated. This is observed only for MfgView and not in AFR.	
CW-29822	10-3863	Toolpath	For the specific part, bore finish toolpath generated with a user defined insert gouges the part and doesn't consider the user defined z end point.	
CW-29851	--	EDM	For the attached part, when the user tries to edit the EDM operation or generate EDM toolpath for the open profile feature, its causes CAMWorks to hang.	
CW-29915	10-3333	Operation	Following issue is observed the system contains "," (comma) as a decimal point. In such a case, in feature and operations of Mill, when the user clicks on parameters to define tool, then an error message pops up if user selects a tool from the tool library.	
CW-29963	10-3559	Post	Face Milling with Free option selected does not create the correct movements on Front turret.	
CW-30225	10-4108	Post	For the specific post, compensation and radius direction codes are not being output in the NC code but the same works with tutorial post. 	
CW-30233
CW-30226	10-4106	Post	Tool comments are not posted with CAMWorks 2012 tutorial posts.	
CW-30281	10-4153	System	CAMWorks doesn't allow overriding the setup Rotary/Tilt indexing angle with a negative value although the rotation direction is set to both. This was working in CAMWorks 10 SP3.1. With override it should accept any value.	
CW-30283	10-4150	System	In Assembly, mill part setup origin location defined under CAMWorks feature tree doesn't retain itself on rebuild. It gets back to the default location. On doing Edit Definition, it again comes back to the defined location.	
CW-30285	10-4155	System	If split setup is done from a setup which was also previously generated by splitting a setup, then it links all these setups although all the previous setups were unlinked. Due to this, it losses any changes made in the previous setups.	
CAMWorks 2012 – SP 0.1
CPR Number	Help Desk ID	Area	Description	
CW-28908	----	System	In Mill, while working with 5 Axis rotary, if the direction of rotation for the 5th axis is changed from clockwise to counterclockwise, then the following error message is displayed when editing the mill setup:
“Please enter a value between -3600 and 00.”	
CW-28907	10-3379 
10-3344 
10-3384	Operation	The mill tool crib option for filtering tools does not work in CAMWorks 2012 SP0.0. 

All tools are displayed in the window regardless of the diameter range entered.  	

CAMWorks 2012 – SP 0.0
CPR Number	Help Desk ID	Area	Description	
CW-28340	----	Toolpath	The toolpath for turn finish is not correct when a User Defined Insert. 	
CW-28093	10-2752 	
Help	CWPartFinder had been discontinued from CW2010 but the details could still be found in CW Utilities help file. The description of CWPartFinder has to be deleted from the help file.	
CW-27707	----	Toolpath	In turning, the Tip offset control does not modify the display and posted output as it is supposed to for user defined inserts.	
CW-27405	10-2226	Post	When posting with Subroutines, only one sub was created for two different rotary planes. 	

CAMWorks 2012 – Pre Release 1
CPR Number	Help Desk ID	Area	Description	
CW-28541	10-3048 	
Toolpath	In this part file, CW crashes while generating toolpath for a specific contour mill operation which includes a contain area, when bottom finish checked. 	
CW-28537	10-3047 	Post	In this assembly file, CAMWorks crashes when post processing using the APT mill post. 	
CW-28372	10-2947	Operation	CAMWorks results in an exception report when if the stock is edited. 	
CW-28072	Beta-2012
	Operation	We cannot save a file of .stl extension type in CAMWorks. Also if we have .stl file, it cannot be used as stock in SolidWorks2012-CAMWorks2012.	
CW-27225	10-2182 	Toolpath	In the attached part, face finish and bore finish tool paths are not generated as per the defined allowance and gouges the part.	
CW-23705	2-2850 	Help	On the Turn operation->NC tab, the description written in the Help file for the parameters radial, axial and retract distance are incorrect.	
CW-27580	10-2399 	Toolpath	In the turn module, Z limits for single point operations like center drill, drill and tap are working reverse of what they should be i.e. Z start works as Z end and vice versa. 	
CW-28507	10-3018 	Simulation	In this assembly file, the triad shown in simulation is not correct. The X and Y axes are flipped. 	
CW-28281	10-2882	Toolpath	In the attached part, the turn finish toolpath for the  OD feature gouges the adjoining face of the part.	
CW-25727	10-1056	TechDB	In the TechDB, the Center drill operation from the “No center drill” strategy needs to be deleted.	
CW-26469	10-1666 	Help	Modify the help file for VoluMill, regarding the spiral entry move for features containing open air edges.	
CW-27707	---	Operation	In turning, the Tip offset control does not modify the CL and posted output as it is suppose to for user defined inserts.	
CW-28435	---	Operation	GTP is not called on changing the "Approach is rapid" setting for turn operations.	
CW-28291	---	Toolpath	Contour mill tool path extends beyond the feature in the attached part. 	
CW-27552	---	Toolpath	Rough and finish turn toolpaths generate on the wrong side of the feature.	

CAMWorks 2012 – Beta
CPR Number	Help Desk ID	Area	Description	
CW-27790	---	Toolpath	Toolpath Statistics don’t get updated on changing the feed/speed of VoluMill  toolpaths	
CW-27596	10-2410	Operation	In contour mill operations, when the Cut Depth is Retract to Clearance OR leadin overlap is more than 0, then the Final Feedrate of Side final passes (side parameters setting of contour tab) is not considered.	
CW-27784	10-2528	Operation	The contour mill operation not turning "Off" CNC comp and turning "On" again for the last pass when Stay down selected.	
CW-27709	---	Turn	On this turn part the Z extents at certain values will stop the toolpath from generating	
CW-25643	10-0993	UI	In open pocket feature, the blue-point indicator that defines start point for leadin/out works opposite when the Cut depth-Stay down option is On.	
CW-27756	10-2459	Toolpath	In milling, the arc center is not correct when doing thread milling with leadout overlap.	
CW-27633	10-1757	TechDB	The Allowance field in the thread mill operation, for an MSHole feature, doesn't accept decimal values in the TechDB. It does accept it if thread mill is defined for other features.	
CW-26382	10-1552	UI	In the tool tab of any operation parameters, the Tool Number field can be changed by simply scrolling the mouse wheel. This behavior should be blocked as this information is critical and major change can happen with simple scrolling	
CW-27445	10-2335	Operation	CW does not look at the tools in the selected tool crib, when generating operations.	

CAMWorks 2012 – Alpha
CPR Number	Help Desk ID	Area	Description	
CW-27795	---	Operation	When 2 axis rough pattern is Offset Roughing, the ‘contain’ and ‘avoid’ areas create and edit extremely slowly.	
CW-27704	10-2437	Toolpath	In Lathe roughing operations, when selecting between CNC Comp "On" and "Off", the user does not get toolpath regeneration.	
CW-27152	10-2124	Mill	The spin box does not work properly for 3axis mill operations for inch as well as for metric system. 	
CW-27075	10-2076	VoluMill	Maintain Climb/Conventional option available under mirror option doesn't work for VoluMill toolpath. The toolpath with climb cutting direction becomes in conventional.	
CW-21758	2-2001	TechDB	In TechDB- area clearance operation, entry/retract tab, leadin angle is not activated. The user cannot do GOP and SOP.	
CW-26660	10-0320	Turn	In turning for all the point to point toolpaths like, center drill, drill, tapping etc, the approach and retract method always remains as X then Z and Z then X respectively if Auto is selected. User has no control on the same.	
CW-25460	10-0818	Toolpath	Canned boring cycle facing moves are in the opposite direction of what the system cycle toolpath is going. 	
CW-26525	10-0868	Toolpath	Contour Mill toolpath for a boss feature with Ramp at 45 degrees and cleanup pass selected doesn't generate correct toolpath.