; Extended DOS NIF file

[E100B]
   Type = NDIS
   Title = Intel(R) PRO/100 Network Connection
   Version = 4.58
   Drivername = E100B$
   Xports = NETBEUI LANDD

[FILE]
   Name = E100B.DOS

[SPEED]
   display = "Media Speed"
   type = Decimal
   set = 10, 100
   optional = YES
   editable = YES
   help = "The driver can configure the adapter for either 10 or 100 Mbps.
 Assigning a value to this parameter will override the Auto-Speed-Sense feature
 of the driver.  Leave the field blank to enable the Auto-Speed-Sense feature."

[FORCEDUPLEX]
   display = "Force Duplex Mode"
   type = Decimal
   set = 1, 2
   optional = YES
   editable = YES
   help = "The driver can configure the adapter for either Half or Full Duplex.
 Automatic detection of Full Duplex REQUIRES a hub with ports which are capable
 of performing N-Way auto-negotiation, so forcing the duplex mode to Full is
 recommended for most users connecting to a Full Duplex hub.  Assigning a value
 of 1 (Half) or 2 (Full) to this parameter will override the auto-negotiation
 feature of the adapter, and will also make the SPEED parameter REQUIRED.
 Leave the field blank to enable the auto-negotiation feature."

[SLOT]
   display = "Slot/Device Identifier"
   type = Hexadecimal
   range = 0-1FFF
   optional = YES
   editable = YES
   help = "Use of this parameter is only required in systems with more than one
 adapter installed. If you are installing more than one PCI adapter: 1) complete
 the configuration process, but leave the Slot field blank for each driver;
 2) restart the system and record the list of Slots that each driver displays;
 3) complete the configuration by assigning one of the values from the list to
 the Slot parameter of each driver. Leave the field blank if you have only one
 adapter installed."

[NODE]
   display = "Locally Administered Address"
   type = String
   strlength = 12
   optional = YES
   editable = YES
   help = "Use of this parameter to modify the network address used by
 the adapter."
