# iSCSI Target Configuration

For specific information on configuring your iSCSI target system and disk volume, refer to instructions provided by the 3rd party vendor. Listed below are the basic steps necessary to setup Intel® iSCSI Remote Boot to work with most iSCSI target systems. The specific steps will vary from one vendor to another.

| NOTE: In order to be able to support iSCSI Remote Boot, the target needs to be able to support multiple sessions from the same initiator. Both the iSCSI Remote Boot firmware initiator and the OS High Initiator need to establish an iSCSI session at the same time. Both these initiators use the same Initiator Name and IP Address to connect and access the OS disk but these two initiators will establish a different iSCSI session. In order for the target to support iSCSI Remote Boot, the target must be capable of supporting multiple sessions and client logins.

1. Configure a disk volume on your iSCSI target system. Note the LUN ID of this volume for use when configuring in Intel iSCSI Remote Boot firmware setup.

2. Note the iSCSI Qualified Name (IQN) of the iSCSI target, which will likely look like:

   `iqn.1986-03.com.intel:target1`

   This value will be used as the iSCSI target name when configuring in Intel iSCSI Remote Boot firmware setup.

3. Configure the iSCSI target system to accept the iSCSI connection from the iSCSI initiator. This usually requires listing the initiator's IQN name or MAC address for permitting the initiator to access to the disk volume. See the section "Firmware Setup" for information on how to set the iSCSI initiator name.

4. One-way authentication protocol can be enabled optionally for secure communications. Challenge-Handshake Authentication Protocol (CHAP) is enabled by configuring username/password on iSCSI target system. For setting up CHAP on the iSCSI initiator, refer to the section "Firmware Setup" for information.

`Last modified on 5/28/10 9:51a Revision 7`