 /************************************************************************
*                                                                       *
*               INTEL CORPORATION PROPRIETARY INFORMATION               *
*  This software is supplied under the terms of a license agreement or  *
*  nondisclosure agreement with Intel Corporation and may not be copied *
*   or disclosed except in accordance with the terms of that agreement. *
*        Copyright (c) 2008 Intel Corporation. All Rights Reserved.     *
*                                                                       *
************************************************************************/
/***********************************************************************\
*
* NAME:	Ncs2IVL.mof	
* 
* DESCRIPTION: Master MOF file with class definitions for the 
*			   Intel PRO Network VLANs (802.3 schema).
*
* PREREQUISITE: Ncs2Cm.mof and Ncs2ICr.mof [In that order]
*
* NOTE:	This file generates language neutral MOF for IntelNcs2 namespace.
*		This file also generates ENU language specific MFL. 
*
\***********************************************************************/

#pragma namespace ("\\\\.\\Root\\IntelNcs2")


// ============================================================================
// VLAN class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
		 Description("IANet_VLAN objectifies "
		 "the properties of a VLAN.  All of the needed properties "
		 "of the VLAN object are inherited from CIM_VLAN."):Amended,  LOCALE(0x409)
		]
class IANet_VLAN : CIM_VLAN
{
		[Description (
		 "VLANName is the name of the VLAN as chosen by the user."):Amended
		]
	string VLANName;

		
	  [Description (
	   "Contains the VLAN's parent device ID."): Amended]
    string ParentID;

	[Description (
	"Contains the VLAN's parent device type."):Amended,
	ValueMap{"0", "1", "2"}:Amended,
	Values {"Adapter", "Team", "Unknown"} : Amended
	]
    uint16 ParentType;
	[Description (
        "The StatusInfo property indicates whether the Logical"
        "Device is in an enabled (value = 3), disabled (value = "
        "4) or some other (1) or unknown (2) state. If this "
        "property does not apply to the LogicalDevice, the value, "
        "5 (\"Not Applicable\"), should be used.  "
        "If a Device is (\"Enabled\")(value=3), it has been "
        "powered up, and is configured and operational.  The Device "
        "may or may not be functionally active, depending on whether "
        "its Availability (or AdditionalAvailability) indicate that "
        "it is (\"Running/Full Power\")(value=3) or (\"Off line\")"
        "(value=8). In an enabled but offline mode, a Device may be "
        "performing out-of-band requests, such as running Diagnostics.  "
        "If (\"Disabled\") StatusInfo value=4), a Device can only be " 
        "\"enabled\" or powered off.  In a personal computer environment, "
        "(\"Disabled\") means that the Device's driver is not "
        "available in the stack. In other environments, a Device can "
        "be disabled by removing its configuration file. A disabled "
        "device is physically present in a System and consuming "
        "resources, but cannot be communicated with until a load "
        "of a driver, a load of a configuration file or some other "
        "\"enabling\" activity has occurred."): Amended,
       ValueMap {"1", "2", "3", "4", "5"}: Amended,
       Values {"Other", "Unknown", "Enabled",
               "Disabled", "Not Applicable"}: Amended
	]
       
   uint16 StatusInfo;

   [Description (
	"ValidateSetting validates the vlan settings. The 1st input parameter Adapter "
	"is a reference to an IANet_PhysicalEthernetAdapter for which the setting is "
	"validated. Value is the setting value. SettingName is the vlan setting. "
	"ValResult is the validated result."
	):Amended, implemented
	]
	uint32 ValidateSetting(
		[IN]	string SettingName,
		[IN] sint64 Value,
		[OUT] uint64 ValResult
	);


};

// ============================================================================
// 802.1Q VLAN Service Class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  Description (
         "If the NIC supports 802.1Q, an instance of this class will "
         "be instantiated"):Amended,  LOCALE(0x409) ]
class IANet_802dot1QVLANService : CIM_802dot1QVLANService
{
		[write, Description(
		 "GVRP (GARP VLAN Registration Protocol) is used by workstations and "
		 "switches to dynamically create, change and remove VLANs from across "
		 "a network.  This protocol allows VLAN switches which support GVRP "
		 "to determine which VLANs are active and to identify their switch ports. "
		 "The GVRPEnabled value indicates the GARP VLAN Registration Protocol active status."):Amended
		]
	boolean GVRPEnabled;
		
		[write, Description(
		 "GVRP (GARP VLAN Registration Protocol) is used by workstations and "
		 "switches to dynamically create, change and remove VLANs from across "
		 "a network.  This protocol allows VLAN switches which support GVRP "
		 "to determine which VLANs are active and to identify their switch ports. "
		 "GVRPJoin time sets the frequency of messages issued when a new port "
		 "has been added to the VLAN."):Amended,
		
		  ValueMap { "100", "150", "200", "250", "300", "350", "400", "450",
				   "500",  "550", "600", "650", "700", "750", "800", "850",
				   "900",  "950", "1000" }:Amended,


		  Values { "100 ms", "150 ms", "200 ms", "250 ms", "300 ms", "350 ms", "400 ms", "450 ms",
				   "500 ms",  "550 ms", "600 ms", "650 ms", "700 ms", "750 ms ", "800 ms", "850 ms",
				   "900 ms",  "950 ms", "1000 ms" }:Amended ]
	uint32 GVRPJoinTime;

		[Description(
		 "CreateVLAN is used to create a new VLAN for this service."):Amended,
		 implemented
		]

	uint16 CreateVLAN( [in] uint32 VLANNumber, [in] string Name,
					   [out] IANet_VLAN REF VLANpath );
};

// ===================================================================
// IANet_Device802dot1QVVLANServiceImplementation
// ===================================================================
   [dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"), Association,
    Description (
       "An association between a Service and how it is implemented. "
       "The cardinality of this association is many-to-many. "
       "A Service may be provided by more than one Logical"
       "Device, operating in conjunction.  And, any Device may "
       "provide more than one Service.  When multiple Devices are "
       "associated with a single Service, it is assumed that these "
       "elements operate in conjunction to provide the Service.  If "
       "different implementations of a Service exist, each of these "
       "implementations would result in individual instantiations "
       "of the Service object.  These individual instantiations "
       "would then have associations to the unique implementations."):Amended,  LOCALE(0x409)
   ]
class IANet_Device802dot1QVLANServiceImplementation : CIM_Dependency
{
      [Override ("Antecedent"),
       Description ("The LogicalDevice."):Amended
      ]
   IANet_EthernetAdapter REF Antecedent;
      [Override ("Dependent"),
       Description ("The Service implemented using the LogicalDevice."):Amended
      ]
   IANet_802dot1QVLANService REF Dependent;
};

// ============================================================================
// VLAN For class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  Association, Description(
		 "The  IANet_VLAN used by the IANet_802dot1QVLANService."):Amended,  LOCALE(0x409) ]
class IANet_VLANFor : CIM_VLANFor
{
};

// ============================================================================
// Device Service Implementation class
// ============================================================================
		[Association,dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"), 
		 Description (
         "An association between a Service and how it is implemented. "
         "The cardinality of this association is many-to-many. "
         "A Service may be provided by more than one Logical"
         "Device, operating in conjunction.  And, any Device may "
         "provide more than one Service.  When multiple Devices are "
         "associated with a single Service, it is assumed that these "
         "elements operate in conjunction to provide the Service.  If "
         "different implementations of a Service exist, each of these "
         "implementations would result in individual instantiations "
         "of the Service object.  These individual instantiations "
         "would then have associations to the unique implementations."):Amended,  LOCALE(0x409)
		]
class IANet_Device802dot1QVLANServiceImplementation : CIM_DeviceServiceImplementation
{
	[Override ("Antecedent"),
       Description ("The LogicalDevice."): ToSubclass Amended
      ]
    IANet_EthernetAdapter REF Antecedent;
      [Override ("Dependent"),
       Description ("The Service implemented using the LogicalDevice."): ToSubclass Amended
      ]
    IANet_802dot1QVLANService REF Dependent;
	
};




// ============================================================================
// Intel IANet_VLANSetting Abstract Base Class
// ============================================================================
		[Abstract, IANet_ModuleIdentifier("Ncs2Vlan.dll"),
		 Description("IANet_VLANSetting objectifies VLAN instance related "
		 "driver and network device settings. IANet_VLANSetting is an "
		 "Abstract superclass for a set of concrete classes of different "
		 "types.  This set of classes allows open ended usage of a variable "
		 "number of settings." 
		):Amended,  LOCALE(0x409)
		]
class IANet_VLANSetting : IANet_Setting
{

};


// ============================================================================
// VLANSetting Int Class
// ============================================================================

		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
		 Description("IANet_VLANSettingInt objectifies VLAN related "
		 "driver and network device settings. IANet_VLANSettingInt " 
		 "specifically handles Integer settings. The following "
		 "constraints are placed on the CurrentValue and default value:\n"
		 "	min <= CurrentValue <= max\n"
		 "	( CurrentValue - base ) is a multiple of step\n"):Amended,  LOCALE(0x409)]
class IANet_VLANSettingInt : IANet_VLANSetting
{
		[Description(
		 "Min is the minimum value that the integer can take."):Amended]
	sint64 min;

		[Description(
		 "Max is the maximum value that the integer can take."):Amended]
	sint64 max;

		[Description(
		 "Step is the granularity of the integer value."):Amended]
	sint64 step;

		[Description(
		 "Base is the root from which the integer value may take values. i.e. "
		 " CurrentValue - base is a multiple of step."):Amended]
	uint64 base;

		[Description(
		 "DefaultValue is the initial value of the parameter."):Amended]	
	sint64 DefaultValue;

		[Write, Description(
		 "CurrentValue is the actual value of the parameter - this is the only attribute that "
		 "the user can change."):Amended]	
	sint64 CurrentValue;

		[Description(
		 "Scale is unit of measurement to set or estimate series of marks "
		 "or points at known intervals to measure value of the parameter."):Amended]	
	sint64 Scale;
	
};

// ============================================================================
//  VLAN Setting Enum Class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
		 Description("IANet_VLANSettingEnum objectifies VLAN related "
		 "driver and network device settings. IANet_VLANSettingEnum " 
		 "specifically handles Enumeration settings"):Amended,  LOCALE(0x409)
		]
class IANet_VLANSettingEnum : IANet_VLANSetting
{
		[Description(
		 "PossibleValues is an array of the possible values allowed for the enum."):Amended
		]	
	sint64 PossibleValues[];
		
		[Description(
		 "DescriptionMap describes what each value means."):Amended
		]	
	string DescriptionMap[];
		
		[write, Description(
		 "CurrentValue is the current setting for this parameter."):Amended
		]	 
	sint64 CurrentValue;
		
		[Description(
		 "DefaultValue is the initial setting for this value."):Amended
		]
	sint64 DefaultValue;
};

// ============================================================================
//  VLAN Setting Slider Class
// ============================================================================
    [dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
    Description("IANet_VLANSettingSlider objectifies VLAN related "
    "driver and network device settings. IANet_VLANSettingSlider " 
    "specifically handles Slider settings"):Amended,  LOCALE(0x409)
    ]
class IANet_VLANSettingSlider : IANet_VLANSetting
{
		[Description(
		 "PossibleValues is an array of all the possible values.  The values "
		 "should be arranged with the first value on the left of the slider and "
		 "the last value on the right. "):Amended
		]
	sint64 PossibleValues[];
		[write, Description(
		 "CurrentValue is the current setting for this parameter."):Amended
		] 
	sint64 CurrentValue;

		[Description(
		 "DefaultValue is the initial setting for this parameter."):Amended
		]
	sint64 DefaultValue;
		
		[Description(
		 "FirstLabel is the label that should be displayed on the left of the slider."):Amended
		]
	string FirstLabel;
		[Description(
		 "LastLabel is the label that should be displayed on the right of the slider."):Amended
		]
	string LastLabel;
};

// ============================================================================
//  VLAN Setting Multi Selection Class
// ============================================================================
    [dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
    Description("IANet_VLANSettingMultiSelection objectifies VLAN related "
    "driver and network device settings. IANet_VLANSettingMultiSelection " 
    "specifically handles Multi Selection settings."):Amended,  LOCALE(0x409)
    ]

class IANet_VLANSettingMultiSelection : IANet_VLANSetting
{
		[Description(
		 "PossibleValues is an array of all the possible selections."):Amended
		]
	sint64 PossibleValues[];
		[Description(
		 "DescriptionMap is an array of descriptions of the possible selections."):Amended
		]
	string DescriptionMap[];
		[write, Description(
		 "Current value is a bit-wise OR of the currently chosen options from the "
		 "possible values."):Amended
		] 
	sint64 CurrentValue;

		[write, Description(
		 "Default value is a bit-wise OR of the default options from the "
		 "possible values."):Amended	
		] 
	sint64 DefaultValue;
	
};

// ============================================================================
//  VLAN Setting String Class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
		 Description("IANet_VLANSettingString objectifies VLAN related "
		 "driver and network device settings. IANet_VLANSettingString " 
		 "specifically handles String settings."):Amended,  LOCALE(0x409)
		]
class IANet_VLANSettingString : IANet_VLANSetting
{
		[Description("MaxLength is the maximum length of the string."):Amended]
	uint32  MaxLength;

		[write, Description("CurrentString is the current value for the parameter."):Amended] 
	string  CurrentValue;

		[Description("DefaultString is the initial value for the parameter."):Amended]
	string  DefaultValue;
};

// ============================================================================
//  VLAN Setting Multi-String Class
// ============================================================================
		[dynamic, provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll"),  
		 Description("IANet_VLANSettingMultiString objectifies MultiVLAN related "
		 "driver and network device settings. IANet_VLANSettingString " 
		 "specifically handles multi-String settings."):Amended,  LOCALE(0x409)
		]
class IANet_VLANSettingMultiString : IANet_VLANSetting
{
		[Description("MaxLength is the maximum length of the string."):Amended]
	uint32  MaxLength;

		[write, Description("CurrentString is the current values for the parameter."):Amended] 
	string  CurrentValues[];

		[Description("DefaultString is the initial value for the parameter."):Amended]
	string  DefaultValue;
};


// ============================================================================
// IANet_VLANToSettingAssoc class
// ============================================================================
[   Association, Description("This class associates Intel NICs with their respective settings.")
                :Amended,  LOCALE(0x409),
    Dynamic,
    Provider("Ncs2"), IANet_ModuleIdentifier("Ncs2Vlan.dll")
]
class IANet_VLANToVLANSettingAssoc  : CIM_ElementSetting
{
   [  Override("Element"),
      Description ("The VLAN to which the Setting object belongs."):Amended
   ]
   IANet_VLAN REF Element = NULL;
   [  Override("Setting"),
      Description ("The Setting belonging to the VLAN."):Amended
   ]
   IANet_VLANSetting REF Setting = NULL;
};




