// Copyright (c) 2005 DMTF.  All rights reserved.
// <change cr="ArchCR00066.004" type="add">Add UmlPackagePath
// qualifier values to CIM Schema.</change>
// ==================================================================
//  CIM_PowerManagementCapabilities 
// ==================================================================
   [Version ( "2.7.0" ), 
    UMLPackagePath ( "CIM::Core::PowerMgmt" ), 
    Description ( 
       "A class derived from Capabilities that describes the power "
       "management aspects of an element (typically a system or "
       "device). The element\'s power management capabilities are "
       "decoupled from a PowerManagementService, since a single "
       "service could apply to multiple elements, each with specific "
       "capabilities." )]
class CIM_PowerManagementCapabilities : CIM_Capabilities {

      [Description ( 
          "An enumeration indicating the specific power-related "
          "capabilities of a managed element. Since this is an "
          "array, multiple values may be specified. The current "
          "values in the enumeration are: \n"
          "0 = Unknown \n"
          "1 = Other \n"
          "2 = Power Saving Modes Entered Automatically, describing "
          "that a managed element can change its power state based "
          "on usage or other criteria \n"
          "3 = Power State Settable, indicating that the "
          "SetPowerState method is supported \n"
          "4 = Power Cycling Supported, indicating that the "
          "SetPowerState method can be invoked with the PowerState "
          "input variable set to \'Power Cycle\' \n"
          "5 = Timed Power On Supported, indicating that the "
          "SetPowerState method can be invoked with the PowerState "
          "input variable set to \'Power Cycle\' and the Time "
          "parameter set to a specific date and time, or interval, "
          "for power-on." ), 
       ValueMap { "0", "1", "2", "3", "4", "5" }, 
       Values { "Unknown", "Other", 
          "Power Saving Modes Entered Automatically", 
          "Power State Settable", "Power Cycling Supported", 
          "Timed Power On Supported" }, 
       MappingStrings { "MIF.DMTF|System Power Controls|001.2" }, 
       ModelCorrespondence { 
          "CIM_PowerManagementCapabilities.OtherPowerCapabilitiesDescriptions", 
          "CIM_PowerManagementService.SetPowerState" }]
   uint16 PowerCapabilities[];

      [Description ( 
          "An array of strings describing an element\'s additional "
          "power management capabilities, used when the "
          "PowerCapabilities array includes the value 1, \"Other\"." ), 
       ModelCorrespondence { 
          "CIM_PowerManagementCapabilities.PowerCapabilities" }]
   string OtherPowerCapabilitiesDescriptions[];

      [Description ( 
          "An enumeration that indicates the power states supported "
          "by a managed element. Because this is an array, multiple "
          "values can be specified. The current values in the "
          "enumeration are: \n"
          "2=On, corresponding to ACPI state G0 or S0 or D0. \n"
          "3=Sleep - Light, corresponding to ACPI state G1, S1/S2, "
          "or D1. \n"
          "4=Sleep - Deep, corresponding to ACPI state G1, S3, or D2.\n"
          "5=Power Cycle (Off - Soft), corresponding to ACPI state "
          "G2, S5, or D3, but where the managed element is set to "
          "return to power state \"On\" at a pre-determined time. \n"
          "6=Off - Hard, corresponding to ACPI state G3, S5, or D3. \n"
          "7=Hibernate (Off - Soft), corresponding to ACPI state "
          "S4, where the state of the managed element is preserved "
          "and will be recovered upon powering on. \n"
          "8=Off - Soft, corresponding to ACPI state G2, S5, or D3. "
          "9= Power Cycle (Off-Hard), corresponds to the managed "
          "element reaching the ACPI state G3 followed by ACPI "
          "state S0. \n"
          "10=Master Bus Reset, corresponds to the system reaching "
          "ACPI state S5 followed by ACPI state S0. This is used to "
          "represent system master bus reset. 11=Diagnostic "
          "Interrupt (NMI), corresponding to the system reaching "
          "ACPI state S5 followed by ACPI state S0. This is used to "
          "represent system non-maskable interrupt. 12=Off - Soft "
          "Graceful, equivalent to Off Soft but preceded by a "
          "request to the managed element to perform an "
          "orderlyshutdown. \n"
          "13=Off - Hard Graceful, equivalent to Off Hard but "
          "preceded by a request to the managed element to perform "
          "an orderly shutdown. \n"
          "14=Master Bus Rest Graceful, equivalent to Master Bus "
          "Reset but preceded by a request to the managed element "
          "to perform an orderly shutdown. \n"
          "15=Power Cycle (Off - Soft Graceful), equivalent to "
          "Power Cycle (Off - Soft) but preceded by a request to "
          "the managed element to perform an orderly shutdown. \n"
          "16=Power Cycle (Off - Hard Graceful), equivalent to "
          "Power Cycle (Off - Hard) but preceded by a request to "
          "the managed element to perform an orderly shutdown. \n"
          "..=DMTF Reserved. \n"
          "0x7FFF..0xFFFF = Vendor Specific." ), 
       ValueMap { "1", "2", "3", "4", "5", "6", "7", "8", "9", "10", 
          "11", "12", "13", "14", "15", "16", "..", "0x7FFF..0xFFFF" }, 
       Values { "Other", "On", "Sleep - Light", "Sleep -Deep", 
          "Power Cycle (Off - Soft)", "Off - Hard", 
          "Hibernate (Off - Soft)", "Off - Soft", 
          "Power Cycle (Off-Hard)", "Master Bus Reset", 
          "Diagnostic Interrupt (NMI)", "Off - Soft Graceful", 
          "Off - Hard Graceful", "Master Bus Reset Graceful", 
          "Power Cycle (Off - Soft Graceful)", 
          "Power Cycle (Off - Hard Graceful)", "DMTF Reserved", 
          "Vendor Specific" }, 
       MappingStrings { "IEEE P1621 | 3.2" }, 
       ModelCorrespondence { 
          "CIM_PowerManagementService.RequestPowerStateChange", 
          "CIM_AssociatedPowerManagementService.PowerState" }]
   uint16 PowerStatesSupported[];

      [Description ( 
          "An enumeration indicating the specific power-related "
          "capabilities of a managed element. Since this is an "
          "array, multiple values may be specified. The current "
          "values in the enumeration are: \n"
          "0 = Unknown \n"
          "1 = Other \n"
          "2 = Power Saving Modes Entered Automatically, describing "
          "that a managed element can change its power state based "
          "on usage or other criteria \n"
          "3 = Power State Settable, indicating that the "
          "RequestPowerStateChange method is supported \n"
          "4 = Power Cycling Supported, indicating that the "
          "RequestPowerStateChange method can be invoked with the "
          "PowerState input variable set to \'Power Cycle (Off "
          "Soft)\' \n"
          "5 = Timed Power On Supported, indicating that the "
          "RequestPowerStateChange method can be invoked with the "
          "PowerState input variable set to \'Power On\' and the "
          "Time parameter set to a specific date and time, or "
          "interval, for power-on.8 = Graceful Shutdown Supported, "
          "indicating that the managed element can be sent a "
          "hardware signal requesting an orderly shutdown prior to "
          "the requested power state change." ), 
       ValueMap { "0", "1", "2", "3", "4", "5", "6", "7", "8" }, 
       Values { "Unknown", "Other", 
          "Power Saving Modes Entered Automatically", 
          "Power State Settable", "Power Cycling Supported", 
          "Timed Power On Supported", 
          "Off Hard Power Cycling Supported", "HW Reset Supported", 
          "Graceful Shutdown Supported" }, 
       ModelCorrespondence { 
          "CIM_PowerManagementService.RequestPowerStateChange", 
          "CIM_PowerManagementCapabilities.OtherPowerChangeCapabilities" }]
   uint16 PowerChangeCapabilities[];

      [Description ( 
          "A string describing the additional power management "
          "capabilities of the element, used when the "
          "PowerChangeCapabilities is set to the value 1, \"Other\"." ), 
       ModelCorrespondence { 
          "CIM_PowerManagementCapabilities.PowerChangeCapabilities" }]
   string OtherPowerChangeCapabilities;


};
