;*****************************************
; Netwew00.INF
;
; Intel Wireless WiFi Link Adapters
; Installation Script for Windows8 64 bit
;
; Copyright (C) 1997-2011 Intel Corporation. All rights reserved.
;
; The information and source code contained herein is the exclusive
; property of Intel Corporation and may not be disclosed, examined
; or reproduced in whole or in part without explicit written authorization
; from the company.
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[version]
Signature   = "$Windows NT$"
Compatible  = 1
Class       = net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %PROVIDER_NAME%
DriverVer   = 02/25/2014,15.12.0.6 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY

CatalogFile = NETwew00.cat


;*****************************************
; Manufacturer
;-----------------------------------------

[Manufacturer]
%COMPANY_NAME% = Device, NTamd64.6.2

;[ControlFlags]
;ExcludeFromSelect = \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_40608086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_40648086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_406A8086 , \ 
;        PCI\VEN_8086&DEV_088F&SUBSYS_42608086 , \ 
;        PCI\VEN_8086&DEV_088F&SUBSYS_42648086 , \ 
;        PCI\VEN_8086&DEV_088F&SUBSYS_426A8086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_50608086 , \ 
;        PCI\VEN_8086&DEV_088F&SUBSYS_52608086 , \ 
;        PCI\VEN_8086&DEV_088F&SUBSYS_526A8086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_44608086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_44648086 , \ 
;        PCI\VEN_8086&DEV_088E&SUBSYS_446A8086 , \ 
;        PCI\VEN_8086&DEV_0887&SUBSYS_40628086 , \ 
;        PCI\VEN_8086&DEV_0887&SUBSYS_40668086 , \ 
;        PCI\VEN_8086&DEV_0888&SUBSYS_42628086 , \ 
;        PCI\VEN_8086&DEV_0888&SUBSYS_42668086 , \ 
;        PCI\VEN_8086&DEV_0887&SUBSYS_44628086 , \ 
;        PCI\VEN_8086&DEV_0887&SUBSYS_44668086 , \ 
;        PCI\VEN_8086&DEV_0890&SUBSYS_40228086 , \ 
;        PCI\VEN_8086&DEV_0890&SUBSYS_40268086 , \ 
;        PCI\VEN_8086&DEV_0891&SUBSYS_42228086 , \ 
;        PCI\VEN_8086&DEV_0891&SUBSYS_42268086 , \ 
;        PCI\VEN_8086&DEV_0890&SUBSYS_44228086 , \ 
;        PCI\VEN_8086&DEV_0890&SUBSYS_44268086 , \ 
;        PCI\VEN_8086&DEV_0892&SUBSYS_00628086 , \ 
;        PCI\VEN_8086&DEV_0892&SUBSYS_00668086 , \ 
;        PCI\VEN_8086&DEV_0893&SUBSYS_02628086 , \ 
;        PCI\VEN_8086&DEV_0893&SUBSYS_02668086 , \ 
;        PCI\VEN_8086&DEV_0892&SUBSYS_04628086 , \ 
;        PCI\VEN_8086&DEV_0892&SUBSYS_04668086 , \ 
;        PCI\VEN_8086&DEV_0894&SUBSYS_00228086 , \ 
;        PCI\VEN_8086&DEV_0894&SUBSYS_00268086 , \ 
;        PCI\VEN_8086&DEV_0895&SUBSYS_02228086 , \ 
;        PCI\VEN_8086&DEV_0895&SUBSYS_02268086 , \ 
;        PCI\VEN_8086&DEV_0894&SUBSYS_04228086 , \ 
;        PCI\VEN_8086&DEV_0894&SUBSYS_04268086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13018086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13068086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13078086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13088086 , \ 
;        PCI\VEN_8086&DEV_0085&SUBSYS_13118086 , \ 
;        PCI\VEN_8086&DEV_0085&SUBSYS_13168086 , \ 
;        PCI\VEN_8086&DEV_0085&SUBSYS_13188086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13218086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13268086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_13288086 , \ 
;        PCI\VEN_8086&DEV_0082&SUBSYS_C0208086 , \ 
;        PCI\VEN_8086&DEV_0085&SUBSYS_C2208086 , \ 
;        PCI\VEN_8086&DEV_0085&SUBSYS_C2288086 , \ 
;        PCI\VEN_8086&DEV_0885&SUBSYS_13078086 , \ 
;        PCI\VEN_8086&DEV_0885&SUBSYS_13058086 , \ 
;        PCI\VEN_8086&DEV_0087&SUBSYS_13018086 , \ 
;        PCI\VEN_8086&DEV_0087&SUBSYS_13068086 , \ 
;        PCI\VEN_8086&DEV_422B&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_422B&SUBSYS_11088086 , \ 
;        PCI\VEN_8086&DEV_0886&SUBSYS_13178086 , \ 
;        PCI\VEN_8086&DEV_0886&SUBSYS_13158086 , \ 
;        PCI\VEN_8086&DEV_0089&SUBSYS_13118086 , \ 
;        PCI\VEN_8086&DEV_0089&SUBSYS_13168086 , \ 
;        PCI\VEN_8086&DEV_4238&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4238&SUBSYS_11188086 , \ 
;        PCI\VEN_8086&DEV_0885&SUBSYS_13278086 , \ 
;        PCI\VEN_8086&DEV_0885&SUBSYS_13258086 , \ 
;        PCI\VEN_8086&DEV_0087&SUBSYS_13218086 , \ 
;        PCI\VEN_8086&DEV_0087&SUBSYS_13268086 , \ 
;        PCI\VEN_8086&DEV_422B&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_422B&SUBSYS_11288086 , \ 

;*****************************************
;Device
;-----------------------------------------

;*****************************************
;Device WIN8_64
;-----------------------------------------
[Device.NTamd64.6.2]

; GEN_6235_AGN_2x2_HMC
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_088E&SUBSYS_40608086 ; AGN
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_ABG15    ,   PCI\VEN_8086&DEV_088E&SUBSYS_40648086 ; ABG15
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN10    ,   PCI\VEN_8086&DEV_088E&SUBSYS_406A8086 ; AGN10

; Gui_6235_AGN_2x2_HMC
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_088F&SUBSYS_42608086 ; AGN
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_ABG15    ,   PCI\VEN_8086&DEV_088F&SUBSYS_42648086 ; ABG15
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN10    ,   PCI\VEN_8086&DEV_088F&SUBSYS_426A8086 ; AGN10

; GENNGFF_6235_AGN_2x2_HMC
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_GENNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_088E&SUBSYS_50608086 ; AGN

; LenovoNGFF_6235_AGN_2x2_HMC
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_088F&SUBSYS_52608086 ; AGN
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN10    ,   PCI\VEN_8086&DEV_088F&SUBSYS_526A8086 ; AGN10

; Dell_6235_AGN_2x2_HMC
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_088E&SUBSYS_44608086 ; AGN
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_ABG15    ,   PCI\VEN_8086&DEV_088E&SUBSYS_44648086 ; ABG15
%NIC_MPCIEX_6235AGN_2x2_HMC% = Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN10    ,   PCI\VEN_8086&DEV_088E&SUBSYS_446A8086 ; AGN10

; GEN_2230_BGN_2x2_HMC
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0887&SUBSYS_40628086 ; BGN15
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0887&SUBSYS_40668086 ; BG15

; Gui_2230_BGN_2x2_HMC
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0888&SUBSYS_42628086 ; BGN15
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0888&SUBSYS_42668086 ; BG15

; Dell_2230_BGN_2x2_HMC
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0887&SUBSYS_44628086 ; BGN15
%NIC_MPCIEX_2230BGN_2x2_HMC% = Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0887&SUBSYS_44668086 ; BG15

; GEN_2200_BGN_2x2_HMC
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0890&SUBSYS_40228086 ; BGN15
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0890&SUBSYS_40268086 ; BG15

; Gui_2200_BGN_2x2_HMC
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0891&SUBSYS_42228086 ; BGN15
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0891&SUBSYS_42268086 ; BG15

; Dell_2200_BGN_2x2_HMC
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0890&SUBSYS_44228086 ; BGN15
%NIC_MPCIEX_2200BGN_2x2_HMC% = Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0890&SUBSYS_44268086 ; BG15

; GEN_0135_BGN_1x1_HMC
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0892&SUBSYS_00628086 ; BGN15
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0892&SUBSYS_00668086 ; BG15

; Gui_0135_BGN_1x1_HMC
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0893&SUBSYS_02628086 ; BGN15
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0893&SUBSYS_02668086 ; BG15

; Dell_0135_BGN_1x1_HMC
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0892&SUBSYS_04628086 ; BGN15
%NIC_MPCIEX_0135BGN_1x1_HMC% = Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0892&SUBSYS_04668086 ; BG15

; GEN_0105_BGN_1x1_HMC
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0894&SUBSYS_00228086 ; BGN15
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0894&SUBSYS_00268086 ; BG15

; Gui_0105_BGN_1x1_HMC
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0895&SUBSYS_02228086 ; BGN15
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0895&SUBSYS_02268086 ; BG15

; Dell_0105_BGN_1x1_HMC
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BGN15    ,   PCI\VEN_8086&DEV_0894&SUBSYS_04228086 ; BGN15
%NIC_MPCIEX_0105BGN_1x1_HMC% = Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BG15    ,   PCI\VEN_8086&DEV_0894&SUBSYS_04268086 ; BG15

; GEN_6205_AGN_2x2_HMC
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13018086 ; MOW
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13068086 ; ABG
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_BG7    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13078086 ; BG7
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13088086 ; ABG10

; Gui_6205_AGN_2x2_HMC
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0085&SUBSYS_13118086 ; MOW
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG    ,   PCI\VEN_8086&DEV_0085&SUBSYS_13168086 ; ABG
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_0085&SUBSYS_13188086 ; ABG10

; Dell_6205_AGN_2x2_HMC
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13218086 ; MOW
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13268086 ; ABG
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_0082&SUBSYS_13288086 ; ABG10

; GEN_6205S_AGN_2x2_HMC
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_GEN_6205S_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_0082&SUBSYS_C0208086 ; AGN

; Lenovo_6205S_AGN_2x2_HMC
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_AGN    ,   PCI\VEN_8086&DEV_0085&SUBSYS_C2208086 ; AGN
%NIC_MPCIEX_6205AGN_2x2_HMC% = Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_0085&SUBSYS_C2288086 ; ABG10

; GEN_6150_BGN_1x2_HMC
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BG7    ,   PCI\VEN_8086&DEV_0885&SUBSYS_13078086 ; BG7
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BGN    ,   PCI\VEN_8086&DEV_0885&SUBSYS_13058086 ; BGN

; GEN_6250_AGN_2x2_HMC
%NIC_MPCIEX_6250AGN_2x2_HMC% = Install_MPCIEX_GEN_6250_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0087&SUBSYS_13018086 ; MOW

; GEN_6250_ABG_2x2_HMC
%NIC_MPCIEX_6250ABG_2x2_HMC% = Install_MPCIEX_GEN_6250_ABG_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0087&SUBSYS_13068086 ; MOW

; GEN_6300_AGN_3x3_HMC
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_422B&SUBSYS_11018086 ; MOW
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_422B&SUBSYS_11088086 ; ABG10

; Lenovo_6150_BGN_1x2_HMC
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BG7    ,   PCI\VEN_8086&DEV_0886&SUBSYS_13178086 ; BG7
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BGN    ,   PCI\VEN_8086&DEV_0886&SUBSYS_13158086 ; BGN

; Lenovo_6250_AGN_2x2_HMC
%NIC_MPCIEX_6250AGN_2x2_HMC% = Install_MPCIEX_Lenovo_6250_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0089&SUBSYS_13118086 ; MOW

; Lenovo_6250_ABG_2x2_HMC
%NIC_MPCIEX_6250ABG_2x2_HMC% = Install_MPCIEX_Lenovo_6250_ABG_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0089&SUBSYS_13168086 ; MOW

; Lenovo_6300_AGN_3x3_HMC
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_4238&SUBSYS_11118086 ; MOW
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_4238&SUBSYS_11188086 ; ABG10

; Dell_6150_BGN_1x2_HMC
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BG7    ,   PCI\VEN_8086&DEV_0885&SUBSYS_13278086 ; BG7
%NIC_MPCIEX_6150BGN_1x2_HMC% = Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BGN    ,   PCI\VEN_8086&DEV_0885&SUBSYS_13258086 ; BGN

; Dell_6250_AGN_2x2_HMC
%NIC_MPCIEX_6250AGN_2x2_HMC% = Install_MPCIEX_Dell_6250_AGN_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0087&SUBSYS_13218086 ; MOW

; Dell_6250_ABG_2x2_HMC
%NIC_MPCIEX_6250ABG_2x2_HMC% = Install_MPCIEX_Dell_6250_ABG_2x2_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_0087&SUBSYS_13268086 ; MOW

; Dell_6300_AGN_3x3_HMC
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_MOW    ,   PCI\VEN_8086&DEV_422B&SUBSYS_11218086 ; MOW
%NIC_MPCIEX_6300AGN_3x3_HMC% = Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_ABG10    ,   PCI\VEN_8086&DEV_422B&SUBSYS_11288086 ; ABG10



;*****************************************
;INSTALL WIN8_64
;-----------------------------------------

;-----------------------------------------
; Intel  WIN8_64 GEN_6235_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6235_AGN_2x2_HMC, Reg_GEN_6235_AGN_2x2_HMC_AGN, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_ABG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6235_AGN_2x2_HMC, Reg_GEN_6235_AGN_2x2_HMC_ABG15, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_ABG15.CoInstallers]

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_ABG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_ABG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6235_AGN_2x2_HMC, Reg_GEN_6235_AGN_2x2_HMC_AGN10, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN10.CoInstallers]

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6235_AGN_2x2_HMC_WIN8_64_AGN10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_6235_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6235_AGN_2x2_HMC, Reg_Gui_6235_AGN_2x2_HMC_AGN, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_ABG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6235_AGN_2x2_HMC, Reg_Gui_6235_AGN_2x2_HMC_ABG15, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_ABG15.CoInstallers]

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_ABG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_ABG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6235_AGN_2x2_HMC, Reg_Gui_6235_AGN_2x2_HMC_AGN10, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN10.CoInstallers]

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6235_AGN_2x2_HMC_WIN8_64_AGN10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GENNGFF_6235_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GENNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GENNGFF_6235_AGN_2x2_HMC, Reg_GENNGFF_6235_AGN_2x2_HMC_AGN, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GENNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_GENNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 LenovoNGFF_6235_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_LenovoNGFF_6235_AGN_2x2_HMC, Reg_LenovoNGFF_6235_AGN_2x2_HMC_AGN, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_LenovoNGFF_6235_AGN_2x2_HMC, Reg_LenovoNGFF_6235_AGN_2x2_HMC_AGN10, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN10.CoInstallers]

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_LenovoNGFF_6235_AGN_2x2_HMC_WIN8_64_AGN10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6235_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6235_AGN_2x2_HMC, Reg_Dell_6235_AGN_2x2_HMC_AGN, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_ABG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6235_AGN_2x2_HMC, Reg_Dell_6235_AGN_2x2_HMC_ABG15, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_ABG15.CoInstallers]

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_ABG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_ABG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6235_AGN_2x2_HMC, Reg_Dell_6235_AGN_2x2_HMC_AGN10, Reg_MPCIEX_6235AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP2, Reg_NDI, Reg_NDI_JP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN10.CoInstallers]

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6235_AGN_2x2_HMC_WIN8_64_AGN10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_2230_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_2230_BGN_2x2_HMC, Reg_GEN_2230_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_2230_BGN_2x2_HMC, Reg_GEN_2230_BGN_2x2_HMC_BG15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_2230_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_2230_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_2230_BGN_2x2_HMC, Reg_Gui_2230_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_2230_BGN_2x2_HMC, Reg_Gui_2230_BGN_2x2_HMC_BG15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_2230_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_2230_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_2230_BGN_2x2_HMC, Reg_Dell_2230_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_2230_BGN_2x2_HMC, Reg_Dell_2230_BGN_2x2_HMC_BG15, Reg_MPCIEX_2230BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_JP1, Reg_NDI, Reg_NDI_JP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_2230_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_2200_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_2200_BGN_2x2_HMC, Reg_GEN_2200_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_2200_BGN_2x2_HMC, Reg_GEN_2200_BGN_2x2_HMC_BG15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_2200_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_2200_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_2200_BGN_2x2_HMC, Reg_Gui_2200_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_2200_BGN_2x2_HMC, Reg_Gui_2200_BGN_2x2_HMC_BG15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_2200_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_2200_BGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_2200_BGN_2x2_HMC, Reg_Dell_2200_BGN_2x2_HMC_BGN15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_2200_BGN_2x2_HMC, Reg_Dell_2200_BGN_2x2_HMC_BG15, Reg_MPCIEX_2200BGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_MBP, Reg_NDI, Reg_NDI_MBP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_2200_BGN_2x2_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_0135_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_0135_BGN_1x1_HMC, Reg_GEN_0135_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_0135_BGN_1x1_HMC, Reg_GEN_0135_BGN_1x1_HMC_BG15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_0135_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_0135_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_0135_BGN_1x1_HMC, Reg_Gui_0135_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_0135_BGN_1x1_HMC, Reg_Gui_0135_BGN_1x1_HMC_BG15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_0135_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_0135_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_0135_BGN_1x1_HMC, Reg_Dell_0135_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_0135_BGN_1x1_HMC, Reg_Dell_0135_BGN_1x1_HMC_BG15, Reg_MPCIEX_0135BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP2, Reg_NDI, Reg_NDI_CYP2, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_0135_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_0105_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_0105_BGN_1x1_HMC, Reg_GEN_0105_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_0105_BGN_1x1_HMC, Reg_GEN_0105_BGN_1x1_HMC_BG15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_0105_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_0105_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_0105_BGN_1x1_HMC, Reg_Gui_0105_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_0105_BGN_1x1_HMC, Reg_Gui_0105_BGN_1x1_HMC_BG15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_0105_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_0105_BGN_1x1_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BGN15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_0105_BGN_1x1_HMC, Reg_Dell_0105_BGN_1x1_HMC_BGN15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BGN15.CoInstallers]

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BG15]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_0105_BGN_1x1_HMC, Reg_Dell_0105_BGN_1x1_HMC_BG15, Reg_MPCIEX_0105BGN_1x1_HMC, Reg_NDIS_WIN8_64, Reg_CYP1, Reg_NDI, Reg_NDI_CYP1, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BG15.CoInstallers]

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BG15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_0105_BGN_1x1_HMC_WIN8_64_BG15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6205_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6205_AGN_2x2_HMC, Reg_GEN_6205_AGN_2x2_HMC_MOW, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6205_AGN_2x2_HMC, Reg_GEN_6205_AGN_2x2_HMC_ABG, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG.CoInstallers]

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_BG7]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6205_AGN_2x2_HMC, Reg_GEN_6205_AGN_2x2_HMC_BG7, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_BG7.CoInstallers]

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_BG7.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_BG7.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6205_AGN_2x2_HMC, Reg_GEN_6205_AGN_2x2_HMC_ABG10, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6205_AGN_2x2_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Gui_6205_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6205_AGN_2x2_HMC, Reg_Gui_6205_AGN_2x2_HMC_MOW, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6205_AGN_2x2_HMC, Reg_Gui_6205_AGN_2x2_HMC_ABG, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG.CoInstallers]

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Gui_6205_AGN_2x2_HMC, Reg_Gui_6205_AGN_2x2_HMC_ABG10, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Gui_6205_AGN_2x2_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6205_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6205_AGN_2x2_HMC, Reg_Dell_6205_AGN_2x2_HMC_MOW, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6205_AGN_2x2_HMC, Reg_Dell_6205_AGN_2x2_HMC_ABG, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG.CoInstallers]

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6205_AGN_2x2_HMC, Reg_Dell_6205_AGN_2x2_HMC_ABG10, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6205_AGN_2x2_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6205S_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6205S_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6205S_AGN_2x2_HMC, Reg_GEN_6205S_AGN_2x2_HMC_AGN, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6205S_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_GEN_6205S_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6205S_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Lenovo_6205S_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_AGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6205S_AGN_2x2_HMC, Reg_Lenovo_6205S_AGN_2x2_HMC_AGN, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_AGN.CoInstallers]

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6205S_AGN_2x2_HMC, Reg_Lenovo_6205S_AGN_2x2_HMC_ABG10, Reg_MPCIEX_6205AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_TYL, Reg_NDI, Reg_NDI_TYL, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6205S_AGN_2x2_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6150_BGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BG7]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6150_BGN_1x2_HMC, Reg_GEN_6150_BGN_1x2_HMC_BG7, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BG7.CoInstallers]

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BG7.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BG7.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6150_BGN_1x2_HMC, Reg_GEN_6150_BGN_1x2_HMC_BGN, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BGN.CoInstallers]

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6150_BGN_1x2_HMC_WIN8_64_BGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6250_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6250_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6250_AGN_2x2_HMC, Reg_GEN_6250_AGN_2x2_HMC_MOW, Reg_MPCIEX_6250AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6250_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_GEN_6250_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6250_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6250_ABG_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6250_ABG_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6250_ABG_2x2_HMC, Reg_GEN_6250_ABG_2x2_HMC_MOW, Reg_MPCIEX_6250ABG_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6250_ABG_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_GEN_6250_ABG_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6250_ABG_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 GEN_6300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6300_AGN_3x3_HMC, Reg_GEN_6300_AGN_3x3_HMC_MOW, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_GEN_6300_AGN_3x3_HMC, Reg_GEN_6300_AGN_3x3_HMC_ABG10, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_6300_AGN_3x3_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Lenovo_6150_BGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BG7]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6150_BGN_1x2_HMC, Reg_Lenovo_6150_BGN_1x2_HMC_BG7, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BG7.CoInstallers]

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BG7.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BG7.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6150_BGN_1x2_HMC, Reg_Lenovo_6150_BGN_1x2_HMC_BGN, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BGN.CoInstallers]

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6150_BGN_1x2_HMC_WIN8_64_BGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Lenovo_6250_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_6250_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6250_AGN_2x2_HMC, Reg_Lenovo_6250_AGN_2x2_HMC_MOW, Reg_MPCIEX_6250AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6250_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Lenovo_6250_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6250_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Lenovo_6250_ABG_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_6250_ABG_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6250_ABG_2x2_HMC, Reg_Lenovo_6250_ABG_2x2_HMC_MOW, Reg_MPCIEX_6250ABG_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6250_ABG_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Lenovo_6250_ABG_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6250_ABG_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Lenovo_6300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6300_AGN_3x3_HMC, Reg_Lenovo_6300_AGN_3x3_HMC_MOW, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Lenovo_6300_AGN_3x3_HMC, Reg_Lenovo_6300_AGN_3x3_HMC_ABG10, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Lenovo_6300_AGN_3x3_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6150_BGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BG7]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6150_BGN_1x2_HMC, Reg_Dell_6150_BGN_1x2_HMC_BG7, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BG7.CoInstallers]

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BG7.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BG7.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BGN]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6150_BGN_1x2_HMC, Reg_Dell_6150_BGN_1x2_HMC_BGN, Reg_MPCIEX_6150BGN_1x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_BG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BGN.CoInstallers]

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6150_BGN_1x2_HMC_WIN8_64_BGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6250_AGN_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6250_AGN_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6250_AGN_2x2_HMC, Reg_Dell_6250_AGN_2x2_HMC_MOW, Reg_MPCIEX_6250AGN_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6250_AGN_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Dell_6250_AGN_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6250_AGN_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6250_ABG_2x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6250_ABG_2x2_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6250_ABG_2x2_HMC, Reg_Dell_6250_ABG_2x2_HMC_MOW, Reg_MPCIEX_6250ABG_2x2_HMC, Reg_NDIS_WIN8_64, Reg_KLP, Reg_NDI, Reg_NDI_KLP, Reg_NDI_AGN, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6250_ABG_2x2_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Dell_6250_ABG_2x2_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6250_ABG_2x2_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

;-----------------------------------------
; Intel  WIN8_64 Dell_6300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_MOW]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6300_AGN_3x3_HMC, Reg_Dell_6300_AGN_3x3_HMC_MOW, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_MOW.CoInstallers]

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_MOW.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_MOW.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_ABG10]
FeatureScore = 0xFE
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
DelReg    	= DelReg_Common
AddReg          = Reg_Common, Reg_Common_WIN8_64, Reg_Dell_6300_AGN_3x3_HMC, Reg_Dell_6300_AGN_3x3_HMC_ABG10, Reg_MPCIEX_6300AGN_3x3_HMC, Reg_NDIS_WIN8_64, Reg_PMA, Reg_NDI, Reg_NDI_PMA, Reg_NDI_ABG, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WIN8_64
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

;WUMarker[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_ABG10.CoInstallers]

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_ABG10.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_Dell_6300_AGN_3x3_HMC_WIN8_64_ABG10.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNe64, 2, NIC_Service_WIN8_64, Common_EventLog_WIN8_64

[DelReg_Common]
HKR, Ndi\

[Reg_Common]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,BTEnableFlags,0x10001,0x3
HKR,,CardType,0x00010001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,BTOnThreshold,0x10001,0x4
HKR,,APMMode,0x10001,0x0
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E

; following registry keys define the Advanced Property Page (NDI) values. they are common, and the defult values vary between the different reg sections.
[Reg_NDI_BG]
HKR, Ndi\Params\WirelessMode,			ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode, 			Type, 	    0, "enum",
HKR, Ndi\params\WirelessMode, 			Default,    0, "32" ;bg
HKR, Ndi\Params\WirelessMode, 			Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 	        "0",  	    0, "1. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 	        "16", 	    0, "2. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 	        "32", 	    0, "3. 802.11b/g"

[Reg_NDI_AGN]
HKR, Ndi\Params\WirelessMode,               	ParamDesc,	0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       	0, "enum",
HKR, Ndi\params\WirelessMode,      		Default,    	0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   	0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"17",       	0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 		"0",        	0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 		"16",       	0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 		"32",       	0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum, 		"18",       	0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 		"34",       	0, "6. 802.11a/b/g"

HKR, Ndi\params\RoamingPreferredBandType,     	ParamDesc,	0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	Type,      	0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	Default,   	0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	Optional,  	0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	"0",       	0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	"1",       	0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,  "2",     	0x00000000, "3. "%PREFER_52_BAND_STR%

[Reg_NDI_ABG]
HKR, Ndi\Params\WirelessMode,               	ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      	    	Default,   	0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   0, "0"  
HKR, Ndi\params\WirelessMode\enum, 	    	"17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 	    	"0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 	    	"16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 	    	"32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum, 	    	"18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 	    	"34",       0, "6. 802.11a/b/g"


HKR, Ndi\params\RoamingPreferredBandType,     	  ParamDesc, 	0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	  Type,      	0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	  Default,   	0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	  Optional,  	0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	  "0",       	0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	  "1",       	0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	  "2",     	0x00000000, "3. "%PREFER_52_BAND_STR%

[Reg_NDI]
HKR, Ndi\params\RecommendedChannel24,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL24_STR%
HKR, Ndi\params\RecommendedChannel24,      	Type,       0x00000002, "int"
HKR, Ndi\params\RecommendedChannel24,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel24,      	Min,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Step,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\IbssTxPower,      			    ParamDesc, 	0x00000000, %IBSS_TX_POWER_STR%
HKR, Ndi\params\IbssTxPower,      			    Type,      	0x00000002, "enum"
HKR, Ndi\params\IbssTxPower,      			    Default,   	0x00000002, "100"
HKR, Ndi\params\IbssTxPower,      			    Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssTxPower\enum, 			    "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "25",       0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "50",       0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "75",       0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "100",      0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RoamAggressiveness,     	  ParamDesc, 	0x00000000, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\params\RoamAggressiveness,     	  Type,      	0x00000002, "enum"
HKR, Ndi\params\RoamAggressiveness,     	  Default,   	0x00000002, "2"
HKR, Ndi\params\RoamAggressiveness,     	  Optional,  	0x00000002, "0"
HKR, Ndi\params\RoamAggressiveness\enum,	  "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "1",       	0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "2",     	0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "3", 	    	0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\RoamAggressiveness\enum,    	  "4",          0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\IbssQosEnabled,			  ParamDesc, 	0x00000000, %ADHOC_QOS_MODE_STR%
HKR, Ndi\params\IbssQosEnabled,			  Type,  			0x00000002, "enum"
HKR, Ndi\params\IbssQosEnabled,			  Default, 		0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled,			  Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled\enum,  "0",  			0x00000000, %WMM_DISABLED_STR%
HKR, Ndi\params\IbssQosEnabled\enum,  "1",  			0x00000000, %WMM_ENABLED_STR%

HKR, Ndi\params\CtsToItself,		  ParamDesc, 			0x00000000, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\params\CtsToItself,		  Type,  					0x00000002, "enum"
HKR, Ndi\params\CtsToItself,		  Default, 				0x00000002, "1"
HKR, Ndi\params\CtsToItself,		  Optional,  			0x00000002, "0"
HKR, Ndi\params\CtsToItself\enum, "0",  					0x00000000, %RTS_CTS_ENABLED_STR%
HKR, Ndi\params\CtsToItself\enum, "1",  					0x00000000, %CTS_TO_SELF_ENABLED_STR%

[Reg_NDI_PMA]
HKR,,CLSGUID,0,"{3B3B2612-1CC9-4116-AFCC-6FAB08F007FD}"

[Reg_NDI_KLP]
HKR,,CLSGUID,0,"{254CF178-922C-4250-870D-72D95D84AFCE}"

[Reg_NDI_TYL]
HKR,,CLSGUID,0,"{BC8E4978-A13C-41b0-A232-88E977540EB6}"

[Reg_NDI_JP2]
HKR,,CLSGUID,0,"{B5F5DA9F-A10B-46fa-8F7E-2A867922EEDD}"

[Reg_NDI_JP1]
HKR,,CLSGUID,0,"{B5F5DA9F-A10B-46fa-8F7E-2A867922EEDD}"

[Reg_NDI_CYP2]
HKR,,CLSGUID,0,"{EA88A61D-5965-47d0-B00C-53EE98E92763}"

[Reg_NDI_CYP1]
HKR,,CLSGUID,0,"{E7955D85-C452-4d61-8FD3-659B10FCB6F6}"

[Reg_NDI_MBP]
HKR,,CLSGUID,0,"{04E042A5-913E-48b7-A796-D1D4A740F6E7}"

[Reg_NDI_11N]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%


[Reg_NDIS_WIN8_64]
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5,wifipro"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet,wlan,vwifi"
HKR, Ndi,             Service,      0, "NETwNe64"

; =========================
; Registry settings by HW
; =========================

[Reg_PMA]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x0577
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR,,TxPower2040Mode,0x10001,0x0
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

[Reg_KLP]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x0576
HKR,,CalibrationActiveUcode,0x10001,0x202
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,CoexistenceSystemMode,0x10001,0x0
HKR,,CoexistenceEnabled,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR,,TxPower2040Mode,0x10001,0x0
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

[Reg_TYL]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,UsePumaMacAsTaylors,0x10001,0x1
HKR,,IsSip,0x10001,0x0
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x8577
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

[Reg_JP2]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,IsSip,0x10001,0x0
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x8577
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,BTAntennaCouplingThresh,0x10001,0x23
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,BTEnableFlags,0x10001,0x91
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

[Reg_JP1]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,IsSip,0x10001,0x0
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x8577
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,BTEnableFlags,0x10001,0x91
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

[Reg_CYP1]
HKR,,IsSip,0x10001,0x0
HKR,,CalibrationActive,0x10001,0x8177
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,tlcValidAntenna,0x10001,0x1
HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       	0, %CHANNELWIDTHAUTO%
;HKR,,BTEnableFlags,0x10001,0x11

[Reg_CYP2]
HKR,,IsSip,0x10001,0x0
HKR,,CalibrationActive,0x10001,0x8177
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,tlcValidAntenna,0x10001,0x1
HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       	0, %CHANNELWIDTHAUTO%
HKR,,BTEnableFlags,0x10001,0x91

[Reg_MBP]
HKR,,*MiracastSupported,0x10001,0x1
HKR,,UsePumaMacAsTaylors,0x10001,0x1
HKR,,IsSip,0x10001,0x0
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x8577
HKR,,CalibrationActiveUcode,0x10001,0x302
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,PanEnabled,0x10001,0x1
HKR,,PanStealthMode,0x10001,0x0
HKR,,TxPacketCopyLowerWatermark,0x10001,0x0
HKR,,TxPacketCopyUpperWatermark,0x10001,0x0
HKR,,RxStbc,0x10001,0x1
HKR,,NetDetectEnable,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1
HKR,,RemoteWakeEnable,0x10001,0x1
HKR,,ARPOffloadEnable,0x10001,0x1
HKR,,NSOffloadEnable,0x10001,0x1
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            	ParamDesc,              0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	type,                   0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            	default,                0, "1"

HKR, Ndi\Params\*PMARPOffload,                  	ParamDesc,              0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  	type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  	default,                0, "1"

HKR, Ndi\Params\*PMNSOffload,                   	ParamDesc,              0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   	type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   	default,                0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	ParamDesc,              0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  	"1",                    0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	type,                   0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       	default,                0, "0"

; =========================
; Registry settings by OS
; =========================

[Reg_Common_WIN8_64]
HKR,,TGeEnableBits,0x10001,0x27

; =========================
; Registry settings by SKU
; =========================
[Reg_GEN_6205_AGN_2x2_HMC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_6205_AGN_2x2_HMC_MOW]
HKR,,BandType,0x10003,0x2
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,		 	ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,		 	Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,		 	Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,		 	Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 	 	"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 	 	"1",       	0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,		 	ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,		 	Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,		 	Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,		 	Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 	 	"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 	 	"1",        	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedChannel24,  	 	Max,	  	0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,    	Default,    	0x00000002, "11"


[Reg_GEN_6205_AGN_2x2_HMC_ABG]
HKR,,BandType,0x10003,0x2
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6205_AGN_2x2_HMC_BG7]
HKR,,BandType,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6205_AGN_2x2_HMC_ABG10]
HKR,,BandType,0x10003,0x2
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_6205_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_6205_AGN_2x2_HMC_MOW]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%


[Reg_Gui_6205_AGN_2x2_HMC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_6205_AGN_2x2_HMC_ABG10]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_6205_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,PowerIndex,0x00000002,"3"
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_6205_AGN_2x2_HMC_MOW]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%


[Reg_Dell_6205_AGN_2x2_HMC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_6205_AGN_2x2_HMC_ABG10]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6205S_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,PowerIndex,0x00000002,"3"
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Lenovo_6205S_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,PowerIndex,0x00000002,"3"
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\FatChannelIntolerant, 	    		ParamDesc,	0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 			Type,	 	0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 			Default,	0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 			Optional, 	0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  		"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  		"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        	0, %ENABLED_STR%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        	0, %ENABLED_STR%


[Reg_GEN_6205S_AGN_2x2_HMC_AGN]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       	0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       	0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        	0, %ENABLED_STR%


[Reg_Lenovo_6205S_AGN_2x2_HMC_AGN]
HKR,,IEEE11nMode,0x00000004,"1"
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20

HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_6300_AGN_3x3_HMC_MOW]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_6300_AGN_3x3_HMC_ABG10]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Lenovo_6300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20

HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_6300_AGN_3x3_HMC_MOW]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Lenovo_6300_AGN_3x3_HMC_ABG10]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Dell_6300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR,,PowerIndex,0x00000002,"3"

HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_6300_AGN_3x3_HMC_MOW]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Dell_6300_AGN_3x3_HMC_ABG10]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,tlcInvalidAntsConfigsHB,0x10001,0x20
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_6150_BGN_1x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x301

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_6150_BGN_1x2_HMC_BG7]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6150_BGN_1x2_HMC_BGN]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_6250_AGN_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_6250_ABG_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",            0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",            0, %ENABLED_STR%

[Reg_Lenovo_6150_BGN_1x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x301

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%


[Reg_Lenovo_6150_BGN_1x2_HMC_BG7]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Lenovo_6150_BGN_1x2_HMC_BGN]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%


[Reg_Lenovo_6250_AGN_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_6250_ABG_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,PowerIndex,0x00000002,"6"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",            0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",            0, %ENABLED_STR%

[Reg_Dell_6150_BGN_1x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"101"
HKR,,PowerIndex,0x00000002,"3"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x301


HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_6150_BGN_1x2_HMC_BG7]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_6150_BGN_1x2_HMC_BGN]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_6250_AGN_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,PowerIndex,0x00000002,"3"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_6250_ABG_2x2_HMC]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,PowerIndex,0x00000002,"3"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "0"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",            0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",            0, %ENABLED_STR%

[Reg_MPCIEX_6150BGN_1x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6150BGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6150BGN_1x2%
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x301

[Reg_MPCIEX_6250AGN_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6250AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6250AGN_2x2%
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303

[Reg_MPCIEX_6250ABG_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6250ABG_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6250ABG_2x2%
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303

[Reg_MPCIEX_6300AGN_3x3_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6300AGN_3x3%
HKR,,DriverDesc,0,%NIC_DriverDesc_6300AGN_3x3%
HKR,,rlcChainSettings,0x10001,0xE

[Reg_MPCIEX_6205AGN_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

[Reg_MPCIEX_6235AGN_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6235AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6235AGN_2x2%

[Reg_MPCIEX_2230BGN_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_2230BGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_2230BGN_2x2%

[Reg_MPCIEX_2200BGN_2x2_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_2200BGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_2200BGN_2x2%

[Reg_MPCIEX_0135BGN_1x1_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_0135BGN_1x1%
HKR,,DriverDesc,0,%NIC_DriverDesc_0135BGN_1x1%

[Reg_MPCIEX_0105BGN_1x1_HMC]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_0105BGN_1x1%
HKR,,DriverDesc,0,%NIC_DriverDesc_0105BGN_1x1%


; =============================
; Registry settings for Binding
; =============================

[MSI_NDIS.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

; ===============================
; Registry settings for EventLogs
; ===============================

[Common_EventLog_WIN8_64]
AddReg = Reg_CommonAddEventLog_WIN8_64

[Reg_CommonAddEventLog_WIN8_64]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\NETwew00.sys"
HKR,, TypesSupported,   0x00010001, 7

[Reg_GEN_6250_AGN_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_6250_ABG_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_6250_AGN_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_6250_ABG_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Dell_6250_AGN_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_6250_ABG_2x2_HMC_MOW]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_GEN_6235_AGN_2x2_HMC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_6235_AGN_2x2_HMC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_6235_AGN_2x2_HMC]
HKR,,DesiredSsid,0x00000002,"101"
HKR,,PowerIndex,0x00000002,"3"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_2230_BGN_2x2_HMC]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_2230_BGN_2x2_HMC]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_2230_BGN_2x2_HMC]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"101"
HKR,,PowerIndex,0x00000002,"3"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_2200_BGN_2x2_HMC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_2200_BGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_2200_BGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"1"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,PowerIndex,0x00000002,"3"
HKR,,tlcValidAntenna,0x10001,0x3
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_0135_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x11
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_0135_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x11
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%


[Reg_Dell_0135_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x11
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_0105_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x3
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Gui_0105_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x3
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_0105_BGN_1x1_HMC]
HKR,,BTEnableFlags,0x10001,0x3
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"101"
HKR,,RecommendedChannel24,2,"11"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x301
HKR,,FixedSupportedHtRates,0x10001,0x000000FF

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_6235_AGN_2x2_HMC_AGN]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_GEN_6235_AGN_2x2_HMC_ABG15]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_GEN_6235_AGN_2x2_HMC_AGN10]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Gui_6235_AGN_2x2_HMC_AGN]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Gui_6235_AGN_2x2_HMC_ABG15]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Gui_6235_AGN_2x2_HMC_AGN10]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Dell_6235_AGN_2x2_HMC_AGN]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Dell_6235_AGN_2x2_HMC_ABG15]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_Dell_6235_AGN_2x2_HMC_AGN10]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_LenovoNGFF_6235_AGN_2x2_HMC_AGN10]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_LenovoNGFF_6235_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       	0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    		ParamDesc,	0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 			Type,	 	0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 			Default,	0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 			Optional, 	0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  		"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  		"1",	  	0, %ENABLED_STR%


[Reg_GENNGFF_6235_AGN_2x2_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,rlcChainSettings,0x10001,0x6
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       	0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       	0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    		ParamDesc,	0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 			Type,	 	0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 			Default,	0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 			Optional, 	0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  		"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  		"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_6205S_AGN_2x2_HMC_ABG10]
HKR,,IEEE11nMode,0x00000004,"1"
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_6205AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_6205AGN_2x2%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_LenovoNGFF_6235_AGN_2x2_HMC_AGN]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

[Reg_GENNGFF_6235_AGN_2x2_HMC_AGN]
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%


[Reg_GEN_2230_BGN_2x2_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_2230_BGN_2x2_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_2230_BGN_2x2_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_2230_BGN_2x2_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_2230_BGN_2x2_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_2230_BGN_2x2_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_2200_BGN_2x2_HMC_BGN15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_2200_BGN_2x2_HMC_BG15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_2200_BGN_2x2_HMC_BGN15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_2200_BGN_2x2_HMC_BG15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_2200_BGN_2x2_HMC_BGN15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_2200_BGN_2x2_HMC_BG15]
HKR,,BandType,0x10003,0x0

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_0135_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_0135_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_0135_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_0135_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_0135_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_0135_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_0105_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_GEN_0105_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_0105_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Gui_0105_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_0105_BGN_1x1_HMC_BGN15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_Dell_0105_BGN_1x1_HMC_BG15]
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

[Reg_NDI_BTHS]
HKR, Ndi\params\BT3HSMode,					ParamDesc, 	0, %BTHSMode%
HKR, Ndi\params\BT3HSMode,					Type,      	0, "enum"
HKR, Ndi\params\BT3HSMode,					Default,   	0, "1"
HKR, Ndi\params\BT3HSMode,					Optional,  	0, "0"
HKR, Ndi\params\BT3HSMode\enum,			"0",        0, %DISABLED_STR%
HKR, Ndi\params\BT3HSMode\enum,			"1",        0, %ENABLED_STR%
HKR, Ndi\Interfaces,								UpperRange,	0, "ndis5,wifipro,intel_amp"



[NIC_Service_WIN8_64]
DisplayName = "___" %NIC_Service_DispName_WIN8_64%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\NETwew00.sys
LoadOrderGroup  = NDIS

[Common_EventLog_WIN8_64]
AddReg = Reg_CommonAddEventLog_WIN8_64

;-----------------------------------------
; DestinationDirs
;-----------------------------------------

[CopyFiles_Driver_WIN8_64]
NETwew00.sys,,,2
Netwfw00.dat,,,2

[SourceDisksNames]
1=%SOURCEDISK1%,,

[SourceDisksFiles]
NETwew00.sys   = 1,,
Netwfw00.dat   = 1,,

[DestinationDirs]
DefaultDestDir = 11 ; Windows\System32
CopyFiles_Driver_WIN8_64=12;Windows\System32\Drivers

[Strings]
PROVIDER_NAME                        = "Intel"
COMPANY_NAME                         = "Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC = "Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC = "Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC = "Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC = "Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC = "Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         = "Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         = "Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         = "Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         = "Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         = "Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 = "Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 = "Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 = "Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 = "Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 = "Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  = "Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  = "Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  = "Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  = "Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  = "Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 = "Intel(R) Centrino(R) Advanced-N 6235 Driver"
NIC_DriverDesc_2230BGN_2x2 = "Intel(R) Centrino(R) Wireless-N 2230 Driver"
NIC_DriverDesc_2200BGN_2x2 = "Intel(R) Centrino(R) Wireless-N 2200 Driver"
NIC_DriverDesc_0135BGN_1x1 = "Intel(R) Centrino(R) Wireless-N 135 Driver"
NIC_DriverDesc_0105BGN_1x1 = "Intel(R) Centrino(R) Wireless-N 105 Driver"

NIC_DriverDesc_6205AGN_2x2              = "Intel(R) Centrino(R) Advanced-N 6205 Driver"

NIC_DriverDesc_6150BGN_1x2              = "Intel(R) Centrino(R) Wireless-N 6150 Driver"
NIC_Service_DispName_6150BGN_1x2    	= "Intel(R) Centrino(R) Wireless-N 6150 Adapter Driver for Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              = "Intel(R) Centrino(R) Advanced-N 6250 AGN Driver"
NIC_Service_DispName_6250AGN_2x2    	= "Intel(R) Centrino(R) Advanced-N 6250 AGN Adapter Driver for Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              = "Intel(R) Centrino(R) Advanced-N 6250 ABG Driver"
NIC_Service_DispName_6250ABG_2x2    	= "Intel(R) Centrino(R) Advanced-N 6250 ABG Adapter Driver for Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              = "Intel(R) Centrino(R) Ultimate-N 6300 AGN Driver"
NIC_Service_DispName_6300AGN_3x3    	= "Intel(R) Centrino(R) Ultimate-N 6300 AGN Adapter Driver for Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								= "Intel(R) Wireless WiFi Link 5000 Series Adapter Driver for Windows 8 - 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	= "Ad Hoc Channel 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	= "Ad Hoc Channel 802.11a"
RECOMMENDED_BAND            	= "Ad Hoc Default Wireless Mode"
IBSS_TX_POWER_STR           	= "Transmit Power"
ROAMING_AGGRESSIVENESS_STR  	= "Roaming Aggressiveness"
ADHOC_POWER_MANAGEMENT_STR  	= "Ad Hoc Power Management"
ADHOC_QOS_MODE_STR          	= "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR   	= "Mixed Mode Protection"
THROUGHPUT_ENHANCEMENT_STR  	= "Throughput Enhancement"
WIRELESS_MODE_STR           	= "Wireless Mode"
PREFERRED_BAND_STR          	= "Preferred Band"
CHANNELWIDTH52              	= "802.11n Channel Width for band 5.2"
CHANNELWIDTH24              	= "802.11n Channel Width for band 2.4"
TGnMode                     	= "802.11n Mode"
BTHSMode                    	= "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	= "Fat Channel Intolerant"

LOWEST_STR		    	= "Lowest"
MEDIUM_LOW_STR		    	= "Medium-low"
MEDIUM_STR		    	= "Medium"
MEDIUM_HIGH_STR		    	= "Medium-High"
HIGHEST_STR		    	= "Highest"
DISABLED_STR		    	= "Disabled"
ENABLED_STR 		    	= "Enabled"
MAXIMUM_POWER_SAVING_STR	= "Maximum Power Savings"
NOISY_ENVIRONMENT_STR		= "Noisy Environment"
WMM_STR                     	= "WMM"
CTS_TO_SELF_ENABLED_STR     	= "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR         	= "RTS/CTS Enabled"
AUTO_STR                    	= "Auto"
CHANNELWIDTH20ONLY          	= "20 MHz Only"
CHANNELWIDTHAUTO            	= "Auto"
WMM_DISABLED_STR            	= "WMM Disabled"
WMM_ENABLED_STR             	= "WMM Enabled"
NO_PREFERECE_STR            	= "No Preference"
PREFER_24_BAND_STR          	= "Prefer 2.4GHz band"
PREFER_52_BAND_STR          	= "Prefer 5.2GHz band"
WAKE_ON_MAGIC_PACKET        	= "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	= "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	= "GTK rekeying for WoWLAN"
PM_ARP_OFFLOAD			= "ARP offload for WoWLAN"
PM_NS_OFFLOAD			= "NS offload for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	= "Sleep on WoWLAN Disconnect"

SOURCEDISK1                  = "Intel(R) Wireless WiFi Link 5000 Series Install Disk"

[Strings.0419] ; Russian (Russia)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Wireless-N 6150 äëÿ Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6250 AGN äëÿ Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Advanced-N 6250 ABG äëÿ Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Äðàéâåð àäàïòåðà Intel(R) Centrino(R) Ultimate-N 6300 AGN äëÿ Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link ñåðèè 5000 äëÿ Windows 8 64 Bit "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Êàíàë Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Êàíàë Ad Hoc 802.11a"
RECOMMENDED_BAND            	="Ðåæèì ñåòè Ad Hoc ïî óìîë÷àíèþ"
IBSS_TX_POWER_STR           	="Ìîùíîñòü ïåðåäà÷è"
ROAMING_AGGRESSIVENESS_STR  	="Àãðåññèâíîñòü ðîóìèíãà"
ADHOC_POWER_MANAGEMENT_STR  	="Ìîùíîñòü ïåðåäà÷è Ad Hoc"
ADHOC_QOS_MODE_STR          	="Ðåæèì Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Çàùèòà â ñìåøàííîì ðåæèìå"
THROUGHPUT_ENHANCEMENT_STR  	="Ïîâûøåííàÿ ïðîïóñê. ñïîñîáíîñòü"
WIRELESS_MODE_STR           	="Ðåæèì áåñïðîâîäíîé ñåòè"
PREFERRED_BAND_STR          	="Ïðåäïî÷èòàåìàÿ ÷àñòîòà"
CHANNELWIDTH52              	="Øèðèíà êàíàëà 802.11n (5,2 ÃÃö)"
CHANNELWIDTH24              	="Øèðèíà êàíàëà 802.11n (2,4 ÃÃö)"
TGnMode                     	="Ðåæèì 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Íåñîâìåñòèìîñòü ñ êàíàëîì"

LOWEST_STR		    	="Ìèí."
MEDIUM_LOW_STR		    	="Ñðåäí.-ìèí."
MEDIUM_STR		    	="Ñðåäí."
MEDIUM_HIGH_STR		    	="Ñðåäí.-ìàêñ."
HIGHEST_STR		    	="Ìàêñ."
DISABLED_STR		    	="Âûêëþ÷åíî"
ENABLED_STR 		    	="Âêëþ÷åíî"
MAXIMUM_POWER_SAVING_STR	="Ìàêñ. ýêîíîìèÿ ýíåðãèè"
NOISY_ENVIRONMENT_STR		="Óñëîâèÿ ñ ïîìåõàìè"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self âêëþ÷åíî"
RTS_CTS_ENABLED_STR         	="RTS/CTS âêëþ÷åíî"
AUTO_STR                    	="Àâòî"
CHANNELWIDTH20ONLY          	="20 ÌÃö"
CHANNELWIDTHAUTO            	="Àâòî"
WMM_DISABLED_STR            	="WMM Âûêëþ÷åíî"
WMM_ENABLED_STR             	="WMM Âêëþ÷åíî"
NO_PREFERECE_STR            	="Íåò ïðåäïî÷òåíèé"
PREFER_24_BAND_STR          	="Ïðåäïî÷òåíèå ÷àñòîòó 2,4 ÃÃö"
PREFER_52_BAND_STR          	="Ïðåäïî÷òåíèå ÷àñòîòó 5,2 ÃÃö"
WAKE_ON_MAGIC_PACKET        	="Ïðîáóæäåíèå ïàêåòîì Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Ïðîáóæäåíèå ïðè ñîîòâåòñòâèè øàáëîíó"
PM_WIFI_REKEY_OFFLOAD	    	="Ïîâòîðíûé ââîä êëþ÷à GTK äëÿ ðåæèìà ïðîáóæäåíèÿ Wake on Wireless LAN"
PM_ARP_OFFLOAD			="Âûãðóçêà ARP äëÿ ðåæèìà ïðîáóæäåíèÿ Wake on Wireless LAN"
PM_NS_OFFLOAD			="Âûãðóçêà NS äëÿ ðåæèìà ïðîáóæäåíèÿ Wake on Wireless LAN"
DEVICE_SLEEP_ON_DISCONNECT	="Ïåðåõîä â ñîñòîÿíèå ñíà ïðè îòêëþ÷åíèè ðåæèìà ïðîáóæäåíèÿ Wake on Wireless LAN"

SOURCEDISK1                  ="Óñòàíîâî÷íûé äèñê àäàïòåðà Intel(R) Wireless WiFi Link ñåðèè 5000"

[Strings.0401] ; Arabic (Saudi Arabia)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Centrino(R) Wireless-N 6150 áäÙÇã Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Centrino(R) Advanced-N 6250 AGN áäÙÇã Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Centrino(R) Advanced-N 6250 ABG áäÙÇã Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="ÈÑäÇãÌ ÊÔÛíá Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Centrino(R) Ultimate-N 6300 AGN áäÙÇã Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="ÈÑäÇãÌ ÊÔÛíá ãÍæá ãÌãæÚÉ Intel(R) Wireless WiFi Link 5000 áäÙÇã Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="ÞäÇÉ ÇáÃÞÑÇä 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="ÞäÇÉ ÇáÃÞÑÇä 802.11a"
RECOMMENDED_BAND            	="æÖÚ ÇááÇÓáßí ÇáÇÝÊÑÇÖí ááÃÞÑÇä"
IBSS_TX_POWER_STR           	="ØÇÞÉ ÇáÅÑÓÇá"
ROAMING_AGGRESSIVENESS_STR  	="äÔÇØ ÇáÊÌæÇá"
ADHOC_POWER_MANAGEMENT_STR  	="ÅÏÇÑÉ ØÇÞÉ ÇáÃÞÑÇä"
ADHOC_QOS_MODE_STR          	="ÇáæÖÚ QoS ááÃÞÑÇä"
MIXED_MODE_PROTECTION_STR   	="ÍãÇíÉ ÇáæÖÚ ÇáãÎÊáØ"
THROUGHPUT_ENHANCEMENT_STR  	="ÊÍÓíä ÇáÎÑÌ"
WIRELESS_MODE_STR           	="æÖÚ ÇááÇÓáßí"
PREFERRED_BAND_STR          	="ãÏì ÇáãæÌÇÊ ÇáãÝÖá"
CHANNELWIDTH52              	="ÚÑÖ ÞäÇÉ 802.11n áãÏì ÇáãæÌÇÊ 5.2"
CHANNELWIDTH24              	="ÚÑÖ ÞäÇÉ 802.11n áãÏì ÇáãæÌÇÊ 2.4"
TGnMode                     	="æÖÚ 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="ÛíÑ ãÊæÇÝÞ ãÚ ÞäÇÉ 40 ãíÌÇåíÑÊÒ"

LOWEST_STR		    	="ÇáÃÏäì"
MEDIUM_LOW_STR		    	="ãÊæÓØ-ãäÎÝÖ"
MEDIUM_STR		    	="ãÊæÓØ"
MEDIUM_HIGH_STR		    	="ãÊæÓØ-ãÑÊÝÚ"
HIGHEST_STR		    	="ÇáÃÚáì"
DISABLED_STR		    	="ãÚØá"
ENABLED_STR 		    	="ããßøóä"
MAXIMUM_POWER_SAVING_STR	="ÃÞÕì ÊæÝíÑ ááØÇÞÉ"
NOISY_ENVIRONMENT_STR		="ÈíÆÉ ÇáÖæÖÇÁ"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="Êãßíä CTS ÇáÐÇÊí"
RTS_CTS_ENABLED_STR         	="Êãßíä RTS/CTS"
AUTO_STR                    	="ÊáÞÇÆí"
CHANNELWIDTH20ONLY          	="20 ãíÌÇåíÑÊÒ"
CHANNELWIDTHAUTO            	="ÊáÞÇÆí"
WMM_DISABLED_STR            	="WMM ãÚØá"
WMM_ENABLED_STR             	="WMM ããßøóä"
NO_PREFERECE_STR            	="ÈáÇ ÊÝÖíá"
PREFER_24_BAND_STR          	="íÝÖá ãÏì ãæÌÇÊ 2.4 ÌíÌÇåíÑÊÒ"
PREFER_52_BAND_STR          	="íÝÖá ãÏì ãæÌÇÊ 5.2 ÌíÌÇåíÑÊÒ"
WAKE_ON_MAGIC_PACKET        	="ÇáÊäÈíå ÚäÏ ÇáÍÒãÉ ÇáÓÍÑíÉ"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="ÅÚÇÏÉ ÅäÔÇÁ ãÝÊÇÍ GTK áÊäÈíå WLAN"
PM_ARP_OFFLOAD			="ÊæÒíÚ äÞá ÇáÈíÇäÇÊ ÈÇÓÊÎÏÇã ARP áÊäÈíå WLAN"
PM_NS_OFFLOAD			="ÊæÒíÚ äÞá ÇáÈíÇäÇÊ ÈÇÓÊÎÏÇã NS áÊäÈíå WLAN"
DEVICE_SLEEP_ON_DISCONNECT	="ÇáÓßæä ÚäÏ ÝÕá ÊäÈíå WLAN"

SOURCEDISK1                  ="ÞÑÕ ÊËÈíÊ ãÌãæÚÉ Intel(R) Wireless WiFi Link 5000"

[Strings.0804] ; Chinese (Simplified)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 Çý¶¯³ÌÐò"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 Çý¶¯³ÌÐò"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 Çý¶¯³ÌÐò"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 Çý¶¯³ÌÐò"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 Çý¶¯³ÌÐò"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 Çý¶¯³ÌÐò"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 Çý¶¯³ÌÐò"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows 8 64 Î»£©"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN Çý¶¯³ÌÐò"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows 8 64 Î»£©"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG Çý¶¯³ÌÐò"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows 8 64 Î»£©"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN Çý¶¯³ÌÐò"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows 8 64 Î»£©"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000 ÏµÁÐÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows 8 64 Î»£©"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad Hoc ÐÅµÀ 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad Hoc ÐÅµÀ 802.11a"
RECOMMENDED_BAND            	="Ad Hoc Ä¬ÈÏÎÞÏßÄ£Ê½"
IBSS_TX_POWER_STR           	="´«ÊäµçÔ´"
ROAMING_AGGRESSIVENESS_STR  	="ÂþÓÎÖ÷¶¯ÐÔ"
ADHOC_POWER_MANAGEMENT_STR  	="Ad Hoc µçÔ´¹ÜÀí"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS Ä£Ê½"
MIXED_MODE_PROTECTION_STR   	="»ìºÏÄ£Ê½±£»¤"
THROUGHPUT_ENHANCEMENT_STR  	="ÍÌÍÂÁ¿ÔöÇ¿"
WIRELESS_MODE_STR           	="ÎÞÏßÄ£Ê½"
PREFERRED_BAND_STR          	="Ê×Ñ¡Æµ´ø"
CHANNELWIDTH52              	="5.2 Æµ´øµÄ 802.11n ÐÅµÀ¿í¶È"
CHANNELWIDTH24              	="2.4 Æµ´øµÄ 802.11n ÐÅµÀ¿í¶È"
TGnMode                     	="802.11n Ä£Ê½"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Óë 40Mhz ÐÅµÀ²»¼æÈÝ"

LOWEST_STR		    	="×îµÍÖµ"
MEDIUM_LOW_STR		    	="ÖÐµÍ"
MEDIUM_STR		    	="ÖÐ¼ä"
MEDIUM_HIGH_STR		    	="ÖÐ¸ß"
HIGHEST_STR		    	="×î¸ßÖµ"
DISABLED_STR		    	="ÒÑ½ûÓÃ"
ENABLED_STR 		    	="ÒÑÆôÓÃ"
MAXIMUM_POWER_SAVING_STR	="×î´ó½ÚÄÜ"
NOISY_ENVIRONMENT_STR		="àÐÔÓ»·¾³"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self ÒÑÆôÓÃ"
RTS_CTS_ENABLED_STR         	="RTS/CTS ÒÑÆôÓÃ"
AUTO_STR                    	="×Ô¶¯"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="×Ô¶¯"
WMM_DISABLED_STR            	="WMM ÒÑ½ûÓÃ"
WMM_ENABLED_STR             	="WMM ÒÑÆôÓÃ"
NO_PREFERECE_STR            	="ÎÞÊ×Ñ¡Ïî"
PREFER_24_BAND_STR          	="Ê×Ñ¡ 2.4 GHz Æµ´ø"
PREFER_52_BAND_STR          	="Ê×Ñ¡ 5.2 GHz Æµ´ø"
WAKE_ON_MAGIC_PACKET        	="»½ÐÑ»ÃÊý¾Ý°ü"
WAKE_ON_PATTERN_MATCH       	="»½ÐÑÄ£Ê½Æ¥Åä"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN µÄ GTK ÖØÐÂÉú³ÉÃÜÔ¿"
PM_ARP_OFFLOAD			="WoWLAN µÄ ARP Ð¶ÔØ"
PM_NS_OFFLOAD			="WoWLAN µÄ NS Ð¶ÔØ"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN ¶Ï¿ªÁ¬½ÓÊ±Ë¯Ãß"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 ÏµÁÐ°²×°ÅÌ"

[Strings.0404] ; Chinese (Traditional)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 ÅX°Êµ{¦¡"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 ÅX°Êµ{¦¡"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 ÅX°Êµ{¦¡"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 ÅX°Êµ{¦¡"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 ÅX°Êµ{¦¡"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 ÅX°Êµ{¦¡"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 ÅX°Êµ{¦¡"
NIC_Service_DispName_6150BGN_1x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Wireless-N 6150 ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN ÅX°Êµ{¦¡"
NIC_Service_DispName_6250AGN_2x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Ultimate-N 6250 AGN ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG ÅX°Êµ{¦¡"
NIC_Service_DispName_6250ABG_2x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Advanced-N 6250 ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AG ÅX°Êµ{¦¡"
NIC_Service_DispName_6300AGN_3x3    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Ultimate-N 6300 AGN ¤¶­±¥dÅX°Êµ{¦¡"

NIC_Service_DispName_WIN8_64								="¥Î©ó Windows 8 64 Bit ªº Intel(R) Wireless WiFi Link 5000 ¨t¦C¤¶­±¥dÅX°Êµ{¦¡"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11a"
RECOMMENDED_BAND            	="ÂI¹ïÂI (ad hoc) ¹w³]µL½u¼Ò¦¡"
IBSS_TX_POWER_STR           	="¶Ç¿é¹q·½"
ROAMING_AGGRESSIVENESS_STR  	="º©¹C¿n·¥«×"
ADHOC_POWER_MANAGEMENT_STR  	="ÂI¹ïÂI (ad hoc) ¹q·½ºÞ²z"
ADHOC_QOS_MODE_STR          	="ÂI¹ïÂI (ad hoc) QoS ¼Ò¦¡"
MIXED_MODE_PROTECTION_STR   	="²V¦X¼Ò¦¡«OÅ@"
THROUGHPUT_ENHANCEMENT_STR  	="¿é°e¶q¼W±j¥\¯à"
WIRELESS_MODE_STR           	="µL½u¼Ò¦¡"
PREFERRED_BAND_STR          	="°¾¦nªºÀW±a"
CHANNELWIDTH52              	="802.11n ³q¹D¼e«× (5.2 GHz)"
CHANNELWIDTH24              	="802.11n ³q¹D¼e«× (2.4 GHz)"
TGnMode                     	="802.11n ¼Ò¦¡"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="¤£®e¤j¶q³q¹D"

LOWEST_STR		    	="³Ì§C"
MEDIUM_LOW_STR		    	="¤¤§C"
MEDIUM_STR		    	="¤¤"
MEDIUM_HIGH_STR		    	="¤¤°ª"
HIGHEST_STR		    	="³Ì°ª"
DISABLED_STR		    	="°±¥Î"
ENABLED_STR 		    	="±Ò¥Î"
MAXIMUM_POWER_SAVING_STR	="³Ì¬Ù¹q"
NOISY_ENVIRONMENT_STR		="¾¸­µÀô¹Ò"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="±Ò¥Î CTS-to-self"
RTS_CTS_ENABLED_STR         	="±Ò¥Î RTS/CTS"
AUTO_STR                    	="¦Û°Ê"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="¦Û°Ê"
WMM_DISABLED_STR            	="WMM °±¥Î"
WMM_ENABLED_STR             	="WMM ±Ò¥Î"
NO_PREFERECE_STR            	="µL°¾¦n³]©w"
PREFER_24_BAND_STR          	="³ß¦n 2.4 GHz ÀW±a"
PREFER_52_BAND_STR          	="³ß¦n 5.2 GHz ÀW±a"
WAKE_ON_MAGIC_PACKET        	="¦¬¨ì Magic «Ê¥]®É³ê¿ô"
WAKE_ON_PATTERN_MATCH       	="¦¬¨ì¼Ò¦¡¹ïÀ³®É³ê¿ô"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK ª÷Æ_­««Ø"
PM_ARP_OFFLOAD			="WoWLAN ARP ¨ø¸ü"
PM_NS_OFFLOAD			="WoWLAN NS ¨ø¸ü"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN ¤¤Â_³s½u®ÉºÎ¯v"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 ¨t¦C¦w¸ËºÏºÐ"

[Strings.0C04] ; Chinese (Hong Kong)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 ÅX°Êµ{¦¡"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 ÅX°Êµ{¦¡"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 ÅX°Êµ{¦¡"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 ÅX°Êµ{¦¡"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 ÅX°Êµ{¦¡"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 ÅX°Êµ{¦¡"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 ÅX°Êµ{¦¡"
NIC_Service_DispName_6150BGN_1x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Wireless-N 6150 ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN ÅX°Êµ{¦¡"
NIC_Service_DispName_6250AGN_2x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Ultimate-N 6250 AGN ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG ÅX°Êµ{¦¡"
NIC_Service_DispName_6250ABG_2x2    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Advanced-N 6250 ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AG ÅX°Êµ{¦¡"
NIC_Service_DispName_6300AGN_3x3    	="¥Î©ó Windows 8 64 Bit ªº Intel(R) Centrino(R) Ultimate-N 6300 AGN ¤¶­±¥dÅX°Êµ{¦¡"

NIC_Service_DispName_WIN8_64								="¥Î©ó Windows 8 64 Bit ªº Intel(R) Wireless WiFi Link 5000 ¨t¦C¤¶­±¥dÅX°Êµ{¦¡"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11a"
RECOMMENDED_BAND            	="ÂI¹ïÂI (ad hoc) ¹w³]µL½u¼Ò¦¡"
IBSS_TX_POWER_STR           	="¶Ç¿é¹q·½"
ROAMING_AGGRESSIVENESS_STR  	="º©¹C¿n·¥«×"
ADHOC_POWER_MANAGEMENT_STR  	="ÂI¹ïÂI (ad hoc) ¹q·½ºÞ²z"
ADHOC_QOS_MODE_STR          	="ÂI¹ïÂI (ad hoc) QoS ¼Ò¦¡"
MIXED_MODE_PROTECTION_STR   	="²V¦X¼Ò¦¡«OÅ@"
THROUGHPUT_ENHANCEMENT_STR  	="¿é°e¶q¼W±j¥\¯à"
WIRELESS_MODE_STR           	="µL½u¼Ò¦¡"
PREFERRED_BAND_STR          	="°¾¦nªºÀW±a"
CHANNELWIDTH52              	="802.11n ³q¹D¼e«× (5.2 GHz)"
CHANNELWIDTH24              	="802.11n ³q¹D¼e«× (2.4 GHz)"
TGnMode                     	="802.11n ¼Ò¦¡"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="¤£®e¤j¶q³q¹D"

LOWEST_STR		    	="³Ì§C"
MEDIUM_LOW_STR		    	="¤¤§C"
MEDIUM_STR		    	="¤¤"
MEDIUM_HIGH_STR		    	="¤¤°ª"
HIGHEST_STR		    	="³Ì°ª"
DISABLED_STR		    	="°±¥Î"
ENABLED_STR 		    	="±Ò¥Î"
MAXIMUM_POWER_SAVING_STR	="³Ì¬Ù¹q"
NOISY_ENVIRONMENT_STR		="¾¸­µÀô¹Ò"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="±Ò¥Î CTS-to-self"
RTS_CTS_ENABLED_STR         	="±Ò¥Î RTS/CTS"
AUTO_STR                    	="¦Û°Ê"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="¦Û°Ê"
WMM_DISABLED_STR            	="WMM °±¥Î"
WMM_ENABLED_STR             	="WMM ±Ò¥Î"
NO_PREFERECE_STR            	="µL°¾¦n³]©w"
PREFER_24_BAND_STR          	="³ß¦n 2.4 GHz ÀW±a"
PREFER_52_BAND_STR          	="³ß¦n 5.2 GHz ÀW±a"
WAKE_ON_MAGIC_PACKET        	="¦¬¨ì Magic «Ê¥]®É³ê¿ô"
WAKE_ON_PATTERN_MATCH       	="¦¬¨ì¼Ò¦¡¹ïÀ³®É³ê¿ô"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK ª÷Æ_­««Ø"
PM_ARP_OFFLOAD			="WoWLAN ARP ¨ø¸ü"
PM_NS_OFFLOAD			="WoWLAN NS ¨ø¸ü"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN ¤¤Â_³s½u®ÉºÎ¯v"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 ¨t¦C¦w¸ËºÏºÐ"

[Strings.0405] ; Czech (Czech Republic)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Ovladaè adaptéru Intel(R) Centrino(R) Wireless-N 6150 pro systém Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6250 AGN pro systém Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Ovladaè adaptéru Intel(R) Centrino(R) Advanced-N 6250 ABG pro systém Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Ovladaè adaptéru Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Ovladaè adaptéru Intel(R) Centrino(R) Ultimate-N 6300 AGN pro systém Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Ovladaè adaptéru øady Intel(R) Wireless WiFi Link 5000 pro systém Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Kanál ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Kanál ad hoc 802.11a"
RECOMMENDED_BAND            	="Výchozí bezdrátový režim ad hoc"
IBSS_TX_POWER_STR           	="Vysílací energie"
ROAMING_AGGRESSIVENESS_STR  	="Agresivita roamingu"
ADHOC_POWER_MANAGEMENT_STR  	="Správa napájení ad hoc"
ADHOC_QOS_MODE_STR          	="Režim Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Ochrana smíšeného režimu"
THROUGHPUT_ENHANCEMENT_STR  	="Zlepšení propustnosti"
WIRELESS_MODE_STR           	="Bezdrátový režim"
PREFERRED_BAND_STR          	="Upøednostòované pásmo"
CHANNELWIDTH52              	="Šíøka kanálu 802.11n pro pásmo 5,2"
CHANNELWIDTH24              	="Šíøka kanálu 802.11n pro pásmo 2,4"
TGnMode                     	="Režim 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Nekompatibilní s šíøkou kanálu 40 MHz"

LOWEST_STR		    	="Nejnižší"
MEDIUM_LOW_STR		    	="Støednì nízký"
MEDIUM_STR		    	="Støední"
MEDIUM_HIGH_STR		    	="Støednì vysoký"
HIGHEST_STR		    	="Nejvyšší"
DISABLED_STR		    	="Zakázáno"
ENABLED_STR 		    	="Povoleno"
MAXIMUM_POWER_SAVING_STR	="Maximální úspora energie"
NOISY_ENVIRONMENT_STR		="Prostøedí s velkým šumem"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self povoleno"
RTS_CTS_ENABLED_STR         	="RTS/CTS povoleno"
AUTO_STR                    	="Automaticky"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaticky"
WMM_DISABLED_STR            	="WMM zakázáno"
WMM_ENABLED_STR             	="WMM povoleno"
NO_PREFERECE_STR            	="Žádná pøedvolba"
PREFER_24_BAND_STR          	="Upøednostòovat pásmo 2,4 GHz"
PREFER_52_BAND_STR          	="Upøednostòovat pásmo 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Probuzení paketem Magic"
WAKE_ON_PATTERN_MATCH       	="Probuzení porovnávacím vzorkem"
PM_WIFI_REKEY_OFFLOAD	    	="Vystavování nových klíèù GTK pro technologii WoWLAN"
PM_ARP_OFFLOAD			="Snižování zatížení ARP pro technologii WoWLAN"
PM_NS_OFFLOAD			="Snižování zatížení NS pro technologii WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Režim spánku pøi odpojení technologie WoWLAN"

SOURCEDISK1                  ="Instalaèní disk adaptéru øady Intel(R) Wireless WiFi Link 5000"

[Strings.0406] ; Danish (Denmark)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 driver"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 driver"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 driver"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 driver"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 driver"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 driver"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 driver"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N  6150 adapter driver til Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN driver"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN adapter driver til Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG driver"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG adapter driver til Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN driver"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN adapter driver til Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000-serien adapter driver til Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad hoc-kanal 802.11a"
RECOMMENDED_BAND            	="Ad hoc standard trådløs tilstand"
IBSS_TX_POWER_STR           	="Sendeeffekt"
ROAMING_AGGRESSIVENESS_STR  	="Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR  	="Ad Hoc-strømstyring"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS-tilstand"
MIXED_MODE_PROTECTION_STR   	="Beskyttelse til blandet miljø"
THROUGHPUT_ENHANCEMENT_STR  	="Forbedring af ydelse"
WIRELESS_MODE_STR           	="Trådløs tilstand"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="802.11n kanalbredde for bånd 5,2"
CHANNELWIDTH24              	="802.11n kanalbredde for bånd 2,4"
TGnMode                     	="802.11n tilstand"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="40Mhz kanal intolerant"

LOWEST_STR		    	="Laveste"
MEDIUM_LOW_STR		    	="Mellem-lav"
MEDIUM_STR		    	="Mellem"
MEDIUM_HIGH_STR		    	="Mellem-høj"
HIGHEST_STR		    	="Højeste"
DISABLED_STR		    	="Deaktiveret"
ENABLED_STR 		    	="Aktiveret"
MAXIMUM_POWER_SAVING_STR	="Maks. strømbesparelse"
NOISY_ENVIRONMENT_STR		="Støjfyldt miljø"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self aktiveret "
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiveret "
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM deaktiveret"
WMM_ENABLED_STR             	="WMM aktiveret"
NO_PREFERECE_STR            	="Ingen indstilling"
PREFER_24_BAND_STR          	="Foretræk 2,4 GHz bånd"
PREFER_52_BAND_STR          	="Foretræk 5,2 GHz bånd"
WAKE_ON_MAGIC_PACKET        	="Vækning ved magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Vækning ved mønstermatch"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nøglefornyelse til WoWLAN"
PM_ARP_OFFLOAD			="ARP-aflastning til WoWLAN"
PM_NS_OFFLOAD			="NS-aflastning til WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slumring ved afbrydelse af WoWLAN"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000-serien installationsdisk"

[Strings.0407] ; German (Germany)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 Treiber"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 Treiber"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 Treiber"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 Treiber"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 Treiber"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 Treiber"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 Treiber"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 Adaptertreiber für Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN Treiber"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN Adaptertreiber für Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG Treiber"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG Adaptertreiber für Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN Treiber"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN Adaptertreiber für Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link der Serie 5000 Adaptertreiber für Windows 8 64-Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad-Hoc-Kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad-Hoc-Kanal 802.11a"
RECOMMENDED_BAND            	="Ad-hoc Standard-WLAN-Modus"
IBSS_TX_POWER_STR           	="Übertragungsleistung"
ROAMING_AGGRESSIVENESS_STR  	="Roaming-Dynamik"
ADHOC_POWER_MANAGEMENT_STR  	="Ad-Hoc-Energieverwaltung"
ADHOC_QOS_MODE_STR          	="Ad-Hoc QoS-Modus"
MIXED_MODE_PROTECTION_STR   	="Schutz f. gemischte Umgebungen"
THROUGHPUT_ENHANCEMENT_STR  	="Durchsatzverbesserung"
WIRELESS_MODE_STR           	="Drahtloser Modus"
PREFERRED_BAND_STR          	="Bevorzugtes Band"
CHANNELWIDTH52              	="802.11n Kanalbreite für Band 5.2"
CHANNELWIDTH24              	="802.11n Kanalbreite für Band 2.4"
TGnMode                     	="802.11n Modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Fat Kanal Intolerant"

LOWEST_STR		    	="Am niedrigsten"
MEDIUM_LOW_STR		    	="Mittel-niedrig"
MEDIUM_STR		    	="Mittel"
MEDIUM_HIGH_STR		    	="Mittel-hoch"
HIGHEST_STR		    	="Am höchsten"
DISABLED_STR		    	="Deaktiviert"
ENABLED_STR 		    	="Aktiviert"
MAXIMUM_POWER_SAVING_STR	="Maximale Energieersparnis"
NOISY_ENVIRONMENT_STR		="Laute Umgebung"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="'CTS-to-self' aktiviert"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiviert"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM deaktiviert"
WMM_ENABLED_STR             	="WMM aktiviert"
NO_PREFERECE_STR            	="Keine Einstellung"
PREFER_24_BAND_STR          	="2,4-GHz-Band bevorzugen"
PREFER_52_BAND_STR          	="5,2-GHz-Band bevorzugen"
WAKE_ON_MAGIC_PACKET        	="Aktivierung durch Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivierung durch Musterübereinstimmung"
PM_WIFI_REKEY_OFFLOAD	    	="GTK führt Neuverschlüsselung für WoWLAN durch"
PM_ARP_OFFLOAD			="ARP-Offload für WoWLAN"
PM_NS_OFFLOAD			="NS-Offload für WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Medientrennung beim Aufrechterhalten des Energiesparmodus von WoWLAN"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link der Serie 5000 - Installationsdiskette"

[Strings.0408] ; Greek (Greece)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Centrino(R) Wireless-N 6150 ãéá Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Centrino(R) Advanced-N 6250 AGN ãéá Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Centrino(R) Advanced-N 6250 ABG ãéá Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Ðñüãñáììá ïäÞãçóçò Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Centrino(R) Ultimate-N 6300 AGN ãéá Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 5000 Series ãéá Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="ÊáíÜëé ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="ÊáíÜëé ad hoc 802.11a"
RECOMMENDED_BAND            	="ÐñïåðéëåãìÝíç áóýñìáôç ëåéôïõñãßá ad hoc"
IBSS_TX_POWER_STR           	="Éó÷ýò ìåôÜäïóçò"
ROAMING_AGGRESSIVENESS_STR  	="Äõíáìéêüôçôá ðåñéáãùãÞò"
ADHOC_POWER_MANAGEMENT_STR  	="Äéá÷åßñéóç éó÷ýïò ad hoc"
ADHOC_QOS_MODE_STR          	="Ôñüðïò ëåéôïõñãßáò Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Ðñïóôáóßá ìåéêôÞò ëåéôïõñãßáò"
THROUGHPUT_ENHANCEMENT_STR  	="Âåëôßùóç éêáíüôçôáò ìåôÜäïóçò"
WIRELESS_MODE_STR           	="Áóýñìáôç êáôÜóôáóç"
PREFERRED_BAND_STR          	="Ðñïôéìþìåíç æþíç"
CHANNELWIDTH52              	="Åýñïò êáíáëéïý 802.11n ãéá æþíç 5.2"
CHANNELWIDTH24              	="Åýñïò êáíáëéïý 802.11n ãéá æþíç 2.4"
TGnMode                     	="Ëåéôïõñãßá 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Ìç óõìâáôü ìå éó÷õñÜ êáíÜëéá"

LOWEST_STR		    	="×áìçëüôåñç"
MEDIUM_LOW_STR		    	="Ìåóáßá-×áìçëÞ"
MEDIUM_STR		    	="Ìåóáßá"
MEDIUM_HIGH_STR		    	="Ìåóáßá-ÕøçëÞ"
HIGHEST_STR		    	="Õøçëüôåñç"
DISABLED_STR		    	="ÁðåíåñãïðïéçìÝíç"
ENABLED_STR 		    	="ÅíåñãïðïéçìÝíç"
MAXIMUM_POWER_SAVING_STR	="ÌÝãéóôç åîïéêïíüìçóç éó÷ýïò"
NOISY_ENVIRONMENT_STR		="Èïñõâþäåò ðåñéâÜëëïí"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="ÅíåñãïðïéçìÝíï CTS-to-self"
RTS_CTS_ENABLED_STR         	="ÅíåñãïðïéçìÝíï RTS/CTS"
AUTO_STR                    	="Áõôüìáôá"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Áõôüìáôá"
WMM_DISABLED_STR            	="ÁðåíåñãïðïéçìÝíç WMM"
WMM_ENABLED_STR             	="ÅíåñãïðïéçìÝíç WMM"
NO_PREFERECE_STR            	="Êáìßá ðñïôßìçóç"
PREFER_24_BAND_STR          	="Ðñïôßìçóç æþíç 2,4 GHz"
PREFER_52_BAND_STR          	="Ðñïôßìçóç æþíç 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Åíåñãïðïßçóç ìå Ìáãéêü ðáêÝôï"
WAKE_ON_PATTERN_MATCH       	="Åíåñãïðïßçóç ìå áíôéóôïß÷éóç ìïôßâïõ"
PM_WIFI_REKEY_OFFLOAD	    	="Ôï GTK æçôÜ ôç äçìéïõñãßá íÝïõ êëåéäéïý ãéá WoWLAN"
PM_ARP_OFFLOAD			="Ìåßùóç öüñôïõ ARP ãéá WoWLAN"
PM_NS_OFFLOAD			="Ìåßùóç öüñôïõ NS ãéá WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="ÁíáóôïëÞ ëåéôïõñãßáò êáôÜ ôçí áðïóýíäåóç ôïõ WoWLAN"

SOURCEDISK1                  ="ÄéóêÝôá åãêáôÜóôáóçò Intel(R) Wireless WiFi Link 5000 Series"

[Strings.0C0A] ; Spanish (Spain)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Controlador Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Controlador Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Controlador Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Controlador Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Controlador Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Controlador Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Controlador del adaptador Intel(R) Centrino(R) Wireless-N 6150 para Windows 8 de 64 bits"
NIC_DriverDesc_6250AGN_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Controlador del adaptador Intel(R) Centrino(R) Advanced-N 6250 AGN para Windows 8 de 64 bits"
NIC_DriverDesc_6250ABG_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Controlador del adaptador Intel(R) Centrino(R) Advanced-N 6250 ABG para Windows 8 de 64 bits"
NIC_DriverDesc_6300AGN_3x3              ="Controlador Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Controlador del adaptador Intel(R) Centrino(R) Ultimate-N 6300 AGN para Windows 8 de 64 bits"

NIC_Service_DispName_WIN8_64								="Controlador del adaptador Intel(R) Wireless WiFi Link para Windows 8 de 64 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Canal Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Canal Ad Hoc 802.11a"
RECOMMENDED_BAND            	="Modo inalámbrico predeterminado Ad Hoc"
IBSS_TX_POWER_STR           	="Potencia de transmisión"
ROAMING_AGGRESSIVENESS_STR  	="Agresividad de itinerancia"
ADHOC_POWER_MANAGEMENT_STR  	="Administración de energía Ad Hoc"
ADHOC_QOS_MODE_STR          	="Modo QoS Ad Hoc"
MIXED_MODE_PROTECTION_STR   	="Protección de modo mixto"
THROUGHPUT_ENHANCEMENT_STR  	="Optimización de la capacidad de proceso"
WIRELESS_MODE_STR           	="Modo inalámbrico"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Ancho de canal 802.11n para banda 5,2"
CHANNELWIDTH24              	="Ancho de canal 802.11n para banda 2,4"
TGnMode                     	="Modo 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="No compatible con canal de 40 MHz"

LOWEST_STR		    	="Mínimo"
MEDIUM_LOW_STR		    	="Bajo"
MEDIUM_STR		    	="Mediano"
MEDIUM_HIGH_STR		    	="Alto"
HIGHEST_STR		    	="Máximo"
DISABLED_STR		    	="Desactivado"
ENABLED_STR 		    	="Activado"
MAXIMUM_POWER_SAVING_STR	="Máximo ahorro de energía"
NOISY_ENVIRONMENT_STR		="Entorno ruidoso"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS activado"
AUTO_STR                    	="Automático"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automático"
WMM_DISABLED_STR            	="WMM desactivado"
WMM_ENABLED_STR             	="WMM activado"
NO_PREFERECE_STR            	="Sin preferencias"
PREFER_24_BAND_STR          	="Preferir la banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir la banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet de reactivación"
WAKE_ON_PATTERN_MATCH       	="Coincidencia de patrones de reactivación"
PM_WIFI_REKEY_OFFLOAD	    	="Regeneración de clave GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspensión al desconectar WoWLAN"

SOURCEDISK1                  ="Disco de instalación de Intel(R) Wireless WiFi Link serie 5000"

[Strings.040B] ; Finnish (Finland)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 -ohjain"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 -ohjain"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 -ohjain"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 -ohjain"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 -ohjain"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 -ohjain"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 -ohjain"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 -sovitinohjain Windows 8 64-bit -käyttöjärjestelmään"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN -ohjain"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN -sovitinohjain Windows 8 64-bit -käyttöjärjestelmään"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG -ohjain"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG -sovitinohjain Windows 8 64-bit -käyttöjärjestelmään"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN -ohjain"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN -sovitinohjain Windows 8 64-bit -käyttöjärjestelmään"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000 -sarjan sovitinohjain 8 64-bit -käyttöjärjestelmään"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad Hoc -kanava 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad Hoc -kanava 802.11a "
RECOMMENDED_BAND            	="Langaton Ad Hoc -oletustila"
IBSS_TX_POWER_STR           	="Lähetysteho"
ROAMING_AGGRESSIVENESS_STR  	="Solukonpäivitysaktiivisuus"
ADHOC_POWER_MANAGEMENT_STR  	="Ad Hoc -virranhallinta"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS -tila"
MIXED_MODE_PROTECTION_STR   	="Sekatilan Suojaus"
THROUGHPUT_ENHANCEMENT_STR  	="Läpimenon parantaminen"
WIRELESS_MODE_STR           	="Langaton tila"
PREFERRED_BAND_STR          	="Ensisijainen kaista"
CHANNELWIDTH52              	="802.11n-kanavaleveys kaistalle 5,2"
CHANNELWIDTH24              	="802.11n-kanavaleveys kaistalle 2,4"
TGnMode                     	="802.11n-tila"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Fat Channel -esto"

LOWEST_STR		    	="Pienin"
MEDIUM_LOW_STR		    	="Kohtalainen-pieni"
MEDIUM_STR		    	="Kohtalainen"
MEDIUM_HIGH_STR		    	="Kohtalainen-suuri"
HIGHEST_STR		    	="Suurin"
DISABLED_STR		    	="Poissa käytöstä"
ENABLED_STR 		    	="Käytössä"
MAXIMUM_POWER_SAVING_STR	="Suurin virransäästö"
NOISY_ENVIRONMENT_STR		="Häiriöllinen ympäristö"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS itselle käytössä"
RTS_CTS_ENABLED_STR         	="RTS/CTS käytössä"
AUTO_STR                    	="Automaattinen"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaattinen"
WMM_DISABLED_STR            	="WMM poissa käytöstä"
WMM_ENABLED_STR             	="WMM käytössä"
NO_PREFERECE_STR            	="Ei ensisijaisuutta"
PREFER_24_BAND_STR          	="2,4 GHz:n kaista ensisijainen"
PREFER_52_BAND_STR          	="5,2 GHz:n kaista ensisijainen"
WAKE_ON_MAGIC_PACKET        	="Aktivointi Magic-paketilla"
WAKE_ON_PATTERN_MATCH       	="Aktivointi mallivastaavuudella"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN-toiminnon GTK-uudelleenavainnus "
PM_ARP_OFFLOAD			="WoWLAN-toiminnon ARP-purku"
PM_NS_OFFLOAD			="WoWLAN-toiminnon NS-purku"
DEVICE_SLEEP_ON_DISCONNECT	="Lepotilaan, kun WoWLAN-yhteys katkaistu"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 -sarja asennuslevy"

[Strings.040C] ; French (France)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Pilote Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Pilote Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Pilote Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Pilote Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Pilote Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Pilote Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Pilote Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Pilote de carte réseau Intel(R) Centrino(R) Wireless-N 6150 pour Windows 8 64 bits"
NIC_DriverDesc_6250AGN_2x2              ="Pilote Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Pilote de carte réseau Intel(R) Centrino(R) Advanced-N 6250 AGN pour Windows 8 64 bits"
NIC_DriverDesc_6250ABG_2x2              ="Pilote Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Pilote de carte réseau Intel(R) Centrino(R) Advanced-N 6250 ABG pour Windows 8 64 bits"
NIC_DriverDesc_6300AGN_3x3              ="Pilote Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Pilote de carte réseau Intel(R) Centrino(R) Ultimate-N 6300 AGN pour Windows 8 64 bits"

NIC_Service_DispName_WIN8_64								="Pilote de carte de la série Intel(R) Wireless WiFi Link 5000 pour Windows 8 64 bits "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Canal ad hoc 802.11a"
RECOMMENDED_BAND            	="Mode ad hoc sans fil par défaut"
IBSS_TX_POWER_STR           	="Puissance de transmission"
ROAMING_AGGRESSIVENESS_STR  	="Agressivité de l’itinérance"
ADHOC_POWER_MANAGEMENT_STR  	="Gestion de l'alimentation ad hoc"
ADHOC_QOS_MODE_STR          	="Mode Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protection en mode mixte"
THROUGHPUT_ENHANCEMENT_STR  	="Optimisation du débit"
WIRELESS_MODE_STR           	="Mode Sans fil"
PREFERRED_BAND_STR          	="Bande privilégiée"
CHANNELWIDTH52              	="Largeur de canal 802.11n - bande 5,2"
CHANNELWIDTH24              	="Largeur de canal 802.11n - bande 2,4"
TGnMode                     	="Mode 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Incompatible avec canaux de 40 MHz"

LOWEST_STR		    	="Min."
MEDIUM_LOW_STR		    	="Faible"
MEDIUM_STR		    	="Moyenne"
MEDIUM_HIGH_STR		    	="Élevée"
HIGHEST_STR		    	="Max."
DISABLED_STR		    	="Désactivée"
ENABLED_STR 		    	="Activé"
MAXIMUM_POWER_SAVING_STR	="Économie d'énergie max."
NOISY_ENVIRONMENT_STR		="Environnement bruyant"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="Auto-CTS activée"
RTS_CTS_ENABLED_STR         	="RTS/CTS activée"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM désactivée"
WMM_ENABLED_STR             	="WMM activée"
NO_PREFERECE_STR            	="Aucune préférence"
PREFER_24_BAND_STR          	="Préférer bande 2,4 GHz"
PREFER_52_BAND_STR          	="Préférer bande 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondance au modèle WOL"
PM_WIFI_REKEY_OFFLOAD	    	="Régénération des clés GTK pour WoWLAN"
PM_ARP_OFFLOAD			="Délestage ARP pour WoWLAN"
PM_NS_OFFLOAD			="Délestage NS pour WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Veille à la déconnexion WoWLAN"

SOURCEDISK1                  ="Disque d'installation de la série Intel(R) Wireless WiFi Link 5000"

[Strings.040D] ; Hebrew (Israel)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="îðäì äú÷ï ùì Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="îðäì äú÷ï ùì Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="îðäì äú÷ï ùì Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="îðäì äú÷ï ùì Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="îðäì äú÷ï ùì Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="îðäì äú÷ï ùì Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="îðäì äú÷ï ùì Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="îðäì äú÷ï ùì îúàí Intel(R) Centrino(R) Wireless-N 6150 òáåø Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="îðäì äú÷ï ùì Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="îðäì äú÷ï ùì îúàí Intel(R) Centrino(R) Advanced-N 6250 AGN òáåø Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="îðäì äú÷ï ùì Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="îðäì äú÷ï ùì îúàí Intel(R) Centrino(R) Advanced-N 6250 ABG òáåø Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="îðäì äú÷ï ùì Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="îðäì äú÷ï ùì îúàí Intel(R) Centrino(R) Ultimate-N 6300 AGN òáåø Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link ñãøú 5000 òáåø Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="òøåõ àã äå÷ 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="òøåõ àã äå÷ 802.11a"
RECOMMENDED_BAND            	="îöá àìçåèé áøéøú îçãì ùì àã äå÷"
IBSS_TX_POWER_STR           	="òåöîú ùéãåø"
ROAMING_AGGRESSIVENESS_STR  	="úå÷ôðåú ðãéãä"
ADHOC_POWER_MANAGEMENT_STR  	="ðéäåì öøéëú çùîì àã äå÷"
ADHOC_QOS_MODE_STR          	="îöá QoS àã-äå÷"
MIXED_MODE_PROTECTION_STR   	="äâðú îöá îòåøá"
THROUGHPUT_ENHANCEMENT_STR  	="ùéôåø ÷öá äòáøä"
WIRELESS_MODE_STR           	="îöá àìçåèé"
PREFERRED_BAND_STR          	="ôñ îåòãó"
CHANNELWIDTH52              	="øåçá òøåõ 802.11n òáåø ôñ 5.2"
CHANNELWIDTH24              	="øåçá òøåõ 802.11n òáåø ôñ 2.4"
TGnMode                     	="îöá 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="ìà úåàí ìòøåõ 40Mhz"

LOWEST_STR		    	="ðîåê áéåúø"
MEDIUM_LOW_STR		    	="áéðåðé-ðîåê"
MEDIUM_STR		    	="áéðåðé"
MEDIUM_HIGH_STR		    	="áéðåðé-âáåä"
HIGHEST_STR		    	="âáåä áéåúø"
DISABLED_STR		    	="îðåèøì"
ENABLED_STR 		    	="æîéï"
MAXIMUM_POWER_SAVING_STR	="çéñëåï îøáé áçùîì"
NOISY_ENVIRONMENT_STR		="ñáéáä øåòùú"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="îàåôùø CTS-àì-òöîå"
RTS_CTS_ENABLED_STR         	="îàåôùø RTS/CTS"
AUTO_STR                    	="àåèåîèé"
CHANNELWIDTH20ONLY          	="ý20 MHz"
CHANNELWIDTHAUTO            	="àåèåîèé"
WMM_DISABLED_STR            	="WMM îðåèøì"
WMM_ENABLED_STR             	="WMM æîéï"
NO_PREFERECE_STR            	="àéï äòãôä"
PREFER_24_BAND_STR          	="äòãôú ôñ ý2.4 GHz"
PREFER_52_BAND_STR          	="äòãôú ôñ ý5.2 GHz"
WAKE_ON_MAGIC_PACKET        	="äúòåøø áòú îðú Magic"
WAKE_ON_PATTERN_MATCH       	="äúòåøø áòú äúàîú úáðéú"
PM_WIFI_REKEY_OFFLOAD	    	="äçìôú îôúçåú GTK òáåø WoWLAN"
PM_ARP_OFFLOAD			="äòáøú ARP òáåø WoWLAN"
PM_NS_OFFLOAD			="äòáøú NS òáåø WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="ëðéñä ìîöá ùéðä òí ðéúå÷ WoWLAN"

SOURCEDISK1                  ="ãéñ÷ äú÷ðä ùì Intel(R) Wireless WiFi Link ñãøú 5000"

[Strings.040E] ; Hungarian (Hungary)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 illesztõprogram"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 illesztõprogram"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 illesztõprogram"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 illesztõprogram"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 illesztõprogram"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 illesztõprogram"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 illesztõprogram"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 adapter illesztõprogram 64 bites Windows 8"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN illesztõprogram"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN adapter illesztõprogram 64 bites Windows 8"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG illesztõprogram"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG adapter illesztõprogram 64 bites Windows 8"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN illesztõprogram"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN adapter illesztõprogram 64 bites Windows 8"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000 Series adapter illesztõprogram 64 bites Windows 8"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Alkalmi csatorna 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Alkalmi csatorna 802.11a"
RECOMMENDED_BAND            	="Alkalmi kapcsolat alap üzemmódja"
IBSS_TX_POWER_STR           	="Sugárzási teljesítmény"
ROAMING_AGGRESSIVENESS_STR  	="A barangolás intenzitása"
ADHOC_POWER_MANAGEMENT_STR  	="Alkalmi hálózat energiagazdálkodásai"
ADHOC_QOS_MODE_STR          	="Alkalmi QoS üzemmód"
MIXED_MODE_PROTECTION_STR   	="Vegyes üzemmódú védelem"
THROUGHPUT_ENHANCEMENT_STR  	="Az átviteli kapacitás növelése"
WIRELESS_MODE_STR           	="Vezeték nélküli üzemmód"
PREFERRED_BAND_STR          	="Preferált frekvenciasáv"
CHANNELWIDTH52              	="802.11n csatorna-sávszélesség 5,2 GHz"
CHANNELWIDTH24              	="802.11n csatorna-sávszélesség 2,4 GHz"
TGnMode                     	="802.11n üzemmód"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Csökkentett sávszélességen mûködik"

LOWEST_STR		    	="Legalacsonyabb"
MEDIUM_LOW_STR		    	="Közepes - alacsony"
MEDIUM_STR		    	="Közepes"
MEDIUM_HIGH_STR		    	="Közepes - magas"
HIGHEST_STR		    	="Legmagasabb"
DISABLED_STR		    	="Letiltva"
ENABLED_STR 		    	="Engedélyezve"
MAXIMUM_POWER_SAVING_STR	="Max. energiatakarékosság"
NOISY_ENVIRONMENT_STR		="Zajos környezet"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self engedélyezve"
RTS_CTS_ENABLED_STR         	="RTS/CTS engedélyezve"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM letiltva"
WMM_ENABLED_STR             	="WMM engedélyezve"
NO_PREFERECE_STR            	="Nincs preferencia"
PREFER_24_BAND_STR          	="2,4 GHz-es sáv preferálása"
PREFER_52_BAND_STR          	="5,2 GHz-es sáv preferálása"
WAKE_ON_MAGIC_PACKET        	="Ébresztés magic-csomaggal"
WAKE_ON_PATTERN_MATCH       	="Ébresztés mintaegyezésre"
PM_WIFI_REKEY_OFFLOAD	    	="GTK újrakulcsolás WoWLAN hálózathoz"
PM_ARP_OFFLOAD			="ARP tehermentesítés WoWLAN hálózathoz"
PM_NS_OFFLOAD			="NS tehermentesítés WoWLAN hálózathoz"
DEVICE_SLEEP_ON_DISCONNECT	="Alvó állapot WoWLAN hálózati szétkapcsolás esetén"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 Series telepítõ lemez"

[Strings.0410] ; Italian (Italy)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Driver Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Driver Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Driver Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Driver Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Driver Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Driver Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Driver scheda Intel(R) Centrino(R) Wireless-N 6150 per Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Driver scheda Intel(R) Centrino(R) Advanced-N 6250 AGN per Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Driver scheda Intel(R) Centrino(R) Advanced-N 6250 ABG per Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Driver Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Driver scheda Intel(R) Centrino(R) Ultimate-N 6300 AGN per Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Driver scheda Intel(R) Wireless WiFi Link 5000 Series per Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Canale Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Canale Ad Hoc 802.11a"
RECOMMENDED_BAND            	="Modalità wireless predefinita Ad Hoc"
IBSS_TX_POWER_STR           	="Potenza di trasmissione"
ROAMING_AGGRESSIVENESS_STR  	="Efficacia roaming"
ADHOC_POWER_MANAGEMENT_STR  	="Risparmio energia ad hoc"
ADHOC_QOS_MODE_STR          	="Modalità Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protezione a modalità mista"
THROUGHPUT_ENHANCEMENT_STR  	="Miglioramento velocità effettiva"
WIRELESS_MODE_STR           	="Modalità wireless"
PREFERRED_BAND_STR          	="Banda preferita"
CHANNELWIDTH52              	="Larg. canale 802.11n per banda 5,2"
CHANNELWIDTH24              	="Larg. canale 802.11n per banda 2,4"
TGnMode                     	="Modalità 802.11n "
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Fat Channel incompatibile"

LOWEST_STR		    	="Minimo"
MEDIUM_LOW_STR		    	="Medio-basso"
MEDIUM_STR		    	="Medio"
MEDIUM_HIGH_STR		    	="Medio-alto"
HIGHEST_STR		    	="Massimo"
DISABLED_STR		    	="Disattivata"
ENABLED_STR 		    	="Attivata"
MAXIMUM_POWER_SAVING_STR	="Max. risparmio energetico"
NOISY_ENVIRONMENT_STR		="Ambienti rumorosi"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self attivato"
RTS_CTS_ENABLED_STR         	="Attivato RTS/CTS"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM disattivata"
WMM_ENABLED_STR             	="WMM attivata"
NO_PREFERECE_STR            	="Nessuna preferenza"
PREFER_24_BAND_STR          	="Preferenza a banda a 2,4 GHz"
PREFER_52_BAND_STR          	="Preferenza a banda a 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet per riattivazione"
WAKE_ON_PATTERN_MATCH       	="Corrispondenza motivo per riattivazione"
PM_WIFI_REKEY_OFFLOAD	    	="Rigenerazione delle chiavi GTK per WoWLAN"
PM_ARP_OFFLOAD			="Offload ARP per WoWLAN"
PM_NS_OFFLOAD			="Offload NS per WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Sospensione attiva alla disconnessione da WoWLAN"

SOURCEDISK1                  ="Disco di installazione per Intel(R) Wireless WiFi Link 5000 Series"

[Strings.0411] ; Japanese (Japan)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 ƒhƒ‰ƒCƒo�["

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 ƒhƒ‰ƒCƒo�["

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 ƒhƒ‰ƒCƒo�["
NIC_Service_DispName_6150BGN_1x2    	="Windows 8 64 ƒrƒbƒg—p Intel(R) Centrino(R) Wireless-N 6150 ƒAƒ_ƒvƒ^�[ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN ƒhƒ‰ƒCƒo�["
NIC_Service_DispName_6250AGN_2x2    	="Windows 8 64 ƒrƒbƒg—p Intel(R) Centrino(R) Advanced-N 6250 AGN ƒAƒ_ƒvƒ^�[ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG ƒhƒ‰ƒCƒo�["
NIC_Service_DispName_6250ABG_2x2    	="Windows 8 64 ƒrƒbƒg—p Intel(R) Centrino(R) Advanced-N 6250 ABG ƒAƒ_ƒvƒ^�[ƒhƒ‰ƒCƒo�["
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN ƒhƒ‰ƒCƒo�["
NIC_Service_DispName_6300AGN_3x3    	="Windows 8 64 ƒrƒbƒg—p Intel(R) Centrino(R) Ultimate-N 6300 AGN ƒAƒ_ƒvƒ^�[ƒhƒ‰ƒCƒo�["

NIC_Service_DispName_WIN8_64								="Windows 8 64 ƒrƒbƒg—p Intel(R) Wireless WiFi Link 5000 ƒVƒŠ�[ƒY�EƒAƒ_ƒvƒ^�[�Eƒhƒ‰ƒCƒo�["

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="ƒAƒhƒzƒbƒN ƒ`ƒƒƒlƒ‹ 802.11b/g "
RECOMMENDED_CHANNEL52_STR   	="ƒAƒhƒzƒbƒN ƒ`ƒƒƒlƒ‹ 802.11a"
RECOMMENDED_BAND            	="ƒAƒhƒzƒbƒN ƒfƒtƒHƒ‹ƒg ƒ�ƒCƒ„ƒŒƒX ƒ‚�[ƒh"
IBSS_TX_POWER_STR           	="‘—�Mƒpƒ��["
ROAMING_AGGRESSIVENESS_STR  	="ƒ��[ƒ~ƒ“ƒO‚Ì�Ï‹É�«"
ADHOC_POWER_MANAGEMENT_STR  	="ƒAƒhƒzƒbƒN“dŒ¹ŠÇ—�"
ADHOC_QOS_MODE_STR          	="ƒAƒhƒzƒbƒN QoS ƒ‚�[ƒh"
MIXED_MODE_PROTECTION_STR   	="�¬�Ýƒ‚�[ƒh•ÛŒì"
THROUGHPUT_ENHANCEMENT_STR  	="ƒXƒ‹�[ƒvƒbƒg‚Ì‘�‰Á"
WIRELESS_MODE_STR           	="ƒ�ƒCƒ„ƒŒƒX ƒ‚�[ƒh"
PREFERRED_BAND_STR          	="—D�æƒoƒ“ƒh"
CHANNELWIDTH52              	="ƒoƒ“ƒh 5.2 —p 802.11n ƒ`ƒƒƒlƒ‹•�"
CHANNELWIDTH24              	="ƒoƒ“ƒh 2.4 —p 802.11n ƒ`ƒƒƒlƒ‹•�"
TGnMode                     	="802.11n ƒ‚�[ƒh"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="40Mhz ƒ`ƒƒƒlƒ‹•�”ñŒÝŠ·"

LOWEST_STR		    	="�Å’á"
MEDIUM_LOW_STR		    	="’†’á"
MEDIUM_STR		    	="’†"
MEDIUM_HIGH_STR		    	="’†�‚"
HIGHEST_STR		    	="�Å�‚"
DISABLED_STR		    	="–³Œø"
ENABLED_STR 		    	="—LŒø"
MAXIMUM_POWER_SAVING_STR	="�Å‘å�ß“d"
NOISY_ENVIRONMENT_STR		="ŽG‰¹ŠÂ‹«"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="ŒÂ•Ê CTS —LŒø"
RTS_CTS_ENABLED_STR         	="RTS/CTS —LŒø"
AUTO_STR                    	="Ž©“®"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Ž©“®"
WMM_DISABLED_STR            	="WMM –³Œø"
WMM_ENABLED_STR             	="WMM —LŒø"
NO_PREFERECE_STR            	="—D�æ�‡ˆÊ‚È‚µ"
PREFER_24_BAND_STR          	="2.4 GHz ƒoƒ“ƒh‚Ì—D�æ"
PREFER_52_BAND_STR          	="5.2 GHz ƒoƒ“ƒh‚Ì—D�æ"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN ‚Ì GTK Rekey"
PM_ARP_OFFLOAD			="WoWLAN ‚Ì ARP ƒIƒtƒ��[ƒh"
PM_NS_OFFLOAD			="WoWLAN ‚Ì NS ƒIƒtƒ��[ƒh"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN ‚ÌƒXƒŠ�[ƒv�ó‘Ô‚Ì‰ð�œ"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 ƒVƒŠ�[ƒY�EƒCƒ“ƒXƒg�[ƒ‹�EƒfƒBƒXƒN"

[Strings.0412] ; Korean (Korea)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 µå¶óÀÌ¹ö"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 µå¶óÀÌ¹ö"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 µå¶óÀÌ¹ö"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 µå¶óÀÌ¹ö"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 µå¶óÀÌ¹ö"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 µå¶óÀÌ¹ö"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 µå¶óÀÌ¹ö"
NIC_Service_DispName_6150BGN_1x2    	="Windows 8 64ºñÆ®¿ë Intel(R) Centrino(R) Wireless-N 6150 ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN µå¶óÀÌ¹ö"
NIC_Service_DispName_6250AGN_2x2    	="Windows 8 64ºñÆ®¿ë Intel(R) Centrino(R) Advanced-N 6250 AGN ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG µå¶óÀÌ¹ö"
NIC_Service_DispName_6250ABG_2x2    	="Windows 8 64ºñÆ®¿ë Intel(R) Centrino(R) Advanced-N 6250 ABG ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN µå¶óÀÌ¹ö"
NIC_Service_DispName_6300AGN_3x3    	="Windows 8 64ºñÆ®¿ë Intel(R) Centrino(R) Ultimate-N 6300 AGN ¾î´ðÅÍ µå¶óÀÌ¹ö"

NIC_Service_DispName_WIN8_64								="Windows 8 64ºñÆ®¿ë Intel(R) Wireless WiFi Link 5000 ½Ã¸®Áî ¾î´ðÅÍ µå¶óÀÌ¹ö"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad Hoc Ã¤³Î 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad Hoc Ã¤³Î 802.11a"
RECOMMENDED_BAND            	="Ad Hoc ±âº» ¹«¼± ¸ðµå"
IBSS_TX_POWER_STR           	="Àü¼Û Àü¿ø"
ROAMING_AGGRESSIVENESS_STR  	="·Î¹ÖÀÇ ÁÖµ¿¼º"
ADHOC_POWER_MANAGEMENT_STR  	="Ad Hoc Àü¿ø °ü¸®"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS ¸ðµå"
MIXED_MODE_PROTECTION_STR   	="È¥ÇÕ ¸ðµå º¸È£"
THROUGHPUT_ENHANCEMENT_STR  	="Ã³¸®·® °³¼±"
WIRELESS_MODE_STR           	="¹«¼± ¸ðµå"
PREFERRED_BAND_STR          	="±âº» ¼³Á¤ ¹êµå"
CHANNELWIDTH52              	="¹êµå 5.2¿¡ ´ëÇÑ 802.11n Ã¤³Î Æø"
CHANNELWIDTH24              	="¹êµå 2.4¿¡ ´ëÇÑ 802.11n Ã¤³Î Æø"
TGnMode                     	="802.11n ¸ðµå"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="°úºÎÇÏ Ã¤³Î ºñÁö¿ø"

LOWEST_STR		    	="ÃÖÇÏ"
MEDIUM_LOW_STR		    	="º¸Åë-³·À½"
MEDIUM_STR		    	="º¸Åë"
MEDIUM_HIGH_STR		    	="º¸Åë-³ôÀ½"
HIGHEST_STR		    	="ÃÖ°í"
DISABLED_STR		    	="ºñÈ°¼ºÈ­ÇÔ"
ENABLED_STR 		    	="È°¼ºÈ­ÇÔ"
MAXIMUM_POWER_SAVING_STR	="ÃÖ´ë ÀýÀü"
NOISY_ENVIRONMENT_STR		="ÀâÀ½ È¯°æ"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="ÀÚÃ¼ CTS È°¼ºÈ­ÇÔ"
RTS_CTS_ENABLED_STR         	="RTS/CTS È°¼ºÈ­ÇÔ"
AUTO_STR                    	="ÀÚµ¿"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="ÀÚµ¿"
WMM_DISABLED_STR            	="WMM ºñÈ°¼ºÈ­ÇÔ"
WMM_ENABLED_STR             	="WMM È°¼ºÈ­ÇÔ"
NO_PREFERECE_STR            	="±âº» ¼³Á¤ ¾øÀ½"
PREFER_24_BAND_STR          	="2.4 GHz ¹êµå ¼±ÅÃ"
PREFER_52_BAND_STR          	="5.2 GHz ¹êµå ¼±ÅÃ"
WAKE_ON_MAGIC_PACKET        	="Wake on ¸ÅÁ÷ ÆÐÅ¶"
WAKE_ON_PATTERN_MATCH       	="Wake on ÆÐÅÏ ÀÏÄ¡"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN¿¡ ´ëÇÑ GTK Å° ÀçÀÔ·Â"
PM_ARP_OFFLOAD			="WoWLAN¿¡ ´ëÇÑ ARP ¿ÀÇÁ·Îµå"
PM_NS_OFFLOAD			="WoWLAN¿¡ ´ëÇÑ NS ¿ÀÇÁ·Îµå"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN ¿¬°á ÇØÁ¦ ½Ã ÀýÀü »óÅÂ"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 ½Ã¸®Áî ¼³Ä¡ µð½ºÅ©"

[Strings.0413] ; Dutch (Netherlands)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 stuurprogramma"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 stuurprogramma"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 stuurprogramma"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 stuurprogramma"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 stuurprogramma"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 stuurprogramma"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 stuurprogramma"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 adapter stuurprogramma onder Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN stuurprogramma"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN adapter stuurprogramma onder Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG stuurprogramma"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG adapter stuurprogramma onder Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN stuurprogramma"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN adapter stuurprogramma onder Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000 Series adapter stuurprogramma onder Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad-hockanaal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad-hockanaal 802.11a"
RECOMMENDED_BAND            	="Ad-hoc standaard draadloze modus"
IBSS_TX_POWER_STR           	="Verzendenergie"
ROAMING_AGGRESSIVENESS_STR  	="Agressiviteit bij zwerven"
ADHOC_POWER_MANAGEMENT_STR  	="Energiebeheer ad-hocverbindingen"
ADHOC_QOS_MODE_STR          	="Ad-hoc QoS-modus"
MIXED_MODE_PROTECTION_STR   	="Beveiliging van gemengde modus"
THROUGHPUT_ENHANCEMENT_STR  	="Verbetering van  doorvoer"
WIRELESS_MODE_STR           	="Draadloze modus"
PREFERRED_BAND_STR          	="Voorkeursband"
CHANNELWIDTH52              	="802.11n-kanaalbreedte voor 5.2 band"
CHANNELWIDTH24              	="802.11n-kanaalbreedte voor 2.4 band"
TGnMode                     	="802.11n-modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Niet compatibel met 40-Mhz kanaal"

LOWEST_STR		    	="Laagste"
MEDIUM_LOW_STR		    	="Laag"
MEDIUM_STR		    	="Normaal"
MEDIUM_HIGH_STR		    	="Hoog"
HIGHEST_STR		    	="Hoogste"
DISABLED_STR		    	="Uitgeschakeld"
ENABLED_STR 		    	="Ingeschakeld"
MAXIMUM_POWER_SAVING_STR	="Maximale energiebesparing"
NOISY_ENVIRONMENT_STR		="Omgeving met ruis"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-naar-zelf ingeschakeld"
RTS_CTS_ENABLED_STR         	="RTS/CTS ingeschakeld"
AUTO_STR                    	="Automatisch"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisch"
WMM_DISABLED_STR            	="WMM uitgeschakeld"
WMM_ENABLED_STR             	="WMM ingeschakeld"
NO_PREFERECE_STR            	="Geen voorkeur"
PREFER_24_BAND_STR          	="Voorkeur voor 2,4-GHz band"
PREFER_52_BAND_STR          	="Voorkeur voor 5,2-GHz band"
WAKE_ON_MAGIC_PACKET        	="Activeren na Magic-pakket"
WAKE_ON_PATTERN_MATCH       	="patroonovereenkomst"
PM_WIFI_REKEY_OFFLOAD	    	="GTK opnieuw versleutelen voor WoWLAN"
PM_ARP_OFFLOAD			="ARP-offload voor WoWLAN"
PM_NS_OFFLOAD			="NS-offload voor WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slapen bij verbroken WoWLAN-verbinding"

SOURCEDISK1                  ="Installatieschijf voor Intel(R) Wireless WiFi Link 5000 Series"

[Strings.0414] ; Norwegian (Bokmål) (Norway)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 driver"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 driver"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 driver"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 driver"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 driver"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 driver"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 driver"
NIC_Service_DispName_6150BGN_1x2    	="Intel(R) Centrino(R) Wireless-N 6150 kortdriver for Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN driver"
NIC_Service_DispName_6250AGN_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 AGN kortdriver for Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG driver"
NIC_Service_DispName_6250ABG_2x2    	="Intel(R) Centrino(R) Advanced-N 6250 ABG kortdriver for Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN driver"
NIC_Service_DispName_6300AGN_3x3    	="Intel(R) Centrino(R) Ultimate-N 6300 AGN kortdriver for Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Intel(R) Wireless WiFi Link 5000-serien kortdriver for Windows 8 64-bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad Hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad Hoc-kanal 802.11a"
RECOMMENDED_BAND            	="Ad hoc standard trådløsmodus"
IBSS_TX_POWER_STR           	="Overføringsstrøm"
ROAMING_AGGRESSIVENESS_STR  	="Streifingsaggresjon"
ADHOC_POWER_MANAGEMENT_STR  	="Ad Hoc strømstyring"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS modus"
MIXED_MODE_PROTECTION_STR   	="Blandet modus-beskyttelse"
THROUGHPUT_ENHANCEMENT_STR  	="Gjennomstrømningsutvidelse"
WIRELESS_MODE_STR           	="Trådløsmodus"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="802.11n-kanalbredde for bånd 5.2"
CHANNELWIDTH24              	="802.11n-kanalbredde for bånd 2.4"
TGnMode                     	="802.11n-modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Intolerant for kanal"

LOWEST_STR		    	="Laveste"
MEDIUM_LOW_STR		    	="Middels-lav"
MEDIUM_STR		    	="Middels"
MEDIUM_HIGH_STR		    	="Middels-høy"
HIGHEST_STR		    	="Høyeste"
DISABLED_STR		    	="Deaktivert"
ENABLED_STR 		    	="Aktivert"
MAXIMUM_POWER_SAVING_STR	="Maksimal strømsparing"
NOISY_ENVIRONMENT_STR		="Støyende miljø"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-til-selv aktivert"
RTS_CTS_ENABLED_STR         	="RTS/CTS-aktivert"
AUTO_STR                    	="Automatisk"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisk"
WMM_DISABLED_STR            	="WMM deaktivert"
WMM_ENABLED_STR             	="WMM aktivert"
NO_PREFERECE_STR            	="Ingen preferanser"
PREFER_24_BAND_STR          	="Foretrekk 2,4 GHz-bånd"
PREFER_52_BAND_STR          	="Foretrekk 5,2 GHz-bånd"
WAKE_ON_MAGIC_PACKET        	="Reaktivert etter magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Reaktivert etter samsvarende mønster"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-omnøkling for WoWLAN"
PM_ARP_OFFLOAD			="ARP-avlastning for WoWLAN"
PM_NS_OFFLOAD			="NS-avlastning for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Hvilemodus ved WoWLAN-frakobling"

SOURCEDISK1                  ="Installasjonsplate for Intel(R) Wireless WiFi Link 5000-serien"

[Strings.0415] ; Polish (Poland)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Sterownik Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Sterownik Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Sterownik Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Sterownik Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Sterownik Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Sterownik Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Sterownik Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Sterownik karty Intel(R) Centrino(R) Wireless-N 6150 dla systemu Windows 8 64 Bit"
NIC_DriverDesc_6250AGN_2x2              ="Sterownik Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Sterownik karty Intel(R) Centrino(R) Advanced-N 6250 AGN dla systemu Windows 8 64 Bit"
NIC_DriverDesc_6250ABG_2x2              ="Sterownik Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Sterownik karty Intel(R) Centrino(R) Advanced-N 6250 ABG dla systemu Windows 8 64 Bit"
NIC_DriverDesc_6300AGN_3x3              ="Sterownik Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Sterownik karty Intel(R) Centrino(R) Ultimate-N 6300 AGN dla systemu Windows 8 64 Bit"

NIC_Service_DispName_WIN8_64								="Sterownik karty Intel(R) Wireless WiFi Link 5000 Series dla systemu Windows 8 64 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Kana³ Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Kana³ Ad Hoc 802.11a"
RECOMMENDED_BAND            	="Domyœlny tryb sieci bezprzewodowej Ad Hoc"
IBSS_TX_POWER_STR           	="Moc transmisji"
ROAMING_AGGRESSIVENESS_STR  	="Agresywnoœæ mobilnoœci"
ADHOC_POWER_MANAGEMENT_STR  	="Zarz¹dzanie energi¹ w sieci Ad Hoc"
ADHOC_QOS_MODE_STR          	="Tryb Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Ochrona trybu mieszanego"
THROUGHPUT_ENHANCEMENT_STR  	="Rozszerzenie przep³ywnoœci"
WIRELESS_MODE_STR           	="Tryb bezprzewodowy"
PREFERRED_BAND_STR          	="Pasmo preferowane"
CHANNELWIDTH52              	="Szerokoœæ kana³u 802.11n dla pasma 5,2"
CHANNELWIDTH24              	="Szerokoœæ kana³u 802.11n dla pasma 2,4"
TGnMode                     	="Tryb 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Brak tolerancji dla kana³u 40 MHz"

LOWEST_STR		    	="Najni¿sza"
MEDIUM_LOW_STR		    	="Œrednio-niska"
MEDIUM_STR		    	="Œrednia"
MEDIUM_HIGH_STR		    	="Œrednio-wysoka"
HIGHEST_STR		    	="Najwy¿sza"
DISABLED_STR		    	="Wy³¹czono"
ENABLED_STR 		    	="W³¹czono"
MAXIMUM_POWER_SAVING_STR	="Maks. oszczêdnoœæ energii"
NOISY_ENVIRONMENT_STR		="Œrodowisko z zak³óceniami"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="W³¹czony zwrotny CTS"
RTS_CTS_ENABLED_STR         	="W³¹czony RTS/CTS"
AUTO_STR                    	="Automatyczny"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatyczny"
WMM_DISABLED_STR            	="Wy³¹czono WMM"
WMM_ENABLED_STR             	="W³¹czono WMM"
NO_PREFERECE_STR            	="Bez preferencji"
PREFER_24_BAND_STR          	="Preferowany pasmo 2,4 GHz"
PREFER_52_BAND_STR          	="Preferowany pasmo 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wznawianie na podstawie pakietu Magic"
WAKE_ON_PATTERN_MATCH       	="Wznawianie na podstawie dopasowania do wzorca"
PM_WIFI_REKEY_OFFLOAD	    	="GTK tworzy klucze ponowne dla WoWLAN"
PM_ARP_OFFLOAD			="Odci¹¿anie ARP dla WoWLAN"
PM_NS_OFFLOAD			="Odci¹¿anie NS dla WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Uœpienie WoWLAN Disconnect"

SOURCEDISK1                  ="Dysk instalacyjny Intel(R) Wireless WiFi Link 5000 Series"

[Strings.0416] ; Portuguese (Brazil)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Driver Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Driver Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Driver Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Driver Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Driver Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Driver Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Driver do adaptador Intel(R) Centrino(R) Wireless-N 6150 para Windows 8 64 bits"
NIC_DriverDesc_6250AGN_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Driver do adaptador Intel(R) Centrino(R) Advanced-N 6250 AGN para Windows 8 64 bits"
NIC_DriverDesc_6250ABG_2x2              ="Driver Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Driver do adaptador Intel(R) Centrino(R) Advanced-N 6250 ABG para Windows 8 64 bits"
NIC_DriverDesc_6300AGN_3x3              ="Driver Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Driver do adaptador Intel(R) Centrino(R) Ultimate-N 6300 AGN para Windows 8 64 bits"

NIC_Service_DispName_WIN8_64								="Driver do adaptador Intel(R) Wireless WiFi Link Série 5000 para Windows 8 64 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Canal ad-hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Canal ad-hoc 802.11a"
RECOMMENDED_BAND            	="Modo sem fio padrão ad-hoc"
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR  	="Agressividade de roaming"
ADHOC_POWER_MANAGEMENT_STR  	="Gerenciamento de energia ad-hoc"
ADHOC_QOS_MODE_STR          	="Modo QoS Ad-hoc"
MIXED_MODE_PROTECTION_STR   	="Proteção de modo misto"
THROUGHPUT_ENHANCEMENT_STR  	="Aumento da taxa de transferência"
WIRELESS_MODE_STR           	="Modo sem fio"
PREFERRED_BAND_STR          	="Banda preferencial"
CHANNELWIDTH52              	="Largura do canal 802.11n - banda 5.2"
CHANNELWIDTH24              	="Largura do canal 802.11n - banda 2.4"
TGnMode                     	="Modo 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Sem tolerância a canal gordo"

LOWEST_STR		    	="Mais baixo"
MEDIUM_LOW_STR		    	="Média a baixa"
MEDIUM_STR		    	="Média"
MEDIUM_HIGH_STR		    	="Média a alta"
HIGHEST_STR		    	="Mais alto"
DISABLED_STR		    	="Desabilitado"
ENABLED_STR 		    	="Habilitado"
MAXIMUM_POWER_SAVING_STR	="Economia máx. de energia"
NOISY_ENVIRONMENT_STR		="Ambiente ruidoso"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS auto-ativação ativado"
RTS_CTS_ENABLED_STR         	="RTS/CTS ativado"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM Desativado"
WMM_ENABLED_STR             	="WMM Ativado"
NO_PREFERECE_STR            	="Sem preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Pacote Mágico do Wake on"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Nova geração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarregamento ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarregamento NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender desconexão de WoWLAN"

SOURCEDISK1                  ="Disco da instalação do Intel(R) Wireless WiFi Link Série 5000"

[Strings.0816] ; Portuguese (Portugal)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Controlador Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Controlador Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Controlador Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Controlador Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Controlador Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Controlador Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Controlador do placa Intel(R) Centrino(R) Wireless-N 6150 para Windows 8 64 Bits"
NIC_DriverDesc_6250AGN_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Controlador do placa Intel(R) Centrino(R) Advanced-N 6250 AGN para Windows 8 64 Bits"
NIC_DriverDesc_6250ABG_2x2              ="Controlador Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Controlador do placa Intel(R) Centrino(R) Advanced-N 6250 ABG para Windows 8 64 Bits"
NIC_DriverDesc_6300AGN_3x3              ="Controlador Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="Controlador do placa Intel(R) Centrino(R) Ultimate-N 6300 AGN para Windows 8 64 Bits"

NIC_Service_DispName_WIN8_64								="Controlador da placa Intel(R) Wireless WiFi Link Série 5000 para Windows 8 64 Bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Canal ad hoc 802.11a"
RECOMMENDED_BAND            	="Modo ad hoc sem fios predefinido"
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR  	="Agressividade do roaming"
ADHOC_POWER_MANAGEMENT_STR  	="Gestão de energia ad hoc"
ADHOC_QOS_MODE_STR          	="Modo Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protecção do modo misto"
THROUGHPUT_ENHANCEMENT_STR  	="Melhoria da produtividade"
WIRELESS_MODE_STR           	="Modo sem fios"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Largura do canal 802.11n - banda 5.2"
CHANNELWIDTH24              	="Largura do canal 802.11n - banda 2.4"
TGnMode                     	="Modo 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Canal de grandes volumes incompatível"

LOWEST_STR		    	="Menor"
MEDIUM_LOW_STR		    	="Média-baixa"
MEDIUM_STR		    	="Média"
MEDIUM_HIGH_STR		    	="Média-Elevada"
HIGHEST_STR		    	="Maior"
DISABLED_STR		    	="Desactivado"
ENABLED_STR 		    	="Activado"
MAXIMUM_POWER_SAVING_STR	="Máxima poupança de energia"
NOISY_ENVIRONMENT_STR		="Ambiente ruidoso"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS Activado"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM desactivado"
WMM_ENABLED_STR             	="WMM activado"
NO_PREFERECE_STR            	="Sem Preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Reactivação por Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Regeração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender quando a WoWLAN estiver desligada"

SOURCEDISK1                  ="Disco de Instalação da Intel(R) Wireless WiFi Link Série 5000"

[Strings.041D] ; Swedish (Sweden)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Drivrutin Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="Drivrutin Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="Drivrutin Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="Drivrutin Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="Drivrutin Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="Drivrutin Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="Drivrutin Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="Kortdrivrutin för Windows 8 64-bitars Intel(R) Centrino(R) Wireless-N 6150"
NIC_DriverDesc_6250AGN_2x2              ="Drivrutin Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="Kortdrivrutin för Windows 8 64-bitars Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_DriverDesc_6250ABG_2x2              ="Drivrutin Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="Kortdrivrutin för Windows 8 64-bitars Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_DriverDesc_6300AGN_3x3              ="Drivrutin Intel(R) Centrino(R) Ultimate-N 6300 AGN Driver"
NIC_Service_DispName_6300AGN_3x3    	="Kortdrivrutin för Windows 8 64-bitars Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_Service_DispName_WIN8_64								="Kortdrivrutin för Windows 8 64-bitars Intel(R) Wireless WiFi Link 5000-serien"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Ad hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Ad hoc-kanal 802.11a"
RECOMMENDED_BAND            	="Ad hoc Standard trådlöst läge"
IBSS_TX_POWER_STR           	="Överföringsenergi"
ROAMING_AGGRESSIVENESS_STR  	="Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR  	="Energisparfunktioner för ad hoc"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS-läge"
MIXED_MODE_PROTECTION_STR   	="Skydd för blandat läge"
THROUGHPUT_ENHANCEMENT_STR  	="Genomflödesförbättring"
WIRELESS_MODE_STR           	="Trådlöst läge"
PREFERRED_BAND_STR          	="Förvalt band"
CHANNELWIDTH52              	="802.11n-kanalbredd för bandet 5,2"
CHANNELWIDTH24              	="802.11n-kanalbredd för bandet 2,4"
TGnMode                     	="802.11n-läge"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Inkompatibel med 40 MHz-kanal"

LOWEST_STR		    	="Lägsta"
MEDIUM_LOW_STR		    	="Medel-låg"
MEDIUM_STR		    	="Medel"
MEDIUM_HIGH_STR		    	="Medel-hög"
HIGHEST_STR		    	="Högsta"
DISABLED_STR		    	="Inaktiverad"
ENABLED_STR 		    	="Aktiverad"
MAXIMUM_POWER_SAVING_STR	="Max. energibesparing"
NOISY_ENVIRONMENT_STR		="Miljö med störningar"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-till-själv aktiverat"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiverat"
AUTO_STR                    	="Auto"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM inaktiverad"
WMM_ENABLED_STR             	="WMM aktiverad"
NO_PREFERECE_STR            	="Ingen inställning"
PREFER_24_BAND_STR          	="Föredra 2,4 GHz-bandet"
PREFER_52_BAND_STR          	="Föredra 5,2 GHz-bandet"
WAKE_ON_MAGIC_PACKET        	="Aktivera vid Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivering vid mönstermatchning"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nyckeluppdatering för WoWLAN"
PM_ARP_OFFLOAD			="ARP-avbelastning för WoWLAN"
PM_NS_OFFLOAD			="NS-avbelastning för WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Viloläge vid WoWLAN-frånkoppling"

SOURCEDISK1                  ="Installationsdisk Intel(R) Wireless WiFi Link 5000-serien"

[Strings.041E] ; Thai (Thailand)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Advanced-N 6235"
NIC_DriverDesc_2230BGN_2x2 ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Wireless-N 2230"
NIC_DriverDesc_2200BGN_2x2 ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Wireless-N 2200"
NIC_DriverDesc_0135BGN_1x1 ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Wireless-N 135"
NIC_DriverDesc_0105BGN_1x1 ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Wireless-N 105"

NIC_DriverDesc_6205AGN_2x2              ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Advanced-N 6205"

NIC_DriverDesc_6150BGN_1x2              ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Wireless-N 6150"
NIC_Service_DispName_6150BGN_1x2    	="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Centrino(R) Wireless-N 6150 ÊÓËÃÑº Windows 8 64 ºÔµ"
NIC_DriverDesc_6250AGN_2x2              ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_Service_DispName_6250AGN_2x2    	="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Centrino(R) Advanced-N 6250 AGN ÊÓËÃÑº Windows 8 64 ºÔµ"
NIC_DriverDesc_6250ABG_2x2              ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_Service_DispName_6250ABG_2x2    	="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Centrino(R) Advanced-N 6250 ABG ÊÓËÃÑº Windows 8 64 ºÔµ"
NIC_DriverDesc_6300AGN_3x3              ="ä´ÃàÇÍÃì Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_Service_DispName_6300AGN_3x3    	="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Centrino(R) Ultimate-N 6300 AGN ÊÓËÃÑº Windows 8 64 ºÔµ"

NIC_Service_DispName_WIN8_64								="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link ËÁÒÂàÅ¢ 5000 ÊÓËÃÑº Windows 8 64 ºÔµ"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="áª¹á¹Åà©¾ÒÐ¡Ô¨ 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="áª¹á¹Åà©¾ÒÐ¡Ô¨ 802.11a"
RECOMMENDED_BAND            	="âËÁ´äÃéÊÒÂàÃÔèÁµé¹áººà©¾ÒÐ¡Ô¨"
IBSS_TX_POWER_STR           	="¡ÒÃÊè§¼èÒ¹¾ÅÑ§§Ò¹"
ROAMING_AGGRESSIVENESS_STR  	="¤ÇÒÁáÃ§ã¹¡ÒÃãªé§Ò¹¢éÒÁà¢µ"
ADHOC_POWER_MANAGEMENT_STR  	="¡ÒÃ¨Ñ´¡ÒÃ¾ÅÑ§§Ò¹à©¾ÒÐ¡Ô¨"
ADHOC_QOS_MODE_STR          	="âËÁ´ QoS à©¾ÒÐ¡Ô¨"
MIXED_MODE_PROTECTION_STR   	="¡ÒÃ»éÍ§¡Ñ¹âËÁ´¼ÊÁ"
THROUGHPUT_ENHANCEMENT_STR  	="¡ÒÃà¾ÔèÁ»ÃÐÊÔ·¸ÔÀÒ¾ÍÑµÃÒÃÑºÊè§"
WIRELESS_MODE_STR           	="âËÁ´äÃéÊÒÂ"
PREFERRED_BAND_STR          	="áº¹´ì·ÕèµéÍ§¡ÒÃ"
CHANNELWIDTH52              	="¢¹Ò´áª¹á¹Å 802.11n (5.2 GHz)"
CHANNELWIDTH24              	="¢¹Ò´áª¹á¹Å 802.11n (2.4 GHz)"
TGnMode                     	="âËÁ´ 802.11n"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="äÁèÊÒÁÒÃ¶ãªé¡Ñºáª¹á¹Å¢¹Ò´ãË­è"

LOWEST_STR		    	="µèÓÊØ´"
MEDIUM_LOW_STR		    	="»Ò¹¡ÅÒ§-µèÓ"
MEDIUM_STR		    	="»Ò¹¡ÅÒ§"
MEDIUM_HIGH_STR		    	="»Ò¹¡ÅÒ§-ÊÙ§"
HIGHEST_STR		    	="ÊÙ§ÊØ´"
DISABLED_STR		    	="Â¡àÅÔ¡ãªé§Ò¹"
ENABLED_STR 		    	="à»Ô´¡ÒÃãªé§Ò¹"
MAXIMUM_POWER_SAVING_STR	="¡ÒÃ»ÃÐËÂÑ´¾ÅÑ§§Ò¹ÊÙ§ÊØ´"
NOISY_ENVIRONMENT_STR		="ÊÀÒ¾áÇ´ÅéÍÁ·ÕèÁÕàÊÕÂ§´Ñ§"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="ãªé§Ò¹ CTS-to-self áÅéÇ"
RTS_CTS_ENABLED_STR         	="ãªé§Ò¹ RTS/CTS"
AUTO_STR                    	="ÍÑµâ¹ÁÑµÔ"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="ÍÑµâ¹ÁÑµÔ"
WMM_DISABLED_STR            	="Â¡àÅÔ¡¡ÒÃãªé§Ò¹ WMM"
WMM_ENABLED_STR             	="à»Ô´¡ÒÃãªé§Ò¹ WMM"
NO_PREFERECE_STR            	="äÁèÁÕ¡ÒÃ¡ÓË¹´"
PREFER_24_BAND_STR          	="áº¹´ì 2.4 GHz"
PREFER_52_BAND_STR          	="áº¹´ì 5.2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="GTK ¡ÓÅÑ§¡ÓË¹´¤ÕÂìãËÁèÊÓËÃÑº WoWLAN"
PM_ARP_OFFLOAD			="ARP ÍÍ¿âËÅ´ÊÓËÃÑº WoWLAN"
PM_NS_OFFLOAD			="NS ÍÍ¿âËÅ´ÊÓËÃÑº WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Â¡àÅÔ¡¡ÒÃàª×èÍÁµèÍÊÅÕ»º¹ WoWLAN"

SOURCEDISK1                  ="´ÔÊ¡ìµÔ´µÑé§ Intel(R) Wireless WiFi Link ËÁÒÂàÅ¢ 5000"

[Strings.041F] ; Turkish (Turkey)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_6235AGN_2x2_HMC ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_2230BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_2200BGN_2x2_HMC ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_0135BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_0105BGN_1x1_HMC ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_6205AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_6300AGN_3x3_HMC         ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"
NIC_MPCIEX_6150BGN_1x2_HMC         ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_6250AGN_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_6250ABG_2x2_HMC         ="Intel(R) Centrino(R) Advanced-N 6250 ABG"

NIC_MPCIEX_AdapterModel_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235"
NIC_MPCIEX_AdapterModel_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230"
NIC_MPCIEX_AdapterModel_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200"
NIC_MPCIEX_AdapterModel_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135"
NIC_MPCIEX_AdapterModel_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105"

NIC_MPCIEX_AdapterModel_6205AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6205"

NIC_MPCIEX_AdapterModel_6150BGN_1x2  ="Intel(R) Centrino(R) Wireless-N 6150"
NIC_MPCIEX_AdapterModel_6250AGN_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 AGN"
NIC_MPCIEX_AdapterModel_6250ABG_2x2  ="Intel(R) Centrino(R) Advanced-N 6250 ABG"
NIC_MPCIEX_AdapterModel_6300AGN_3x3  ="Intel(R) Centrino(R) Ultimate-N 6300 AGN"

NIC_DriverDesc_6235AGN_2x2 ="Intel(R) Centrino(R) Advanced-N 6235 Sürücüsü"
NIC_DriverDesc_2230BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2230 Sürücüsü"
NIC_DriverDesc_2200BGN_2x2 ="Intel(R) Centrino(R) Wireless-N 2200 Sürücüsü"
NIC_DriverDesc_0135BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 135 Sürücüsü"
NIC_DriverDesc_0105BGN_1x1 ="Intel(R) Centrino(R) Wireless-N 105 Sürücüsü"

NIC_DriverDesc_6205AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6205 Sürücüsü"

NIC_DriverDesc_6150BGN_1x2              ="Intel(R) Centrino(R) Wireless-N 6150 Sürücüsü"
NIC_Service_DispName_6150BGN_1x2    	="Windows 8 64 Bit için Intel(R) Centrino(R) Wireless-N 6150 Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_6250AGN_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 AGN Sürücüsü"
NIC_Service_DispName_6250AGN_2x2    	="Windows 8 64 Bit için Intel(R) Centrino(R) Advanced-N 6250 AGN Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_6250ABG_2x2              ="Intel(R) Centrino(R) Advanced-N 6250 ABG Sürücüsü"
NIC_Service_DispName_6250ABG_2x2    	="Windows 8 64 Bit için Intel(R) Centrino(R) Advanced-N 6250 ABG Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_6300AGN_3x3              ="Intel(R) Centrino(R) Ultimate-N 6300 AGN Sürücüsü"
NIC_Service_DispName_6300AGN_3x3    	="Windows 8 64 Bit için Intel(R) Centrino(R) Ultimate-N 6300 AGN Baðdaþtýrýcý Sürücüsü"

NIC_Service_DispName_WIN8_64								="Windows 8 64 Bit için Intel(R) Wireless WiFi Link Baðdaþtýrýcý Sürücüsü "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR   	="Aygýttan Aygýta Kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR   	="Aygýttan Aygýta Kanal 802.11a"
RECOMMENDED_BAND            	="Ad Hoc Varsayýlan Baðlantý Modu"
IBSS_TX_POWER_STR           	="Yayýn gücü"
ROAMING_AGGRESSIVENESS_STR  	="Gezinme Zorlamasý"
ADHOC_POWER_MANAGEMENT_STR  	="Aygýttan Aygýta Güç Yönetimi"
ADHOC_QOS_MODE_STR          	="Aygýttan Aygýta QoS Modu"
MIXED_MODE_PROTECTION_STR   	="Karýþýk mod korumasý"
THROUGHPUT_ENHANCEMENT_STR  	="Veri Aktarým Geliþtirici"
WIRELESS_MODE_STR           	="Kablosuz Mod"
PREFERRED_BAND_STR          	="Yeðlenen Bant"
CHANNELWIDTH52              	="5.2 bandý için 802.11n Kanal Geniþliði"
CHANNELWIDTH24              	="2.4 bandý için 802.11n Kanal Geniþliði"
TGnMode                     	="802.11n Modu"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT	    	="Geniþ Kanal için Uyumsuz"

LOWEST_STR		    	="En düþük"
MEDIUM_LOW_STR		    	="Düþük"
MEDIUM_STR		    	="Orta"
MEDIUM_HIGH_STR		    	="Yüksek"
HIGHEST_STR		    	="En yüksek"
DISABLED_STR		    	="Devre dýþý"
ENABLED_STR 		    	="Etkin"
MAXIMUM_POWER_SAVING_STR	="Azami Güç Tasarrufu"
NOISY_ENVIRONMENT_STR		="Gürültülü Ortam"
WMM_STR                     	="WMM"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self etkin"
RTS_CTS_ENABLED_STR         	="RTS/CTS etkin"
AUTO_STR                    	="Otomatik"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Otomatik"
WMM_DISABLED_STR            	="WMM devre dýþý"
WMM_ENABLED_STR             	="WMM etkin"
NO_PREFERECE_STR            	="Tercih yok"
PREFER_24_BAND_STR          	="2,4 GHz bant Tercih Et"
PREFER_52_BAND_STR          	="5,2 GHz bant Tercih Et"
WAKE_ON_MAGIC_PACKET        	="Sihirli Paket Uyanmasý"
WAKE_ON_PATTERN_MATCH       	="Desen eþleþtirme uyanmasý"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN için GTK yeniden anahtarlama"
PM_ARP_OFFLOAD			="WoWLAN için ARP yük boþaltma"
PM_NS_OFFLOAD			="WoWLAN için NS yük boþaltma"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN Baðlantý Kesintisinde uyku durumuna geç"

SOURCEDISK1                  ="Intel(R) Wireless WiFi Link 5000 Serisi Yükleme Diski"



