## UEFI Shell Update BIOS & EC & ME

Simple user guide


Example : X11BK / R105

2018 / 11 / 26


Pica Chiu (#3165-TPE)

USER GUIDE

* If you don’t have any USB shell, please create a UEFI Shell at USB dongle.
  + Put these files into USB dongle as blow and follow the path: ( “H” is my USB )
    - H:\efi\boot\bootx64.efi (this file can download from internet)
    - H:\efi\boot\startup.nsh



* + - H:\BIOS\AfuEfix64.efi
    - H:\BIOS\Command.nsh
    - H:\BIOS\Fpt.efi
    - H:\BIOS\fparts.txt
    - H:\BIOS\FME.nsh
    - H:\BIOS\FBIOS.nsh
    - H:\BIOS\X11BD105\_Cons.IMG(ex.)



* + When enter the shell, the script is “FALL.nsh” and “FBIOS.nsh”
    - FME.nsh : ME update
    - FBIOS.nsh : BIOS update
  + Note : Please use one command for one time.