You will require a quote for .35mm thick electrical steel lamination rotors and stator parts.



You need a 2-pole rotor (optional) made, a 6-pole rotor made and a stator made that is composed of 4 'sectors'(see files attached for reference).


The height for both rotor and stator stacks is 440 laminates tall (154mm tall). Both rotor stack and stator stack are the same height.

The 3.5mm diameter bores in the laminations are for you to hot-rivet the laminations together. RIVETS MUST NOT PROTRUDE NO MORE THAN .7MM FROM EITHER END OF THE FINISHED ROTOR/STATOR SURFACES!

There are .stp and .dwg files attached for rotor and stator laminates (also CAD drawings).


Again, units are in millimeters. Each stack is 440 laminates tall. Both rotor stack and stator stack are the same height. 


You need:


NAME		QTY		Total Laminations

2-pole rotor	1			  440

6-pole rotor	1			  440

stator stack	4		4x 440 = 1760




Please see attached files for reference.


You now have the STEP CAD file for each part.


Thank you for your support and participation!




Fix The World





