The older stock of this bearing has inter-hole mount spacing of 49.57mm
instead of 55.1mm. Please confirm the manufacturer has measured this spacing
between the mount holes instead on relying only on the official datasheet.

It may also be worth not to start fabrication of the endplates until you have 
the pillow block bearings in your physical possession and can confirm the 
dimensions.