     STORM TOTAL PRECIPITATION ACCUMULATION                05/08/08 13:57       
                                                                                
                                                                                
          GAGE/RADAR BIAS ESTIMATE .........................       0.664        
          SAMPLE SIZE (EFFECTIVE NO. GAGE/RADAR PAIRS) .....     359.777        
          MEMORY SPAN (HOURS) OVER WHICH BIAS DETERMINED ...     168.007        
          PRODUCT ADJUSTED BY BIAS ESTIMATE? ...............     NO             

RADAR HALF POWER BEAM WIDTH.................................      0.90 DEG      
MAXIMUM ALLOWABLE PERCENT OF BEAM  BLOCKAGE.................     50.00  %       
MAXIMUM ALLOWABLE PERCENT LIKELIHOOD OF CLUTTER.............     50.00          
PERCENT OF BEAM REQUIRED TO COMPUTE AVERAGE POWER...........     50.00          
PERCENT OF HYBRID SCAN NEEDED TO BE CONSIDERED FULL.........     99.70          
LOW REFLECTIVITY THRESHOLD (dBZ) FOR BASE DATA..............    -32.00 DBZ      
REFLECTIVITY (dBZ) REPRESENTING SIGNIFICANT RAIN............     20.00          
AREA WITH REFLECTIVITY EXCEEDING SIGNIFICANT RAIN THRESHOLD.    150.00 KM**2    
THRESHOLD TIME WITHOUT RAIN FOR RESETTING STP ..............     60.00 MINUTES  
REFLECT-TO-PRECIP RATE CONVERSION MULTIPLICATIVE COEFFICIENT    300.00 DBZ      
REFLECT-TO-PRECIP RATE CONVERSION POWER COEFFICIENT.........      1.40 DBZ      
MIN DBZ FOR CONVERTING TO PRECIP RATE (VIA TABLE LOOKUP)....      0.00          
MAX DBZ FOR CONVERTING TO PRECIP RATE (VIA TABLE LOOKUP)....     70.00          
NUMBER OF EXCLUSION ZONES...................................      0.00          

RANGE BEYOND WHICH TO APPLY RANGE-EFFECT CORRECTION.........    230.00 KM       
1ST COEFFICIENT OF RANGE-EFFECT FUNCTION....................      0.00 DBR      
2ND COEFFICIENT OF RANGE-EFFECT FUNCTION....................      1.00          
3RD COEFFICIENT OF RANGE-EFFECT FUNCTION....................      0.00          
MIN RATE SIGNIFYING PRECIPITATION...........................      0.00 MM/Hr    
MAX PRECIPITATION RATE......................................    103.80 MM/Hr    

REINITIALIZATION TIME LAPSE THRESHOLD (FOR ACCUM PROCESS)...     60.00 MINUTES  
MAX TIME DIFFERENCE BETWEEN SCANS FOR INTERPOLATION.........     30.00 MINUTES  
MIN TIME NEEDED TO ACCUMULATE HOURLY TOTALS.................     54.00 MINUTES  
THRESHOLD FOR HOURLY OUTLIER ACCUMULATION...................    400.00 MM       
HOURLY GAGE ACCUMULATION SCAN ENDING TIME...................      0.00 MINUTES  
MAX ACCUMULATION PER SCAN-TO-SCAN PERIOD....................    400.00 MM       
MAX ACCUMULATION PER HOURLY PERIOD..........................    800.00 MM       

MINUTES AFTER CLOCK HOUR WHEN BIAS IS UPDATED...............     50.00 MINUTES  
THRESHOLD # OF GAGE/RADAR PAIRS NEEDED TO SELECT BIAS.......     10.00          
RESET VALUE OF GAGE/RADAR BIAS ESTIMATE.....................      1.00          
LONGEST ALLOWABLE LAG FOR USE OF BIAS FROM BIAS TABLE.......    168.00 HOURS    

