                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040601           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 09/23/1991   Location: I-40 EB                       
        Pavement Width: 3.86 m.   Section Length: 152.50 m.
        Analysis Date: 06/24/1999 Operator Name: DEE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0      2.0      1.0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     34.1     26.8      2.8
        ---Sealed---                METERS    -----     21.3        0        0

        Transverse Crack            METERS    -----     14.1     35.2      4.1
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      9.0     10.0      3.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0      1.0     33.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     98.2     33.3     10.5

        Spall Trans. Joint          METERS    -----        0      2.3     86.0
                                    NUMBER    -----        0      2.0     32.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    148.2      3.5        0

        AC Patch                    SQ. M.    -----     8.78        0     1.06
                                    NUMBER    -----     21.0        0      2.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    128.1    -----    -----    -----
                                    NUMBER     34.0    -----    -----    -----

Date of survey changed from 9/21/1991 to 9/23/1991 based on schedule and time series review
