                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040606           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 11/21/1989   Location: I-40 E                        
        Pavement Width: 3.91 m.   Section Length: 152.50 m.
        Analysis Date: 01/07/2002 Operator Name: MRE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0        0        0

        Durability Cracking         SQ. M.    -----        0     0.30     0.23
                   Total Slabs Distressed     -----        0      2.0      1.0

        Longitudinal Crack          METERS    -----      4.0        0        0
        ---Sealed---                METERS    -----      2.6        0        0

        Transverse Crack            METERS    -----     23.7     32.0        0
        ---Sealed---                METERS    -----     11.7        0        0
                                    NUMBER    -----     13.0     10.0        0
        ---Sealed---                NUMBER    -----      9.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     10.8     14.5    102.6

        Spall Trans. Joint          METERS    -----      0.6      1.3     66.1
                                    NUMBER    -----      1.0      1.0     31.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    130.0        0        0

        AC Patch                    SQ. M.    -----     7.81     7.60     2.71
                                    NUMBER    -----     27.0     25.0      8.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    129.6    -----    -----    -----
                                    NUMBER     33.0    -----    -----    -----

Date of survey changed from 11/12/1989 to 11/21/1989 based on schedule and time series review
