                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040608           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 11/21/1989   Location: I-40 E                        
        Pavement Width: 3.97 m.   Section Length: 152.50 m.
        Analysis Date: 01/08/2002 Operator Name: MRE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0        0        0

        Durability Cracking         SQ. M.    -----     0.32        0     0.23
                   Total Slabs Distressed     -----      1.0        0      1.0

        Longitudinal Crack          METERS    -----     26.4        0        0
        ---Sealed---                METERS    -----     16.3        0        0

        Transverse Crack            METERS    -----     16.4        0        0
        ---Sealed---                METERS    -----      8.0        0        0
                                    NUMBER    -----      9.0        0        0
        ---Sealed---                NUMBER    -----      5.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      2.8      3.0     64.0

        Spall Trans. Joint          METERS    -----      1.6      3.2     81.1
                                    NUMBER    -----      1.0      3.0     29.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    141.6        0        0

        AC Patch                    SQ. M.    -----    12.37     6.83     2.32
                                    NUMBER    -----     31.0     12.0      5.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    132.2    -----    -----    -----
                                    NUMBER     33.0    -----    -----    -----

