                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040659           Pavement Type: Jointed Plain Concrete        
        Survey Date: 11/21/1989   Location: I-40 E                        
        Pavement Width: 3.74 m.   Section Length: 183.00 m.
        Analysis Date: 11/11/2003 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 183.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0      1.0

        Durability Cracking         SQ. M.    -----    10.07     3.84    13.61
                   Total Slabs Distressed     -----     10.0      2.0     28.0

        Longitudinal Crack          METERS    -----      7.3        0      3.3
        ---Sealed---                METERS    -----      6.2        0        0

        Transverse Crack            METERS    -----     19.5     11.9     32.6
        ---Sealed---                METERS    -----     11.1        0        0
                                    NUMBER    -----     16.0      6.0     11.0
        ---Sealed---                NUMBER    -----      7.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      8.0      8.6     24.9

        Spall Trans. Joint          METERS    -----      2.1      2.7     77.2
                                    NUMBER    -----      2.0      2.0     35.0

        Map Cracking                SQ. M.   119.40    -----    -----    -----
                                    NUMBER     36.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    183.4        0        0

        AC Patch                    SQ. M.    -----     4.82    12.80    19.30
                                    NUMBER    -----     19.0     43.0      5.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    150.9    -----    -----    -----
                                    NUMBER     40.0    -----    -----    -----

