                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040660           Pavement Type: Jointed Plain Concrete        
        Survey Date: 11/21/1989   Location: I-40 E                        
        Pavement Width: 3.84 m.   Section Length: 152.50 m.
        Analysis Date: 11/11/2003 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0      1.0      1.0

        Durability Cracking         SQ. M.    -----    10.65     0.14     0.53
                   Total Slabs Distressed     -----     19.0      1.0      3.0

        Longitudinal Crack          METERS    -----     10.3        0        0
        ---Sealed---                METERS    -----      3.4        0        0

        Transverse Crack            METERS    -----     39.7     28.0      7.9
        ---Sealed---                METERS    -----     12.9        0        0
                                    NUMBER    -----     17.0      8.0      2.0
        ---Sealed---                NUMBER    -----      4.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     14.2      5.1     28.2

        Spall Trans. Joint          METERS    -----     11.8     25.9     49.5
                                    NUMBER    -----      6.0     10.0     17.0

        Map Cracking                SQ. M.    79.36    -----    -----    -----
                                    NUMBER     10.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    152.8        0        0

        AC Patch                    SQ. M.    -----     4.11     4.13     0.75
                                    NUMBER    -----     23.0     14.0      4.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    128.2    -----    -----    -----
                                    NUMBER     33.0    -----    -----    -----

