                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 040661           Pavement Type: Jointed Plain Concrete        
        Survey Date: 11/21/1989   Location: I-40 E                        
        Pavement Width: 3.77 m.   Section Length: 134.00 m.
        Analysis Date: 11/18/2003 Operator Name: KAE                           
        Section Start : 0.00 m.   Section End   : 134.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     0.32     0.30    20.13
                   Total Slabs Distressed     -----        0        0     30.0

        Longitudinal Crack          METERS    -----     26.5      4.9      8.3
        ---Sealed---                METERS    -----     20.9        0        0

        Transverse Crack            METERS    -----     13.9     19.5     52.7
        ---Sealed---                METERS    -----      5.5        0        0
                                    NUMBER    -----     14.0     10.0     28.0
        ---Sealed---                NUMBER    -----      4.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      5.9      1.5     40.0

        Spall Trans. Joint          METERS    -----        0        0     73.8
                                    NUMBER    -----        0        0     29.0

        Map Cracking                SQ. M.   116.28    -----    -----    -----
                                    NUMBER     26.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    134.1        0        0

        AC Patch                    SQ. M.    -----     5.59    11.81    12.07
                                    NUMBER    -----     24.0     31.0     17.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    109.8    -----    -----    -----
                                    NUMBER     29.0    -----    -----    -----

