                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 05A602           Pavement Type: Jointed Plain Concrete        
        Survey Date: 01/15/2004   Location: US-65 SB                      
        Pavement Width: 3.89 m.   Section Length: 305.00 m.
        Analysis Date: 04/12/2004 Operator Name: PDE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----    420.5        0        0
        ---Sealed---                METERS    -----    417.8        0        0

        Transverse Crack            METERS    -----      2.0        0        0
        ---Sealed---                METERS    -----      2.0        0        0
                                    NUMBER    -----      2.0        0        0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----        0        0        0

        Spall Trans. Joint          METERS    -----        0        0     13.0
                                    NUMBER    -----        0        0     10.0

        Map Cracking                SQ. M.   681.71    -----    -----    -----
                                    NUMBER     23.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    290.2        0        0

        AC Patch                    SQ. M.    -----   116.65     2.55     3.87
                                    NUMBER    -----     68.0      2.0      3.0

        PCC Patch                   SQ. M.    -----    87.29     0.54     7.62
                                    NUMBER    -----     42.0      2.0      5.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    331.6    -----    -----    -----
                                    NUMBER     86.0    -----    -----    -----

