                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 05a602           Pavement Type: Jointed Plain Concrete        
        Survey Date: 11/11/1999   Location: US-65 SB                      
        Pavement Width: 3.65 m.   Section Length: 305.00 m.
        Analysis Date: 01/13/2000 Operator Name: KAE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----    445.4      3.2        0
        ---Sealed---                METERS    -----    442.2        0        0

        Transverse Crack            METERS    -----      3.3        0        0
        ---Sealed---                METERS    -----      3.3        0        0
                                    NUMBER    -----      4.0        0        0
        ---Sealed---                NUMBER    -----      4.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     63.0     26.0      2.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      0.5        0        0

        Spall Trans. Joint          METERS    -----     11.6        0     12.6
                                    NUMBER    -----     10.0        0     12.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.5        0        0

        AC Patch                    SQ. M.    -----    10.62        0        0
                                    NUMBER    -----     31.0        0        0

        PCC Patch                   SQ. M.    -----   102.86        0     0.14
                                    NUMBER    -----     64.0        0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    329.2    -----    -----    -----
                                    NUMBER     91.0    -----    -----    -----

