                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 060603           Pavement Type: Existing AC Overlay of JCP    
        Survey Date: 10/13/2003   Location: I-5 NB                        
        Pavement Width: 4.63 m.   Section Length: 152.50 m.
        Analysis Date: 02/10/2004 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Fatigue Cracking            SQ. M.    -----     3.73        0        0

        Block Cracking              SQ. M.    -----   266.74   339.62        0

        Edge Cracking               METERS    -----        0        0        0

        Longitudinal Crack  
        WheelPath                   METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Non-WheelPath               METERS    -----        0        0        0
        ----Sealed---               METERS    -----        0        0        0

        Tran. Reflect Crack         METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Long. Reflect. Crack        METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Cracking         METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        AC Patch                    SQ. M.    -----    94.24        0        0
                                    NUMBER    -----      4.0        0        0

        Potholes                    SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Shoving                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Bleeding                    SQ. M.        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Raveling                    SQ. M.        0    -----    -----    -----

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

