                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 060661_A         Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 02/21/1992   Location: I-5 NORTH                     
        Pavement Width: 3.72 m.   Section Length: 274.50 m.
        Analysis Date: 09/07/1999 Operator Name: HJS                           
        Section Start : 0.00 m.   Section End   : 274.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0     11.0      6.0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     26.3    214.0      3.0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      9.7    282.8    134.5
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      7.0    127.0     38.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     54.0      4.0      1.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     13.6      9.5      1.6

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    261.0        0      0.6

        AC Patch                    SQ. M.    -----    13.32        0        0
                                    NUMBER    -----      1.0        0        0

        PCC Patch                   SQ. M.    -----    45.50    42.36    40.52
                                    NUMBER    -----      9.0      6.0     34.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    219.9    -----    -----    -----
                                    NUMBER     59.0    -----    -----    -----

