                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 060662           Pavement Type: Existing AC Overlay of JCP    
        Survey Date: 10/13/2003   Location: I-5 NB                        
        Pavement Width: 4.38 m.   Section Length: 122.00 m.
        Analysis Date: 02/09/2004 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 122.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Fatigue Cracking            SQ. M.    -----     0.34     0.39        0

        Block Cracking              SQ. M.    -----   111.36        0        0

        Edge Cracking               METERS    -----        0        0        0

        Longitudinal Crack  
        WheelPath                   METERS    -----      3.6      0.3        0
        ---Sealed---                METERS    -----      0.8        0        0

        Non-WheelPath               METERS    -----     85.9     67.3      9.6
        ----Sealed---               METERS    -----     54.7        0        0

        Tran. Reflect Crack         METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Long. Reflect. Crack        METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Cracking         METERS    -----     65.7     17.8        0
        ---Sealed---                METERS    -----     39.2        0        0
                                    NUMBER    -----     35.0     10.0        0
        ---Sealed---                NUMBER    -----     18.0        0        0

        AC Patch                    SQ. M.    -----     3.58    10.02    11.48
                                    NUMBER    -----      7.0      7.0      5.0

        Potholes                    SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Shoving                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Bleeding                    SQ. M.        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Raveling                    SQ. M.        0    -----    -----    -----

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

