                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 060662_A         Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 02/21/1992   Location: I-5 NORTH CALI                
        Pavement Width: 3.67 m.   Section Length: 274.50 m.
        Analysis Date: 09/08/1999 Operator Name: HJS                           
        Section Start : 0.00 m.   Section End   : 274.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      2.0     16.0      4.0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     26.8    109.1      1.9
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     14.8    212.5    154.6
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     10.0     74.0     41.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     51.0      1.0      2.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----    118.0     13.9      5.1

        Spall Trans. Joint          METERS    -----        0      4.1        0
                                    NUMBER    -----        0      2.0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    256.8        0        0

        AC Patch                    SQ. M.    -----    41.42        0        0
                                    NUMBER    -----      4.0        0        0

        PCC Patch                   SQ. M.    -----     0.59     0.92     1.94
                                    NUMBER    -----      2.0      2.0      6.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    194.8    -----    -----    -----
                                    NUMBER     54.0    -----    -----    -----

