                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 170605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 03/26/1996   Location: I-57 NB                       
        Pavement Width: 3.75 m.   Section Length: 305.00 m.
        Analysis Date: 08/12/1997 Operator Name: MRE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      7.5     68.9     29.4
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      2.0     23.0      9.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     27.0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     11.5      2.3        0

        Spall Trans. Joint          METERS    -----      1.3        0        0
                                    NUMBER    -----      2.0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    242.9     39.3     22.6

        AC Patch                    SQ. M.    -----        0     0.45     0.24
                                    NUMBER    -----        0      1.0      1.0

        PCC Patch                   SQ. M.    -----    90.31     6.60        0
                                    NUMBER    -----      9.0      1.0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     99.7    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

