                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 175843           Pavement Type: Continuously Reinforced Conc. 
        Survey Date: 03/06/2001   Location: I-39 NB                       
        Pavement Width: 3.83 m.   Section Length: 152.50 m.
        Analysis Date: 04/06/2001 Operator Name: ECH                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Durability Crack            SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Longitudinal Crack          METERS    -----     10.9      1.5      1.8
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----    245.8     30.8     20.9
                                    NUMBER    -----     66.0      8.0      8.0
                               TOT. NUMBER     82.0    -----    -----    -----

        Map Crack                   SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Construction Joint          NUMBER    -----        0        0        0

        Lane-shoulder Sep.          METERS    -----    152.5        0        0

        AC Patch                    SQ. M.    -----        0     0.57     1.14
                                    NUMBER    -----        0      2.0      1.0

        PCC Patch                   SQ. M.    -----    25.95        0        0
                                    NUMBER    -----      2.0        0        0

        Punchouts                   NUMBER    -----        0        0        0

        Spall Long. Joint           METERS    -----        0      0.5      0.8

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

	OTHER					       SET NUMBER OF CONSTRUCTION JOINTS TO ZERO - NONE PRESENT
