                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 180602           Pavement Type: Jointed Plain Concrete        
        Survey Date: 09/12/2001   Location: US-31 NB                      
        Pavement Width: 3.71 m.   Section Length: 152.50 m.
        Analysis Date: 10/08/2001 Operator Name: ECH                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     5.99     2.83     1.26
                   Total Slabs Distressed     -----      8.0      4.0      8.0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     13.2      0.5      0.5

        Spall Trans. Joint          METERS    -----      3.2      2.8     10.6
                                    NUMBER    -----      6.0      5.0     14.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    130.5        0        0

        AC Patch                    SQ. M.    -----     1.65     0.30    78.50
                                    NUMBER    -----      7.0      2.0     18.0

        PCC Patch                   SQ. M.    -----    88.04        0    58.27
                                    NUMBER    -----     16.0        0     10.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    158.1    -----    -----    -----
                                    NUMBER     50.0    -----    -----    -----

