                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 180605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 04/28/1992   Location: US-31 NB                      
        Pavement Width: 3.73 m.   Section Length: 152.50 m.
        Analysis Date: 07/08/1999 Operator Name: DEE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0        0        0

        Durability Cracking         SQ. M.    -----     1.13     3.43     1.83
                   Total Slabs Distressed     -----        0      3.0      7.0

        Longitudinal Crack          METERS    -----      2.9      1.0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     24.0     26.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      5.4      8.2     15.5

        Spall Trans. Joint          METERS    -----      5.4     10.9      4.3
                                    NUMBER    -----      6.0     12.0      4.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.     0.36    -----    -----    -----
                                    NUMBER      1.0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    153.5        0        0

        AC Patch                    SQ. M.    -----     0.61        0     9.92
                                    NUMBER    -----      3.0        0     27.0

        PCC Patch                   SQ. M.    -----   171.50        0        0
                                    NUMBER    -----     26.0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    185.6    -----    -----    -----
                                    NUMBER     50.0    -----    -----    -----

