                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 180605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 06/05/1991   Location: US-31 N                       
        Pavement Width: 3.77 m.   Section Length: 152.50 m.
        Analysis Date: 02/08/2001 Operator Name: LLP                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0      1.0        0

        Durability Cracking         SQ. M.    -----     0.47        0     0.27
                   Total Slabs Distressed     -----      1.0        0      1.0

        Longitudinal Crack          METERS    -----      1.7      0.9        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     27.0     23.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      6.4     51.0     28.5

        Spall Trans. Joint          METERS    -----      6.7     10.4     14.2
                                    NUMBER    -----      8.0     12.0     14.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    152.9        0        0

        AC Patch                    SQ. M.    -----     1.13     0.18     1.12
                                    NUMBER    -----      5.0      2.0      6.0

        PCC Patch                   SQ. M.    -----   165.34     0.19     0.20
                                    NUMBER    -----     28.0      1.0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    186.2    -----    -----    -----
                                    NUMBER     50.0    -----    -----    -----

