                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 180904           Pavement Type: Planned AC Overlay of CRCP    
        Survey Date: 04/28/1992   Location: I-65 SB                       
        Pavement Width: 3.81 m.   Section Length: 152.50 m.
        Analysis Date: 02/11/2000 Operator Name: MJE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Durability Crack            SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Longitudinal Crack          METERS    -----      1.1        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----    482.0     22.4     11.2
                                    NUMBER    -----    131.0      6.0      3.0
                               TOT. NUMBER    140.0    -----    -----    -----

        Map Crack                   SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Construction Joint          NUMBER    -----      1.0      3.0      3.0

        Lane-shoulder Sep.          METERS    -----    140.9     10.9        0

        AC Patch                    SQ. M.    -----     0.52     0.46        0
                                    NUMBER    -----      3.0      1.0        0

        PCC Patch                   SQ. M.    -----    16.58        0     9.05
                                    NUMBER    -----      2.0        0      1.0

        Punchouts                   NUMBER    -----      1.0        0        0

        Spall Long. Joint           METERS    -----        0      1.1      4.9

        Water Bleed & Pump          METERS      0.6    -----    -----    -----
                                    NUMBER      1.0    -----    -----    -----

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

