                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 190602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 05/19/1991   Location: I-35 S                        
        Pavement Width: 3.78 m.   Section Length: 305.00 m.
        Analysis Date: 01/26/2001 Operator Name: LLP                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     6.29     3.33        0
                   Total Slabs Distressed     -----      4.0      3.0        0

        Longitudinal Crack          METERS    -----      2.4        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     47.7      5.0        0
        ---Sealed---                METERS    -----      1.0        0        0
                                    NUMBER    -----     17.0      2.0        0
        ---Sealed---                NUMBER    -----      1.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     15.0     13.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     22.9      5.4      0.7

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.1        0        0

        AC Patch                    SQ. M.    -----    24.32        0        0
                                    NUMBER    -----     39.0        0        0

        PCC Patch                   SQ. M.    -----    76.99     0.44    29.49
                                    NUMBER    -----     29.0      1.0      8.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    100.7    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

