                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 190605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 04/21/1993   Location: I-35 SB                       
        Pavement Width: 3.79 m.   Section Length: 305.00 m.
        Analysis Date: 03/24/1998 Operator Name: SMF                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      0.7        0        0
        ---Sealed---                METERS    -----      0.7        0        0

        Transverse Crack            METERS    -----     72.3      0.6     10.4
        ---Sealed---                METERS    -----     60.8        0        0
                                    NUMBER    -----     29.0      1.0      4.0
        ---Sealed---                NUMBER    -----     25.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      6.0     26.0      3.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      1.4      1.0      6.1

        Spall Trans. Joint          METERS    -----        0        0      4.8
                                    NUMBER    -----        0        0      2.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.6        0        0

        AC Patch                    SQ. M.    -----    24.21    13.55     9.21
                                    NUMBER    -----     36.0     10.0     11.0

        PCC Patch                   SQ. M.    -----   194.04    19.84    27.77
                                    NUMBER    -----     31.0      2.0      3.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    125.3    -----    -----    -----
                                    NUMBER     35.0    -----    -----    -----

