                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 190605           Pavement Type: Jointed Plain Concrete        
        Survey Date: 05/19/1991   Location: I-35 S                        
        Pavement Width: 3.82 m.   Section Length: 305.00 m.
        Analysis Date: 01/31/2001 Operator Name: LLP                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     2.43     0.88        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      9.3        0        0
        ---Sealed---                METERS    -----      1.2        0        0

        Transverse Crack            METERS    -----     66.1      6.0        0
        ---Sealed---                METERS    -----      4.4        0        0
                                    NUMBER    -----     27.0      2.0        0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     15.0     20.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     20.0      7.2        0

        Spall Trans. Joint          METERS    -----      0.5        0        0
                                    NUMBER    -----      1.0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    304.7        0        0

        AC Patch                    SQ. M.    -----    31.82        0     0.20
                                    NUMBER    -----     44.0        0      1.0

        PCC Patch                   SQ. M.    -----   157.77    37.97    56.02
                                    NUMBER    -----     25.0      6.0     13.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    130.2    -----    -----    -----
                                    NUMBER     35.0    -----    -----    -----

