                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 190605_a         Pavement Type: Jointed Plain Concrete        
        Survey Date: 05/09/1990   Location: I-35 S                        
        Pavement Width: 4.12 m.   Section Length: 305.00 m.
        Analysis Date: 12/14/2001 Operator Name: DJK                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     4.62     5.40     6.95
                   Total Slabs Distressed     -----      8.0      5.0      3.0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     37.0      0.4        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     13.0      1.0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      3.8      2.8        0

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.     0.05    -----    -----    -----
                                    NUMBER      1.0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    306.0        0        0

        AC Patch                    SQ. M.    -----     0.77        0     0.13
                                    NUMBER    -----      5.0        0      1.0

        PCC Patch                   SQ. M.    -----   241.27    21.54        0
                                    NUMBER    -----     36.0      6.0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    142.3    -----    -----    -----
                                    NUMBER     35.0    -----    -----    -----

