                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260601           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 06/16/1995   Location: US-10EB                       
        Pavement Width: 3.86 m.   Section Length: 152.50 m.
        Analysis Date: 08/06/1997 Operator Name: LRL                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     27.3     42.1     61.1
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      9.0     11.0     18.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     10.0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      6.9      0.5      2.7

        Spall Trans. Joint          METERS    -----        0      0.4        0
                                    NUMBER    -----        0      1.0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   279.10    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    151.3        0        0

        AC Patch                    SQ. M.    -----     0.49        0     3.28
                                    NUMBER    -----      3.0        0      6.0

        PCC Patch                   SQ. M.    -----     6.91     6.72    20.05
                                    NUMBER    -----      2.0      1.0      4.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     37.6    -----    -----    -----
                                    NUMBER     10.0    -----    -----    -----

