                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 05/01/1990   Location: US-10 E                       
        Pavement Width: 3.76 m.   Section Length: 305.00 m.
        Analysis Date: 06/04/2003 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     0.24     0.10        0
                   Total Slabs Distressed     -----        0      1.0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     55.9     98.0     58.0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     18.0     30.0     22.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----    148.3      8.4     20.4

        Spall Trans. Joint          METERS    -----      6.4      2.7      9.0
                                    NUMBER    -----      3.0      1.0      7.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.     0.25    -----    -----    -----
                                    NUMBER      3.0    -----    -----    -----

        Polished Aggregate          SQ. M.   509.50    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    306.5        0        0

        AC Patch                    SQ. M.    -----     0.61     0.63    17.14
                                    NUMBER    -----      5.0      4.0     28.0

        PCC Patch                   SQ. M.    -----     6.52    12.55    11.96
                                    NUMBER    -----      1.0      2.0      2.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     56.1    -----    -----    -----
                                    NUMBER     15.0    -----    -----    -----

