                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 06/16/1995   Location: US-10 EB                      
        Pavement Width: 3.83 m.   Section Length: 305.00 m.
        Analysis Date: 08/12/1997 Operator Name: LRL                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      4.0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     43.5     76.8     72.7
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     15.0     22.0     26.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      7.0      7.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     12.9      7.7      3.5

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   623.91    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    301.6        0        0

        AC Patch                    SQ. M.    -----     3.26     7.17    32.24
                                    NUMBER    -----     12.0     15.0     30.0

        PCC Patch                   SQ. M.    -----        0     5.98    24.91
                                    NUMBER    -----        0      1.0      3.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     42.9    -----    -----    -----
                                    NUMBER     14.0    -----    -----    -----

