                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260602           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 10/11/1990   Location: US-10 E                       
        Pavement Width: 3.80 m.   Section Length: 305.00 m.
        Analysis Date: 02/21/2001 Operator Name: MMW                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     84.2     74.6      7.7
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     27.0     22.0      2.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     11.0      3.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      2.7      3.6      1.7

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.     0.13    -----    -----    -----
                                    NUMBER      1.0    -----    -----    -----

        Polished Aggregate          SQ. M.   507.84    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.1        0        0

        AC Patch                    SQ. M.    -----    22.27     8.11    11.95
                                    NUMBER    -----     26.0      5.0      8.0

        PCC Patch                   SQ. M.    -----    13.69     6.59    12.25
                                    NUMBER    -----      2.0      1.0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     52.4    -----    -----    -----
                                    NUMBER     14.0    -----    -----    -----

