                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 06/09/1993   Location: US-10 EB                      
        Pavement Width: 3.75 m.   Section Length: 305.00 m.
        Analysis Date: 03/12/1998 Operator Name: SMF                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      2.8        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     49.4     59.1     59.0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     23.0     18.0     24.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      7.0      7.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     16.7     15.4      8.3

        Spall Trans. Joint          METERS    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   646.74    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.3        0        0

        AC Patch                    SQ. M.    -----     6.43    11.41    24.63
                                    NUMBER    -----     21.0     14.0     16.0

        PCC Patch                   SQ. M.    -----     6.34        0    24.49
                                    NUMBER    -----      1.0        0      3.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     43.1    -----    -----    -----
                                    NUMBER     14.0    -----    -----    -----

