                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 260605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 06/16/1995   Location: US-10 EB                      
        Pavement Width: 3.83 m.   Section Length: 305.00 m.
        Analysis Date: 08/14/1997 Operator Name: LRL                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     24.3     41.0     41.3
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      8.0     13.0     16.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     53.0      6.0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     12.7      8.4        0

        Spall Trans. Joint          METERS    -----      0.5      0.6        0
                                    NUMBER    -----      1.0      1.0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   527.89    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    297.5      5.1        0

        AC Patch                    SQ. M.    -----     3.59     3.14     1.30
                                    NUMBER    -----     16.0      7.0      2.0

        PCC Patch                   SQ. M.    -----   185.66     6.24        0
                                    NUMBER    -----     26.0      1.0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    215.6    -----    -----    -----
                                    NUMBER     59.0    -----    -----    -----

