                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 270703           Pavement Type: Bonded PCC Overlay on CRC     
        Survey Date: 10/06/1991   Location: I-94 E                        
        Pavement Width: 3.74 m.   Section Length: 152.50 m.
        Analysis Date: 04/21/1999 Operator Name: SLS                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Durability Crack            SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     26.5        0        0
                                    NUMBER    -----     10.0        0        0
                               TOT. NUMBER     10.0    -----    -----    -----

        Map Crack                   SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Construction Joint          NUMBER    -----        0        0        0

        Lane-shoulder Sep.          METERS    -----    151.3        0        0

        AC Patch                    SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Punchouts                   NUMBER    -----        0        0        0

        Spall Long. Joint           METERS    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

