                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 290605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 08/10/1999   Location: I-35 SB                       
        Pavement Width: 3.72 m.   Section Length: 305.00 m.
        Analysis Date: 10/08/1999 Operator Name: MJE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0      5.5
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      7.7      1.8     17.8
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      4.0      1.0      5.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     34.0      4.0     10.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      1.9      1.8      1.0

        Spall Trans. Joint          METERS    -----      2.2      1.9      0.5
                                    NUMBER    -----      2.0      1.0      1.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    256.6      5.3      1.7

        AC Patch                    SQ. M.    -----     1.26        0     1.39
                                    NUMBER    -----      5.0        0      3.0

        PCC Patch                   SQ. M.    -----   324.15    60.03   218.79
                                    NUMBER    -----     23.0      4.0      3.0

        Water Bleed & Pump          METERS      6.8    -----    -----    -----
                                    NUMBER      4.0    -----    -----    -----

        Transverse Joint            METERS    175.4    -----    -----    -----
                                    NUMBER     48.0    -----    -----    -----

